
10 June 199

WARNING WARNING WARNING WARNING WARNING WARNING WARNING WARNING WARNING
 Do not run the feildflash operation unless directed by Phobos support.

Reflashing the FirmWare on the Phobos P1000 Gigabit Adapter.

If it should become necessary to reload the firmware on the NIC the
executable "pge_feildflash1f" in this directory will (re)load version
1a of the Firmware. The interface must be unconfigured, 
Ie. "ifconfig pge0 down".  

Execute:

	./pge_feildflash1f pge0

The flash operation will take a few seconds. The machine must then be
shutdown and power-cycled for the new firmware image to be loaded.

NOTE: It on rare occasions the machine may have to be power cycled
twice for the new firmware to begin proper operation.



