| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
GPRS_DynamicOrFixedAllocation_t Struct Reference

## Public Attributes
uint8_t | TFI_ASSIGNMENT
uint8_t | POLLING
uint8_t | UnionType
union { |
DynamicAllocation_t DynamicAllocation |
uint8_t FixedAllocationDummy |
} | Allocation |
uint8_t | CHANNEL_CODING_COMMAND
uint8_t | TLLI_BLOCK_CHANNEL_CODING
uint8_t | Exist_ALPHA
uint8_t | ALPHA
uint8_t | GAMMA
uint8_t | Exist_TIMING_ADVANCE_INDEX
uint8_t | TIMING_ADVANCE_INDEX
uint8_t | Exist_TBF_STARTING_TIME
StartingTime_t | TBF_STARTING_TIME

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-gsm_rlcmac.h