#

Table of Contents | Previous Page | Next Page

# Xircom Ethernet PC Card
Specifications

The Xircom Ethernet PC Card provides connection to 10Mbps or 100Mbps Ethernet networks for access to network utilities, the Internet, E-mail and other network resources.

- Supports 10Base-T Ethernet networks
- IEEE 802.3 compliant
- Full-duplex operation boosts performance
- LEDs indicate network connection status at a glance

### Specifications:

Cable and Connector: | 100Base-TX unshielded twisted pair for use on category 5 (data grade) cabling; 10Base-T unshielded twisted pair (UTP) Connector Type: RJ-45 Operating Distance: 328 ft. (100m)
Certification: | FCC Part 15, FCC Class B, CE Mark, Class B (Except FCC and CE Mark Class A for Model CE3-10)
Ethernet Standards: | IEEE 802.3 for 10Mbps, 802.3u for 100Mbps
Non-volatile RAM: | LAN adapter ID and serial number
LEDs: | Transmission activity (yellow) Link (green) or power (red)
Operating System Compatibility: | Supports Windows 95 (OSR2) or later, Windows 98, Windows NT 4.0 and Windows 2000, using Xircom drivers supplied
Network Operating System Compatibility: | Supports all popular network operating systems including Novell NetWare, Microsoft Windows 95/98, Windows NT, Windows 2000, Windows 3.x, Microsoft LAN Manager, Artisoft LANtastic, Banyan VINES, DEC Pathworks and IBM OS/2

Table of Contents | Previous Page | Next Page