;*****************************************************************************
;
; OEMSETNT.INF
;
;       Xircom Ethernet Adapter 10/100 Network Setup for NT 3.51 and higher
;
; $Revision:   1.2  $
;
;*****************************************************************************

[Identification]
    OptionType = NetAdapter

[PlatformsSupported]
    ISA
    EISA
    MCA

[Options]
	CE3NT

[OptionsTextENG]
    CE3NT    = "Xircom Ethernet Adapter 10/100 for Softex"
    
[AllFileConstants]
GenericInfVersion  = " v1.90"
;  File names, etc. ----------------------------------------
UtilityInf      = "UTILITY.INF"
ParamInf        = "NCPARAM.INF"
subroutineinf   = "SUBROUTN.INF"
SoftwareType    = "driver"
Exit_Code       = 0
; EventLog Message File	 ----------------------------------------
NetEventDLL     = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\drivers\ce3nt.sys"
IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"
; Product Info ----------------------------------------
Manufacturer    = "Xircom"
; Flow control variables  ----------------------------------------
RUNDLLCODE       = 1
;HOTPROGRAMPCMCIA = 1

GenericTextName ="Ethernet Adapter 10/100 for Softex"
DEFAULT_LANMEM = 1   ;Auto
DEFAULT_LANIO = 1    ;Auto
DEFAULT_IRQ = 1      ;Auto 


[FileConstants-CE3NT]
GenericAdapterName = "Xircom Ethernet Adapter 10/100 for Softex"
GenericDriverName  = "Xircom Ethernet Adapter 10/100 for Softex"
GenericSysName     = "CE3NT.sys"
GenericName        = "CE3NT"

; Product Info ----------------------------------------
ProductMajorVersion     = "3"
ProductMinorVersion     = "51"
ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)
; Software  ----------------------------------------
ProductSoftwareName     = "CE3NT"
ProductSoftwareDescription = "Xircom Ethernet Adapter 10/100"
ProductSoftwareImagePath = "\SystemRoot\System32\drivers\"$(GenericSysName)
NetRuleSoftwareType     = "ce3ntSys ndisDriver ce3ntDriver"
NetRuleSoftwareUse      = $(SoftwareType)
NetRuleSoftwareBindForm = """ce3ntSys"" yes no container"
NetRuleSoftwareClass    = {"ce3ntDriver basic"}
NetRuleSoftwareBindable = {"ce3ntDriver ce3ntAdapter non exclusive 100"}
; Hardware  ----------------------------------------
ProductHardwareName        = "CE3NT"
ProductHardwareDescription = "Xircom Ethernet Adapter 10/100 for Softex"
NetRuleHardwareType        = "ce3nt ce3ntAdapter"
NetRuleHardwareBindForm    = " yes yes container"
NetRuleHardwareClass       = {"ce3ntAdapter basic"}
; Registry Key  ----------------------------------------
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"
; Tuple Information -----------------------------------
VERS1Manufacturer = "Xircom"
VERS1Product      = "CreditCard 10/100 for Softex"
VERS1Product2     = "RealPort2 Ethernet 10/100 Adapter for Softex"
VERS1Type	  = "CE3-10/100"




[GeneralConstants]
;  Program flow control variables.
from      = ""
to        = ""
;  Return codes; Exit_Code is set to one of these
ExitCodeOk     = 0
ExitCodeCancel = 1
ExitCodeFatal  = 2
KeyNull         = ""
MAXIMUM_ALLOWED   = 33554432
RegistryErrorIndex = NO_ERROR
KeyProduct      = ""
KeyParameters   = ""
TRUE            = 1
FALSE           = 0
NoTitle            = 0
ExitState   = "Active"
OldVersionExisted = $(FALSE)
DriverPath      = $(!STF_NTPATH)\drivers




[date]
    ; Now is a list which contains { Sec from 1-1-1970, Year, Month, Day, Hour,
    ; Minute, Second }
    Now = {} ? $(!LIBHANDLE) GetSystemDate


;---------------------------------------------------------------------------
; 1. Identify
;
; DESCRIPTION:   To verify that this INF deals with the same type of options
;                as we are choosing currently.
;
; INPUT:         None
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL
;                $($R1): Option Type (COMPUTER ...)
;                $($R2): Diskette description
;---------------------------------------------------------------------------

[Identify]
    ;
    ;
    read-syms Identification

    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)

    Return $(Status) $(Identifier) $(Media)

;------------------------------------------------------------------------
; 2. ReturnOptions:
;
; DESCRIPTION:   To return the option list supported by this INF and the
;                localised text list representing the options.
;
;
; INPUT:         $($0):  Language used. ( ENG | FRN | ... )
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL |
;                                STATUS_NOLANGUAGE
;                                STATUS_FAILED
;                                STATUS_NOTSUPPORTED
;
;                $($R1): Option List
;                $($R2): Option Text List
;------------------------------------------------------------------------

[ReturnOptions]
    ;
    ;
    set Status        = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
        ;
        ; Check if the platforms requested is supported
        ;
        ifstr(i) $($1) == ""
                        goto returnoptions
        endif

        set PlatformList = ^(PlatformsSupported, 1)
        Ifcontains(i) $($1) in $(PlatformList)
                        goto returnoptions
        else
                        set Status = STATUS_NOTSUPPORTED
                        goto finish_ReturnOptions
        endif
    else
                set Status = STATUS_NOLANGUAGE
                goto finish_ReturnOptions
    endif

    ;
    ; form a list of all the options and another of the text representing
    ;

returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status         = STATUS_SUCCESSFUL

finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)

;------------------------------------------------------------------------
;
; InstallOption:
;
;      This section is shelled to by main installation processing
;      or by NCPASHEL.INF during reconfig, removal, update, etc.
;
;
; FUNCTION:  To copy files representing Options
;            To configure the installed option
;            To update the registry for the installed option
;
; INPUT:     $($0):  Language to use
;            $($1):  OptionID to install
;            $($2):  SourceDirectory
;            $($3):  AddCopy  (YES | NO)
;            $($4):  DoCopy   (YES | NO)
;            $($5):  DoConfig (YES | NO)
;
; OUTPUT:    $($R0): STATUS: STATUS_SUCCESSFUL |
;                            STATUS_NOLANGUAGE |
;                            STATUS_USERCANCEL |
;                            STATUS_FAILED
;
;------------------------------------------------------------------------
[InstallOption]
    ;
    ; Set default values for
    ;
    set Status   = STATUS_FAILED
    ;
    ; extract parameters
    ;
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)

    Set !DebugOutputControl = 1

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
        Return STATUS_NOLANGUAGE
    endif

    set-subst LF = "\n"

    read-syms GeneralConstants
	read-syms AllFileConstants
    read-syms FileConstants"-"$(Option)
    read-syms DialogConstants$(!STF_LANGUAGE)"-"$(Option)
    ifstr(i) $(!NTN_Origination) == "NCPA"
        set Continue = $(OK)
    endif

    read-syms AllFileConstants$(!STF_LANGUAGE)
    read-syms FileConstants$(!STF_LANGUAGE)"-"$(Option)

    detect date

    set-title  $(FunctionTitle)

    set to   = Begin
    set from = Begin
;
;  Assume all is well.
;
    set CommonStatus = STATUS_SUCCESSFUL

    EndWait

;
;   Set up the operation-mode-based variables and gaily welcome
;   the user.  If the "install mode" variable is improperly set,
;   assume this is a new installation.
;

Begin = +
    Set ActivateDetection = FALSE

    Ifstr(i) $(!NTN_InstallMode) == deinstall
        set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
        set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
        set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
;        set ActivateDetection = TRUE
        set StartLabel = configureadapter
        ;
        ;   You cannot config the software component
        ;
        Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
            ;Debug-Output "Cannot configure the software."
            Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
            ifint $($ShellCode) != $(!SHELL_CODE_OK)
                Debug-Output "ShellCode error: cannot get an error string."
                goto ShellCodeError
            endif
            set Error = $($R0)
            set from = end
            set to = end
            goto nonfatalinfo
        endif
    else
;        set ActivateDetection = TRUE
        set StartLabel = installadapter
        set OEM_ABANDON_OPTIONS = {}
        set OEM_ABANDON_SOFTWARE = FALSE
        set OEM_ABANDON_ON = TRUE
    endif


    ;  set the [Default values]

    set IRQValue			= *($(IRQList), $(DEFAULT_IRQ))		; IRQ Level = 10
    set IOBaseAddrValue		= *($(IOBaseAddrList), $(DEFAULT_LANIO))	; IOBase Address = 0x320
    set MemoryAddrValue		= *($(MemoryAddrList), $(DEFAULT_LANMEM))	; Memory Address = 0xD0000
    set CableTypeValue		= *($(CableTypeList), 1)			; Cable Type = Auto Detect
    set LinkIntegrityValue		= "ON"						; Link Integrity = Enabled
    set EarlyTransmitValue		= "ON"						; Early Transmit = on
    set DynamicLinkDetectValue	= "ON"						; Dynamic Link Detection = ON
    set ModeValue			= *($(ModeList), 1)				; Mode = I/O
    set LineSpeedValue		= *($(LineSpeedList), 1)			; LineSpeed = auto
    set LineModeValue		= *($(LineModeList), 1)			; LineMode = auto
    set InitDelayValue		= *($(InitDelayList), 1)			; InitDelay = 0



    Set from = $(fatal)
    Set to = $(fatal)
    Goto $(StartLabel)

;-----------------------------------------------
; Installation Section
;-----------------------------------------------

installadapter = +
;
;   First, check whether the same version of the software exists
;
    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

    Ifstr $(KeyProduct) != $(KeyNull)
        ;
        ; Same version already existed in the local machine
        ; Popup the dialog and ask the user whether he wants to continue
        ;
        CloseRegKey $(KeyProduct)

        ifstr(i) !(NTN_RegBase) == $(ProductKeyName)
           ;
           ; Cannot Install the same software again
           ;
           Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
               $(ProductVersion)
           ifint $($ShellCode) != $(!SHELL_CODE_OK)
               Debug-Output "ShellCode error: cannot get an error string."
               goto ShellCodeError
           endif

           goto end
        else
           ;
           ; Add a new adapter card?
           ;
           Shell $(UtilityInf), CardExistedDlg

           ifint $($ShellCode) != $(!SHELL_CODE_OK)
               Debug-Output "ShellCode error: cannot get an error string."
               goto ShellCodeError
           endif

           ifstr(i) $($R1) != "OK"
               goto end
           endif
           set OldVersionExisted = $(TRUE)
        endif
    endif

;
;  dll load addition
;
    Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) NO

    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Goto ShellCodeError
    Else-Ifstr(i) $($R0) == STATUS_FAILED
        Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
        Goto fatal
    Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
        Goto successful
    Endif

    Set SrcDir = $($R1)

    install "Install-Dll"

    goto adaptersetup

;-----------------------------------------------
; Configuration Section
;-----------------------------------------------
;
;   Get the current values of all the parameters
;
configureadapter = +
    Ifstr $(KeyProduct) == $(KeyNull)
        OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
        Ifstr $(KeyProduct) == $(KeyNull)
            set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
            Debug-Output "Cannot find component product key"
            goto fatalregistry
        Endif
    Endif

    ;
    ; Get the other parameters;  they're attached to the service parameters key
    ;
    Debug-Output "INF: Shelling to FindService"
    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "INF: FindService shell failure"
        Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
        Debug-Output "INF: FindService Shell error: "$($R0)
        Goto fatalregistry
    endif

    Set KeyParameters = $($R2)

    ;
    ;  We don't need the services key, so close it.
    ;
    CloseRegKey $($R1)

    Ifstr $(KeyParameters) == $(KeyNull)
        set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
        Debug-Output "Cannot find component service"
        goto fatalregistry
    endif

    set OldVersionExisted = $(TRUE)

    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}


    ;
    ; Get the old values from the Registry	[Get Values]
    ; *********************************************************
	EnumRegValue $(KeyParameters) ValueList
    ForListDo $(ValueList)
	set ValueItem = $($)
	set ValueName = *($(ValueItem),1)
	set ValueData = *($(ValueItem),4)
	ifstr(i) $(ValueName) == "IoBaseAddress"
		set IOBaseAddrIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "InterruptNumber"
		set IRQValueIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "EarlyTransmit"
		set EarlyTransmitValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "DynamicLinkDetect"
		set DynamicLinkDetectValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "LinkIntegrity"
		set LinkIntegrityValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "CableType"
		set CableTypeIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "PCCARDAttributeMemoryAddress"
		set MemoryAddrIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "NetworkAddress"
		set NetworkAddressValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "Mode"
		set ModeIndex = $(ValueData)                ; mode value is base 0
	else-ifstr(i) $(ValueName) == "LineSpeed"
		set LineSpeedIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "LineMode"
		set LineModeIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "InitDelay"
		set InitDelayIndex = $(ValueData)

	endif
    EndForListDo

    set IRQValue = *($(IRQList), ~($(IRQValues),$(IRQValueIndex)))
    ifstr(i) $(IRQValue) == ""
	set IRQValue = *($(IRQList), $(DEFAULT_IRQ))
    endif

    set MemoryAddrValue = *($(MemoryAddrList), ~($(MemoryAddrValues),$(MemoryAddrIndex)))
    ifstr(i) $(MemoryAddrValue) == ""
	set MemoryAddrValue = *($(MemoryAddrValues), $(DEFAULT_LANMEM))
    endif

    set IOBaseAddrValue = *($(IOBaseAddrList), ~($(IOBaseAddrValues),$(IOBaseAddrIndex)))
    ifstr(i) $(IOBaseAddrValue) == ""
	set IOBaseAddrValue = *($(IOBaseAddrList), $(DEFAULT_LANIO))
    endif

    set ModeValue = *($(ModeList), ~($(ModeValues),$(ModeIndex)))
    ifstr(i) $(ModeValue) == ""
	set ModeValue = *($(ModeValues), 2)
    endif

    set CableTypeValue = *($(CableTypeList), ~($(CableTypeValues),$(CableTypeIndex)))
    ifstr(i) $(CableTypeValue) == ""
	set CableTypeValue = *($(CableTypeValues), 2)
    endif

    set LineSpeedValue = *($(LineSpeedList), ~($(LineSpeedValues),$(LineSpeedIndex)))
    ifstr(i) $(LineSpeedValue) == ""
	set LineSpeedValue = *($(LineSpeedValues), 0)
    endif
    
    set LineModeValue = *($(LineModeList), ~($(LineModeValues),$(LineModeIndex)))
    ifstr(i) $(LineModeValue) == ""
	set LineModeValue = *($(LineModeValues), 0)
    endif

    set InitDelayValue = *($(InitDelayList), ~($(InitDelayValues),$(InitDelayIndex)))
    ifstr(i) $(InitDelayValue) == ""
	set InitDelayValue = *($(InitDelayValues), 1)
    endif


    ifstr(i) $(EarlyTransmitValue) == ""
	set EarlyTransmitValue = 1
    endif

    ifstr(i) $(DynamicLinkDetectValue) == ""
	set DynamicLinkDetectValue = 1
    endif

    ifstr(i) $(LinkIntegrityValue) == ""
	set LinkIntegrityValue = 1
    endif

    ifint $(EarlyTransmitValue) == 1
	set EarlyTransmitValue = "ON"
    else
	set EarlyTransmitValue = "OFF"
    endif

    ifint $(DynamicLinkDetectValue) == 1
	set DynamicLinkDetectValue = "ON"
    else
	set DynamicLinkDetectValue = "OFF"
    endif

    ifint $(LinkIntegrityValue) == 1
	set LinkIntegrityValue = "ON"
    else
	set LinkIntegrityValue = "OFF"
    endif


    set CheckItemsIn = {$(EarlyTransmitValue),$(LinkIntegrityValue),$(DynamicLinkDetectValue)}
;    set CheckItemsIn = {"OFF", "ON", "OFF"}



    ;  Save the settings as they were read from the Registry.

;    Shell $(ParamInf) Param_SaveValues
;    Set CurrParamSettings = $($R0)
;
;   Put up the adapter configuration dialog if necessary.
;
;   Note that $(CurrParamSettings) has the old known parameter values.
;
adaptersetup = +


    ;Shell "" DebugConfiguration "before displaying dialog"

    Set from = adapteroptions


adapteroptions = +

	set CheckItemsIn = {$(EarlyTransmitValue),$(LinkIntegrityValue),$(DynamicLinkDetectValue)}

    LoadLibrary "disk 1" $(DialogDllName) hLib
    read-syms FileDependentDlg$(!STF_LANGUAGE)"-"$(Option)
;	set ENABLER = 0

;	ifint $(RUNDLLCODE) == 1
;		    LibraryProcedure ENABLER, $(hLib), EnablerRunning 		; check for enabler type
;		    ifint $(ENABLER) == 1
;				set Static1Label = "Configuring driver for Microsoft Enabler"
;		    else-ifint $(ENABLER) == 2
;				set Static1Label = "Configuring driver for third party Card & Socket Services"
;		    else
;				set Static1Label = "Configuring driver for Xircom Enabler"
;			endif
;	endif


	;------------------------------------------------------
	; Call out to the PCMCIA driver only if we're loading a PCMCIA device

;	ifint $(RUNDLLCODE) == 1
			;------------------------------------------------------
			; DLLCODE
			; Locate the slot with the Xircom Card in it
			;------------------------------------------------------
;			LibraryProcedure CONFIG, $(hLib), GetPCMCIAConfig
;			set SLOTCOUNT = 8	; was 	*($(CONFIG),1), but returned 0
;			set CONTROLLERTYPE = *($(CONFIG),3)
			;Debug-Output "slot count="$(SLOTCOUNT)" controller type="$(CONTROLLERTYPE)
;			set SLOT = 0
;		  slotloop = +
;			LibraryProcedure INFO, $(hLib), GetVERS_1Tuple $(SLOT)      ;VERS_1
;			ifstr(i) *($(INFO),3) == $(VERS1Manufacturer)
;				ifstr(i) *($(INFO),4) == $(VERS1Product)
;					goto slotfound
;				else-ifstr(i) *($(INFO),4) == $(VERS1Product2)
;					goto slotfound
;				endif
;			endif

;			set-add SLOT = $(SLOT), 1
;			ifint $(SLOT) == $(SLOTCOUNT)
;				goto slotnotfound
;			else
;				goto slotloop
;			endif
;		  slotfound = +
			;Debug-Output "Xircom card found in slot "$(SLOT)
			;set Static2Label = "CE3 10/100 in slot "$(SLOT)
;			LibraryProcedure INFO, $(hLib), GetFUNCETuple $(SLOT)      ;VERS_1
;			set	Static2Label = "Physical Address:"
;			set	Static3Label = $(INFO)
;			ifstr(i) $(NetworkAddressValue) != ""
;			  set Static4Label = "Network Address:"
;			  set Static5Label = $(NetworkAddressValue)
;			endif
;			set SLOTFOUND = 1
;			goto slotcontinue
;		  slotnotfound = +
;			set SLOTFOUND = ""
			;set Static2Label = "CE3 10/100 was not found"
			;Debug-Output "Xircom card not found"
;		  slotcontinue = +
;	endif



	;------------------------------------------------------

    ;
    ; If this is an unattend installation we need to skip the DLL UI stuff.
    ;
    ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
    	goto skipoptions
    endif
    
    ui start "InputDlg"  $(hLib)

    set ExitButton      = $(ButtonPressed)
    ;Debug-Output " ButtonPressed "$(ButtonPressed)
    ;Debug-Output " DLGEVENT "$(DLGEVENT)
	FreeLibrary $(hLib)

    ifstr(i) $(DLGEVENT) == "CONTINUE"

	set IOBaseAddrIndex	= $(Combo1Out)
	set MemoryAddrIndex	= $(Combo2Out)
	set IRQValueIndex	= $(Combo3Out)
	set ModeIndex		= $(Combo4Out)
	set CableTypeIndex	= $(Combo5Out)
	set LineSpeedIndex	= $(Combo6Out)
	set LineModeIndex	= $(Combo7Out)
	set InitDelayIndex	= $(Combo8Out)
	set EarlyTransmitValue	= *($(CheckItemsOut), 1)
	set LinkIntegrityValue	= *($(CheckItemsOut), 2)
	set DynamicLinkDetectValue = *($(CheckItemsOut), 3)
	set ExitButton		= $(ButtonPressed)

	ui pop 1

    else-ifstr(i) $(DLGEVENT) == "EXIT"
	set CommonStatus = STATUS_USERCANCEL
	ui pop 1
	goto end
    else
	set CommonStatus = STATUS_USERCANCEL
	ui pop 1
	Debug-Output "Action: unknown. Bye."
	goto end
    endif


;
;   If installing, go create the necessary keys;
;   if configuring, they're already open.
;
skipoptions =+

    ifint $(OldVersionExisted) == $(TRUE)
        ifstr(i) $(!NTN_InstallMode) == configure
            goto writeparameters
        endif
    endif
    StartWait
    ;
    ; Add Software Component
    ;
    ifint $(OldVersionExisted) == $(FALSE)

        ifstr(i) $(!NTN_InstallMode) == "install"
           Ifstr(i) $(DoCopy) == "YES"

              Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES

              Ifint $($ShellCode) != $(!SHELL_CODE_OK)
                  Goto ShellCodeError
              Else-Ifstr(i) $($R0) == STATUS_FAILED
                  Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
                  ifint $($ShellCode) != $(!SHELL_CODE_OK)
                      goto ShellCodeError
                  endif
                  set Error = $($R0)
                  Goto fatal
              Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
                  Goto successful
              Endif

              Set SrcDir = $($R1)

           Endif

           install "Install-Option"

           ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
              Shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
              ifint $($ShellCode) != $(!SHELL_CODE_OK)
                  goto ShellCodeError
              endif
              set Error = $($R0)
              goto fatal
           endif
        endif



        Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), +
            $(ProductSoftwareName), +
            $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
            $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
            $(NetEventDLL)

        Set OEM_ABANDON_SOFTWARE = TRUE

        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif
        ;
        ;   At this point:
        ;     $R1 contains the product version key handle;
        ;     $R2 contains the NetRules subkey handle;
        ;     $R3 contains the new Services key handle; and
        ;     $R4 contains the Parameters key
        ;     $R5 contains the Linkage Key
        ;
        set RegistryErrorIndex = $($R0)
        set KeyProduct      = $($R1)
        Set SoftNetRulesKey = $($R2)
        CloseRegKey $($R3)
        CloseRegKey $($R4)
        CloseRegKey $($R5)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
            Debug-Output "Registry error: add software components"
            CloseRegKey $(KeyProduct)
            CloseRegKey $(SoftNetRulesKey)
            goto fatalregistry
        endif

        set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
                           {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
                           {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
                           {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
                           {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
                           {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
                           {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

        Shell  $(UtilityInf), AddValueList, $(KeyProduct), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error."
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
            Debug-Output "Registry error: add value list."
            CloseRegKey $(KeyProduct)
            CloseRegKey $(SoftNetRulesKey)
            goto fatalregistry
        endif

        set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
                            {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
                            {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
                            {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
                            {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareBindable)}, +
                            {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

        Shell  $(UtilityInf), AddValueList, $(SoftNetRulesKey), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error."
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        CloseRegKey $(KeyProduct)
        CloseRegKey $(SoftNetRulesKey)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
            Debug-Output "Resgitry error: add value list."
            goto fatalregistry
        endif
    endif
;
;   Create the HARDWARE\Netcard region and its corresponding service
;
    Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)

    ifint $($R4) != -1
        Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
    endif

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "Cannot add hardware component"
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        EndWait
        Debug-Output "Registry error: add hardware component"
        CloseRegKey $($R1)
        CloseRegKey $($R2)
        CloseRegKey $($R3)
        goto fatalregistry
    endif

;
;   At this point:
;     $R1  Registry key variable for HARDWARE\Netcard\(n)
;     $R2  Registry key variable for HARDWARE\Netcard\(n)\\NetRules
;     $R3  Registry key handle for <service>\Parameters key
;     $R4  Adapter number assigned to adapter
;     $R5  Service name generated by combining svc name with adapter number
;
    set KeyParameters = $($R3)
    set KeyAdapterRules = $($R2)
    set AdapterNumber = $($R4)

    set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
                       {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardwareTitle)},+
                       {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareDescription)},+
                       {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
                       {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
                       {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

    Shell  $(UtilityInf), AddValueList, $($R1), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error"
        goto ShellCodeError
    endif

    CloseRegKey $($R1)

    set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
    set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)

    set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardwareType)},+
                        {bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
                        {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardwareClass)}, +
                        {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

    Shell  $(UtilityInf), AddValueList, $(KeyAdapterRules), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        EndWait
        Debug-Output "Resgitry error: add value list."
        CloseRegKey $(KeyParameters)
        CloseRegKey $(KeyAdapterRules)
        goto fatalregistry
    endif

    CloseRegKey $(KeyAdapterRules)

    goto writeparameters
;
;   REQUIRED:   $(KeyParameters) contains service Parameters key handle
;
writeparameters = +
    Shell $(UtilityInf), GetBusTypeNum
;    set BusTypeNum = $($R1)
    set BusTypeNum = 1
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif
;
;   Add the rest of the parameters to the Services area
;


	ifstr(i) $(EarlyTransmitValue) == "ON"
		set EarlyTransmitValue =  "1"
	else
		set EarlyTransmitValue =  "0"
	endif

	ifstr(i) $(DynamicLinkDetectValue) == "ON"
		set DynamicLinkDetectValue =  "1"
	else
		set DynamicLinkDetectValue =  "0"
	endif

	ifstr(i) $(LinkIntegrityValue) == "ON"
		set LinkIntegrityValue =  "1"
	else
		set LinkIntegrityValue =  "0"
	endif

	ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
		set ModeValue		       	= *($(ModeValues), 1)
		set MemoryAddrValue	       	= *($(MemoryAddrValues), $(DEFAULT_LANMEM))
		set-add CommonMemoryAddrValue	= $(MemoryAddrValue), 4096
		set IRQValue		       	= *($(IRQValues), $(DEFAULT_IRQ))
		set IOBaseAddrValue	       	= *($(IOBaseAddrValues), $(DEFAULT_LANIO))
		set CableTypeValue	       	= *($(CableTypeValues), 1)
		set LineSpeedValue	       	= *($(LineSpeedValues), 1)
		set LineModeValue	       	= *($(LineModeValues), 1)
		set InitDelayValue              	= *($(InitDelayValues), 1)
		set IOLengthValue	       	= 15
	else
		set ModeValue			= *($(ModeValues),       ~($(ModeList),       $(ModeIndex)))
		set MemoryAddrValue  		= *($(MemoryAddrValues), ~($(MemoryAddrList), $(MemoryAddrIndex)))
		set-add CommonMemoryAddrValue	= $(MemoryAddrValue), 4096
		set IRQValue         		= *($(IRQValues),        ~($(IRQList),        $(IRQValueIndex)))
		set IOBaseAddrValue  		= *($(IOBaseAddrValues), ~($(IOBaseAddrList), $(IOBaseAddrIndex)))
		set CableTypeValue  		= *($(CableTypeValues),  ~($(CableTypeList),  $(CableTypeIndex)))
		set LineSpeedValue  		= *($(LineSpeedValues),  ~($(LineSpeedList),  $(LineSpeedIndex)))
		set LineModeValue  		= *($(LineModeValues),   ~($(LineModeList),   $(LineModeIndex)))
		set InitDelayValue		= *($(InitDelayValues),    ~($(InitDelayList),     $(InitDelayIndex)))
		set IOLengthValue		= 15
	endif
    set NewValueList     = {{AdapterType,             $(NoTitle),$(!REG_VT_DWORD),0},+
                            {BusNumber,               $(NoTitle),$(!REG_VT_DWORD),0},+
                            {BusType,                 $(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
                            {CableType,               $(NoTitle),$(!REG_VT_DWORD),$(CableTypeValue)},+
			    {SoftexPcmcia,            $(NoTitle),$(!REG_VT_DWORD),1},+
                            {DynamicLinkDetect,       $(NoTitle),$(!REG_VT_DWORD),$(DynamicLinkDetectValue)},+
                            {EarlyTransmit,           $(NoTitle),$(!REG_VT_DWORD),$(EarlyTransmitValue)},+
                            {InitDelay,			$(NoTitle),$(!REG_VT_DWORD),$(InitDelayValue)},+
                            {InterruptNumber,         $(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
                            {IoBaseAddress,           $(NoTitle),$(!REG_VT_DWORD),$(IOBaseAddrValue)},+
                            {IoLength,                $(NoTitle),$(!REG_VT_DWORD), 15},+
                            {LineSpeed,               $(NoTitle),$(!REG_VT_DWORD),$(LineSpeedValue)},+
                            {LineMode,                $(NoTitle),$(!REG_VT_DWORD),$(LineModeValue)},+
                            {LinkIntegrity,           $(NoTitle),$(!REG_VT_DWORD),$(LinkIntegrityValue)},+
                            {MemoryMappedBaseAddress, $(NoTitle),$(!REG_VT_DWORD),$(CommonMemoryAddrValue)},+
                            {MemoryMappedSize,        $(NoTitle),$(!REG_VT_DWORD),4096},+
                            {Mode,                    $(NoTitle),$(!REG_VT_DWORD),$(ModeValue)},+
                            {MediaType,               $(NoTitle),$(!REG_VT_DWORD),1},+
                            {PCCARDAttributeMemoryAddress, $(NoTitle),$(!REG_VT_DWORD),$(MemoryAddrValue)},+
                            {PCCARDAttributeMemoryOffset,  $(NoTitle),$(!REG_VT_DWORD),0},+
                            {PCCARDAttributeMemorySize,    $(NoTitle),$(!REG_VT_DWORD),4096},+
                            {PCCARDMemoryWindowOffset,     $(NoTitle),$(!REG_VT_DWORD),0},+
                            ;{PCMCIA,                  $(NoTitle),$(!REG_VT_DWORD),1},+
                            {ProductName,             $(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
                            {TransmitBufferSize,      $(NoTitle),$(!REG_VT_DWORD),7168}}



    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)

    ;---------------------------------------------------------
    ; To workaround the bugs in PCMCIA.SYS when the adapter
    ; number is greater than 10, add a copy of the key
    ; with a number less than 10 (i.e. CE313 -> CE39
    ;---------------------------------------------------------
    ifint $(AdapterNumber) > 10
      Debug-Output "Workaround!"
      set WorkaroundKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)9"\Parameters"
      set KeyWorkaround = ""
      OpenRegKey $(!REG_H_LOCAL) "" $(WorkaroundKeyName) $(MAXIMUM_ALLOWED) KeyWorkaround
      ifstr $(KeyWorkaround) == $(NULL)
          CreateRegKey $(!REG_H_LOCAL) {$(WorkaroundKeyName),0,0} "" +
              $(MAXIMUM_ALLOWED) "" KeyWorkaround
      endif
      Shell  $(UtilityInf), AddValueList, $(KeyWorkaround), $(NewValueList)
      CloseRegKey $(KeyWorkaround)
    endif
	
    ;
    ; If unattended install, update the registry with the values from the unattend.txt file.
    ;
    ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
	Shell $(UtilityInf), AddDefaultNetCardParameters, $(KeyParameters)

	;
	; Now read back the values just written to the registry so we can configure the slot
	; later (if necessary).
	;
	set ValueList = {}
	EnumRegValue $(KeyParameters) ValueList
	ForListDo $(ValueList)
	    set ValueItem = $($)
	    set ValueName = *($(ValueItem),1)
	    set ValueData = *($(ValueItem),4)
	    ifstr(i) $(ValueName) == "InterruptNumber"
	        set IRQValue = $(ValueData)
	
	    else-ifstr(i) $(ValueName) == "IoBaseAddress"
	        set IOBaseAddrValue = $(ValueData)
	
	    else-ifstr(i) $(ValueName) == "PCCARDAttributeMemoryAddress"
	        set MemoryAddrValue = $(ValueData)
	
	    endif
	EndForListDo
    endif

    CloseRegKey $(KeyParameters)

    ; --------------------------------------------------------------------------------
    ; Reprogram the PCMCIA slot with the new parameters.  This should only be done
    ; during first time installation of NT and/or networking, and if our adapter 
    ; has been found.  This should not occur if the user is simply reconfiguring a
    ; previously installed adapter that is up and running.
    ; --------------------------------------------------------------------------------
	
;    ifstr(i) $(!NTN_InstallMode) != configure
;	ifint $(RUNDLLCODE) == 1
;		ifint $(ENABLER) == 1
;			ifint $(HOTPROGRAMPCMCIA) == 1
;				ifint $(SLOTFOUND) == 1		; and a Xircom card was found in a slot
	
					; Add our adapter to the hardware description section of the
					; registry.  This will allow the driver to start running
					; during NT or network installation.
	
;					set PCMCIASYSTEMKeyName = "HARDWARE\DESCRIPTION\System"
;					set PCMCIAPCCARDSKeyName = $(PCMCIASYSTEMKeyName)"\PCMCIA PCCARDs"
	
;					OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIASYSTEMKeyName) $(!REG_KEY_CREATE_SUB_KEY) SYSTEMKeyHandle
;					ifstr $(SYSTEMKeyHandle) != $(NULL)		
;						CreateRegKey $(SYSTEMKeyHandle) {"PCMCIA PCCARDs", 0, 0} "" $(!REG_KEY_SET_VALUE) 0 PCCARDsKeyHandle
;						ifstr $(PCCARDsKeyHandle) != $(NULL)
;							SetRegValue $(PCCARDsKeyHandle) {$(ProductSoftwareName), 0, $(!REG_VT_DWORD), 0}
;							CloseRegKey $(PCCARDsKeyHandle)
;							Debug-Output "CE3 INF - PCMCIA PCCARDs key created, name/value pair set"
;						else
;							Debug-Output "CE3 INF - PCMCIA PCCARDs key already exists"
;						endif
;						CloseRegKey $(SYSTEMKeyHandle)
;					endif
					
;					LoadLibrary "disk 1" $(DialogDllName) hLib
;					Debug-Output "Enabling network resources"
						
;					LibraryProcedure STATUS, $(hLib), SetupSlot $(SLOT) $(IRQValue) 0 $(IOBaseAddrValue) $(IOLengthValue) $(MemoryAddrValue) 4096 0
;					Debug-Output "SetupSlot: "$(STATUS)
;					FreeLibrary $(hLib)
;				endif
;			endif
;		endif
;	endif
;    endif


   ; --------------------------------------------------------------------------------
   ; Write the parameters to the PCMCIA database section, iff running MS Enabler
   ; Add/replace only the parts for the CE3
   ; --------------------------------------------------------------------------------
;   set PCMCIADatabaseKeyName = $(!NTN_ServiceBase)"\Pcmcia\DataBase"
;   set PCMCIADatabaseXircomKeyName = $(PCMCIADatabaseKeyName)"\Xircom"
;   OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseKeyName) $(MAXIMUM_ALLOWED) PCMCIADatabaseKey

;   ifstr $(PCMCIADatabaseKey) == $(NULL)
	;Debug-Output "Pcmcia\DataBase not present"

;   else ; PCMCIA.sys is installed and registry has database section in it.
	; Try to open Xircom section.
	;
;	OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseKeyName)"\Xircom" $(MAXIMUM_ALLOWED) PCMCIADatabaseXircomKey
;	ifstr $(PCMCIADatabaseXircomKey) == $(NULL) ; open failed, so create Xircom subkey
;		CreateRegKey $(PCMCIADatabaseKey) {"Xircom", 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIADatabaseXircomKey
;	endif

	; Open Product Name (i.e. VERS1Product)
	;
;    	OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseXircomKeyName)"\"$(VERS1Product) $(MAXIMUM_ALLOWED) PCMCIADatabaseXircomCE3Key
;	ifstr $(PCMCIADatabaseXircomCE3Key) == $(NULL)
;		CreateRegKey $(PCMCIADatabaseXircomKey) {$(VERS1Product), 0, 0} "" $(MAXIMUM_ALLOWED) 0 PCMCIADatabaseXircomCE3Key
;	endif

	; Set the values
	;
;	SetRegValue $(PCMCIADatabaseXircomCE3Key) {Driver, 0, $(!REG_VT_SZ),"ce3"}
;	SetRegValue $(PCMCIADatabaseXircomCE3Key) {AttributeMemorySize, 0, $(!REG_VT_DWORD),4096}
;	SetRegValue $(PCMCIADatabaseXircomCE3Key) {DeviceType, 0, $(!REG_VT_SZ),"NET"}
;	CloseRegKey $(PCMCIADatabaseXircomCE3Key)
	
	; Open Next Product Name (i.e. VERS1Product2) -------------------------------------------------------------
	set PCMCIADatabaseXircomCE3Key = $(NULL)
    	OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseXircomKeyName)"\"$(VERS1Product2) $(MAXIMUM_ALLOWED) PCMCIADatabaseXircomCE3Key
	ifstr $(PCMCIADatabaseXircomCE3Key) == $(NULL)
		CreateRegKey $(PCMCIADatabaseXircomKey) {$(VERS1Product2), 0, 0} "" $(MAXIMUM_ALLOWED) 0 PCMCIADatabaseXircomCE3Key
	endif

	; Set the values --------------------------------------------------------------------------------------
	SetRegValue $(PCMCIADatabaseXircomCE3Key) {Driver, 0, $(!REG_VT_SZ),"ce3"}
	SetRegValue $(PCMCIADatabaseXircomCE3Key) {AttributeMemorySize, 0, $(!REG_VT_DWORD),4096}
	SetRegValue $(PCMCIADatabaseXircomCE3Key) {DeviceType, 0, $(!REG_VT_SZ),"NET"}
	CloseRegKey $(PCMCIADatabaseXircomCE3Key)
	CloseRegKey $(PCMCIADatabaseXircomKey)
	CloseRegKey $(PCMCIADatabaseKey)
	
   endif


   ; --------------------------------------------------------------------------------
   ; --------------------------------------------------------------------------------


    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        Debug-Output "Registry error: Add value list"
        goto fatalregistry
    endif

    EndWait

    goto successful

;-----------------------------------------------
; Binding section
;-----------------------------------------------
bindingadapter =+
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal

;-----------------------------------------------
; Removeadapter section
;-----------------------------------------------

removeadapter = +
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
        ; Remove Software Component
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    else
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $(!NTN_RegBase)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif


    endif

    ;---------------------------------------------------------
    ; Check if the PCMCIA.SYS workaround needs to be
    ; removed. See the comments and code in the
    ; writeadapter section above.
    ;---------------------------------------------------------
    set WorkaroundKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)9
    set KeyWorkaround = ""
    OpenRegKey $(!REG_H_LOCAL) "" $(WorkaroundKeyName) $(MAXIMUM_ALLOWED) KeyWorkaround
    ifstr $(KeyWorkaround) != $(NULL)
        DeleteRegTree $(KeyWorkaround) ""
    endif

    goto end

;-----------------------------------------------
; Upgrade Software section
;-----------------------------------------------

UpgradeSoftware = +
    ;
    ; First determine whether we want to do upgrade or update for software
    ; or hardware component. Then we will determine whether the Mode is
    ; update or upgrade.
    ;
    ; If the same version of the product existed in the registry, we do
    ; update. Otherwise, we will do a upgrade
    ;
    ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
        ; Upgrade software component
        ;
        ; see whether the same version exist or not
        ;
        OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

        Ifstr $(KeyProduct) != $(KeyNull)
            GetRegValue $(KeyProduct),"MajorVersion", VersionInfo
            set Version = *($(VersionInfo), 4)

            ;
            ; Update the binaries
            ;
            Shell $(UtilityInf), GetInfFileNameFromRegistry, $(KeyProduct)

            ifint $($ShellCode) != $(!SHELL_CODE_OK)
                Debug-Output "ShellCode error"
                goto ShellCodeError
            endif

            set !UG_Filename = $($R0)

            ifstr(i) $(!UG_Filename) != ""
                install "Install-Update"
                ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
                    goto fatal
                endif
            endif

            ; Upgrade the version number
            ;
            SetRegValue $(KeyProduct) {MajorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMajorVersion)}
            SetRegValue $(KeyProduct) {MinorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMinorVersion)}

            ;
            ; do nothing for update
            ;
            ifint $(Version) != $(ProductVersion)
               ;
               ; If the major version number is not the same,
               ; it is major upgrade. So let Upgrade the product
               ;
               ;
               ; make other upgrade change if necessary
               ;
            endif
            CloseRegKey $(KeyProduct)
        else
            ;
            ; Cannot Open software key, goto ERROR
            ;
            goto fatalregistry
        endif
    else
        ;
        ; upgrade/update hardware component
        ; There is no different between upgrade and update for hardware
        ; component
        ;
        ; 1. Get the Service Name
        ; 2. Change the NetRule section if necessary
        ;
        OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) +
              $(MAXIMUM_ALLOWED) NetworkCardKey
        Ifstr(i) $(NetworkCardKey) != $(KeyNull)
            ;
            ; Get Service name
            ;
            GetRegValue $(NetworkCardKey),"ServiceName", ServiceNameInfo
            set ServiceName = *($(ServiceNameInfo), 4)

            ;
            ; Change the NetRule if necessary
            ;
            OpenRegKey $(NetworkCardKey) "" "NetRules" +
                $(MAXIMUM_ALLOWED) NetRuleKey
            Ifstr(i) $(NetRuleKey) != $(KeyNull)
                ;
                ; Make the change....
                ;
            else
                ;
                ; Error, cannot open net rules key
                ;
                goto fatalregistry
            endif

            CloseRegKey $(NetRules)
            CloseRegKey $(NetworkCardKey)
        else
            ;
            ; Error, cannot open network card key
            ;
            goto fatalregistry
        endif
        ;
        ; 3. Change the service section of the hardware. i.e.,
        ;    ParameterName change, value change, etc.
        ;
        OpenRegKey $(!REG_H_LOCAL) "" +
              $(!NTN_ServiceBase)"\"$(ServiceName) +
              $(MAXIMUM_ALLOWED) ServiceKey

        Ifstr(i) $(ServiceKey) != $(KeyNull)
            ;
            ; Get the ServiceKey to change the Start value
            ; or Type value. Or open Parameters key to
            ; change the hardware parameters if necessary.
            ;
            CloseRegKey $(ServiceKey)
        else
            ;
            ; Error, cannot open network card key
            ;
            goto fatalregistry
        endif
    endif

    goto end
    ;
    ; End of Upgrade Software
    ;

;
;  Escape hatches
;
successful = +
    goto end

abandon = +
    ForListDo $(OEM_ABANDON_OPTIONS)
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $($)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    EndForListDo

    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
        ; Remove Software Component
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), FALSE
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    endif

    goto end

;
; warning display
;
warning = +
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
        goto $(from)
    else
        goto "end"
    endif
;
; non fatal error display
;
nonfatalinfo = +
    Set Severity = STATUS
    Set CommonStatus = STATUS_USERCANCEL
    goto nonfatalmsg
nonfatal = +
    Set Severity = NONFATAL
    goto nonfatalmsg
nonfatalmsg = +
    ifstr(i) $(Error) == ""
        Set Severity = NONFATAL
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), $(Severity), $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(from)
    else
        goto "end"
    endif

;
;  Registry is broken
;
fatalregistry = +
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
;
;  Netcard detection failure
;
fataldetect = +
    Shell $(UtilityInf),RegistryErrorString,CANNOT_DETECT
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error: cannot get an error string."
        goto ShellCodeError
    endif
    set Error = $($R0)
    Goto fatal
;
; fatal error display
;
fatal = +
    ifstr(i) $(Error) == ""
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif

    goto setfailed

;
;  Shelling error
;
ShellCodeError = +
    set DlgType      = "MessageBox"
    set STF_MB_TITLE = $(ShellCodeErrorTitle)
    set STF_MB_TEXT  = $(ShellCodeErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed

setfailed = +
    set CommonStatus = STATUS_FAILED
    ;
    ; if OEM_ABANDON_ON == TRUE, then remove the registry entries
    ;
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
        set OEM_ABANDON_ON = FALSE
        goto abandon
    endif
    goto end

end = +
    goto term

term = +

    Return $(CommonStatus)

[DebugConfiguration]

    Set InfName = "OEMSETNT.INF"
    ;Debug-Output $(InfName)" **CONFIGURATION STATE: "$($0)
    ;Debug-Output $(InfName)" IRQ_Level is "$(!p:IRQ_Level)
    ;Debug-Output $(InfName)" IOBaseAddrValue is "$(!p:IOBaseAddrValue)
    ;Debug-Output $(InfName)" TransceiverValue is "$(!p:TransceiverValue)
    ;Debug-Output $(InfName)" MemoryAddr is "$(!p:MemoryAddr)
    ;Debug-Output $(InfName)" MappedValue is "$(!p:MappedValue)

    return


;***************************************************************
;  INSTALL SECTIONS
;***************************************************************
[Install-Option]
    set STF_VITAL = ""

    ifstr(i) $(AddCopy) == "YES"

        AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

    endif

    ifstr(i) $(DoCopy) == "YES"

       ;
       ; Copy files in the copy list
       ;
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList

    endif

    Exit

[Install-Update]
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   ;set STF_VERSION     = "YES"

   AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
   AddSectionFilesToCopyList Files-Inf $(SrcDir) $(!STF_WINDOWSSYSPATH)

   set !STF_NCPA_FLUSH_COPYLIST = TRUE
   CopyFilesInCopyList

   exit


[Install-Dll]
   set STF_VITAL 	= ""
   AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
   set !STF_NCPA_FLUSH_COPYLIST = TRUE
   CopyFilesInCopyList
   exit





[Source Media Descriptions]
    1  = "Xircom Setup Disk for NT"


[ProductType]
STF_PRODUCT  = Winnt
STF_PLATFORM = I386


[Files-Inf]
1, OEMSETNT.INF, SIZE=58000,	RENAME=$(!UG_Filename)

[Files-Dll]
1, CE3.DLL,  SIZE=21000

[Files-CE3NT]
1, CE3NT.SYS, SIZE=53000

[LanguagesSupported]
    ENG

[AllFileConstantsENG]
ProCaption   = "Windows NT Setup"
ProCancel    = "Cancel"
ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
               "Are you sure you want to cancel copying files?"
ProCancelCap = "Network Setup Message"
ProText1     = "Copying:"
ProText2     = "To:"
DialogDllName     = "CE3.DLL"






; START CE3 -------------------------------------------------------------------------------------------

[FileConstantsENG-CE3NT]
FunctionTitle		= $(GenericAdapterName)" Setup"$(GenericInfVersion)
ProductSoftwareTitle	= $(GenericDriverName)
ProductHardwareTitle	= $(GenericAdapterName)
IRQList			= ^(IRQChoices, 1)
IRQValues		= ^(IRQChoices, 2)
IOBaseAddrList		= ^(IOBaseAddrChoices, 1)
IOBaseAddrValues	= ^(IOBaseAddrChoices, 2)
MemoryAddrList		= ^(MemoryAddrChoices,1)
MemoryAddrValues	= ^(MemoryAddrChoices,2)
CableTypeList		= ^(CableTypeChoices, 1)
CableTypeValues		= ^(CableTypeChoices, 2)
ModeList		= ^(ModeChoices, 1)
ModeValues		= ^(ModeChoices, 2)
LineSpeedList		= ^(LineSpeedChoices, 1)
LineSpeedValues		= ^(LineSpeedChoices, 2)
LineModeList		= ^(LineModeChoices, 1)
LineModeValues		= ^(LineModeChoices, 2)
InitDelayList           = ^(InitDelayChoices, 1)
InitDelayValues         = ^(InitDelayChoices, 2)


[DialogConstantsENG-CE3NT]
Help        = "&Help"
Exit        = "Cancel"
OK          = "OK"
HelpContext = ""
Continue    = "Continue"
Cancel      = "Cancel"

[FileDependentDlgENG-CE3NT]
DlgType = "RadioCombination"
;*****************************************************************************
; DO NOT CHANGE THE DlgTemplate.  THIS NEEDS TO BE CE3
;*****************************************************************************
DlgTemplate = "CE3"
Caption = $(FunctionTitle)
HelpContext = $(!IDH_DB_OEMNADE2_INS)
CBOptionsGreyed = {}
NotifyFields = {NO, NO, NO, NO, NO, NO, NO, NO, NO}
Combo1Label = "I/O Port:"
Combo2Label = "Memory Address:"
Combo3Label = "Interrupt:"
Combo4Label = "Mode:"
Combo5Label = "Cable Type:"
Combo6Label = "Line Speed:"
Combo7Label = "Line Mode:"
Combo8Label = "Initialization Delay:"
Check1 = "&Early Transmit"
Check2 = "Link &Integrity"
Check3 = "Dynamic &Link Detect"
Combo1List = $(IOBaseAddrList)
Combo1Out  = $(IOBaseAddrValue)
Combo2List = $(MemoryAddrList)
Combo2Out  = $(MemoryAddrValue)
Combo3List = $(IRQList)
Combo3Out  = $(IRQValue)
Combo4List = $(ModeList)
Combo4Out  = $(ModeValue)
Combo5List = $(CableTypeList)
Combo5Out  = $(CableTypeValue)
Combo6List = $(LineSpeedList)
Combo6Out  = $(LineSpeedValue)
Combo7List = $(LineModeList)
Combo7Out  = $(LineModeValue)
Combo8List = $(InitDelayList)
Combo8Out  = $(InitDelayValue)
ComboListItemsIn  = {Combo1List,Combo2List,Combo3List, Combo4List, Combo5List, Combo6List, Combo7List, Combo8List}
ComboListItemsOut = {Combo1Out, Combo2Out, Combo3Out, Combo4Out, Combo5Out, Combo6Out, Combo7Out, Combo8Out}

CheckItemsIn = {$(EarlyTransmitValue),$(LinkIntegrityValue),$(DynamicLinkDetectValue)}
CheckItemsOut = {Check1Out, Check2Out, Check3Out}
EditTextIn  = {"",""}
EditTextLim = {"",""}


; END CE3 -------------------------------------------------------------------------------------------


[MemoryAddrChoices]
MA_0  = "Auto Detect" , 4294967295
MA_1  = "0xA0000", 655360
MA_2  = "0xA1000", 659456
MA_3  = "0xA2000", 663552
MA_4  = "0xA3000", 667648
MA_5  = "0xA4000", 671744
MA_6  = "0xA5000", 675840
MA_7  = "0xA6000", 679936
MA_8  = "0xA7000", 684032
MA_9  = "0xA8000", 688128
MA_10 = "0xA9000", 692224
MA_11 = "0xAA000", 696320
MA_12 = "0xAB000", 700416
MA_13 = "0xAC000", 704512
MA_14 = "0xAD000", 708608
MA_15 = "0xAE000", 712704
MA_16 = "0xAF000", 716800
MA_17 = "0xB0000", 720896
MA_18 = "0xB1000", 724992
MA_19 = "0xB2000", 729088
MA_20 = "0xB3000", 733184
MA_21 = "0xB4000", 737280
MA_22 = "0xB5000", 741376
MA_23 = "0xB6000", 745472
MA_24 = "0xB7000", 749568
MA_25 = "0xB8000", 753664
MA_26 = "0xB9000", 757760
MA_27 = "0xBA000", 761856
MA_28 = "0xBB000", 765952
MA_29 = "0xBC000", 770048
MA_30 = "0xBD000", 774144
MA_31 = "0xBE000", 778240
MA_32 = "0xBF000", 782336
MA_33 = "0xC0000", 786432
MA_34 = "0xC1000", 790528
MA_35 = "0xC2000", 794624
MA_36 = "0xC3000", 798720
MA_37 = "0xC4000", 802816
MA_38 = "0xC5000", 806912
MA_39 = "0xC6000", 811008
MA_40 = "0xC7000", 815104
MA_41 = "0xC8000", 819200
MA_42 = "0xC9000", 823296
MA_43 = "0xCA000", 827392
MA_44 = "0xCB000", 831488
MA_45 = "0xCC000", 835584
MA_46 = "0xCD000", 839680
MA_47 = "0xCE000", 843776
MA_48 = "0xCF000", 847872
MA_49 = "0xD0000", 851968
MA_50 = "0xD1000", 856064
MA_51 = "0xD2000", 860160
MA_52 = "0xD3000", 864256
MA_53 = "0xD4000", 868352
MA_54 = "0xD5000", 872448
MA_55 = "0xD6000", 876544
MA_56 = "0xD7000", 880640
MA_57 = "0xD8000", 884736
MA_58 = "0xD9000", 888832
MA_59 = "0xDA000", 892928
MA_60 = "0xDB000", 897024
MA_61 = "0xDC000", 901120
MA_62 = "0xDD000", 905216
MA_63 = "0xDE000", 909312
MA_64 = "0xDF000", 913408
MA_65 = "0xE0000", 917504
MA_66 = "0xE1000", 921600
MA_67 = "0xE2000", 925696
MA_68 = "0xE3000", 929792
MA_69 = "0xE4000", 933888
MA_70 = "0xE5000", 937984
MA_71 = "0xE6000", 942080
MA_72 = "0xE7000", 946176
MA_73 = "0xE8000", 950272
MA_74 = "0xE9000", 954368
MA_75 = "0xEA000", 958464
MA_76 = "0xEB000", 962560
MA_77 = "0xEC000", 966656
MA_78 = "0xED000", 970752
MA_79 = "0xEE000", 974848
MA_80 = "0xEF000", 978944
MA_81 = "0xF0000", 983040
MA_82 = "0xF1000", 987136
MA_83 = "0xF2000", 991232
MA_84 = "0xF3000", 995328
MA_85 = "0xF4000", 999424
MA_86 = "0xF5000", 1003520
MA_87 = "0xF6000", 1007616
MA_88 = "0xF7000", 1011712
MA_89 = "0xF8000", 1015808
MA_90 = "0xF9000", 1019904
MA_91 = "0xFA000", 1024000
MA_92 = "0xFB000", 1028096
MA_93 = "0xFC000", 1032192
;MA_94 = "0xFD000", 1036288
;MA_95 = "0xFE000", 1040384

[IRQChoices]
;Interrupts available on the PCIC: { 3,4,5,7,8,10,11,12,14,15 }
;Interrupts available on the TCIC: { 3,4,5,6,7,10,14 }
;14 = fixed disk
;12 = keyboard
;6  = floppy disk
;union(PCIC, TCIC) - {14} = 3,4,5,7,10
IRQ_0 = "Auto Detect" , 0
IRQ_1 = "3",3
IRQ_2 = "4",4
IRQ_3 = "5",5
IRQ_4 = "7",7
IRQ_5 = "9",9
IRQ_6 = "10",10
IRQ_7 = "11",11
IRQ_8 = "15",15
;CE3 10/100 mode values
[ModeChoices]
MO_1 = "I/O", 0
MO_2 = "Memory Mapped", 1

[CableTypeChoices]
CT_1 = "Auto Detect", 0
CT_2 = "10BT/100BTX (TP)", 1
CT_3 = "10B2 (Coax)", 2

[LineSpeedChoices]
LS_1 = "Auto Detect", 0
LS_2 = "10 Mbps", 1
LS_3 = "100 Mbps", 2

[LineModeChoices]
LM_1 = "Auto Detect", 0
LM_2 = "Half Duplex", 1
LM_3 = "Full Duplex", 2

[IOBaseAddrChoices]
; 0x3E0 is where PCIC is located
; 0x240 is where TCIC is located
; therefore user cannot select these for locating the ethernet adapter
IOBase_0  = "Auto Detect" , 65535
IOBase_1  = "0x200",512
IOBase_2  = "0x210",528
IOBase_3  = "0x220",544
IOBase_4  = "0x230",560
;IOBase_5  = "0x240",576
IOBase_6  = "0x250",592
IOBase_7  = "0x260",608
IOBase_8  = "0x270",624
IOBase_9  = "0x280",640
IOBase_10 = "0x290",656
IOBase_11 = "0x2A0",672
IOBase_12 = "0x2B0",698
IOBase_13 = "0x2C0",714
IOBase_14 = "0x2D0",730
IOBase_15 = "0x2E0",746
IOBase_16 = "0x2F0",752
IOBase_17 = "0x300",768
IOBase_18 = "0x310",784
IOBase_19 = "0x320",800
IOBase_20 = "0x330",816
IOBase_21 = "0x340",832
IOBase_22 = "0x350",848
IOBase_23 = "0x360",864
IOBase_24 = "0x370",880
IOBase_25 = "0x380",896
IOBase_26 = "0x390",912
IOBase_27 = "0x3A0",928
IOBase_28 = "0x3B0",944
IOBase_29 = "0x3C0",960
IOBase_30 = "0x3D0",976

[InitDelayChoices]
InitD_0 = "0",0
InitD_1 = "1",1
InitD_2 = "2",2
InitD_3 = "3",3
InitD_4 = "4",4
InitD_5 = "5",5
InitD_6 = "10",10
InitD_7 = "20",20
InitD_8 = "30",30
InitD_9 = "40",40
InitD_10 = "50",50
InitD_11 = "60",60
