[CE3OS2_NIF]
Type = NDIS
Title = "Xircom Ethernet Adapter 10/100"
Version = 2.00 (960603)
DriverName = XIRCOM$
XPORTS = NETBEUI LANDD

[File]
Name = CE3NDIS.OS2
Path = IBMCOM\MACS

[MEMORY]
Display   = "Adapter memory address"
Type      = HexNum
Range     = C000-EC00
Step      = 100
Optional  = Yes
help = "Use this parameter to set the base memory address of 
the adapter in hexadecimal notation.  The adapter supports a 
full 32-bit address space.  If the adapter is using IO mode, 
this memory window is only used during initialization."

[IOADDRESS]
Display   = "Adapter IO address"
Type      = HexNum
Range     = 240-380
Step      = 20
Optional  = Yes
help = "Use this parameter to set the base I/O address of 
the adapter in hexadecimal notation.  The adapter supports 
16-bits of I/O address space, and requires 128 contiguous 
I/O addresses if run in I/O mode.  If using memory-mapped 
I/O mode, no I/O ports are necessary and this field should 
be left blank."

[IRQ]
Display   = "Adapter IRQ number"
Type      = Decimal
Range     = 3-15
Optional  = Yes
help = "This parameter selects a hardware interrupt for use 
by the adapter."

[SOCKET]
Display   = "PC card socket"
Type      = Decimal
Range     = 1-2
Optional  = Yes
help = " This parameter can be used to force the driver to 
use a particular PC card socket (or slot).  Normally this 
field should be left blank and the driver will automatically 
detect the adapter.  Using this parameter will override the 
detection and force the driver to use only the socket specified."

[MODE]
Display   = "Adapter address mode"
Type      = String
StrLength = 6
Set       = MEMORY, IO
Optional  = Yes
help = "This parameter will select a particular operating 
mode for the driver.  If MEMORY is selected, or this parameter 
is left blank, the driver will run in memory-mapped IO mode.  
In this situation the adapter IO address field should be left 
blank.  If IO is selected, the driver will run in I/O mode."

[WORDSIZE]
Display   = "Network data path size"
Type      = Decimal
Set       = 8, 16
Optional  = Yes
help = "This parameter specifies the size of the data path for 
the LAN controller.  Values are 8 or 16 decimal."

[NOCHECK]
Display   = "Disable resource checking?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter disables verification of adapter resources. 
If the driver resource detection and verification code is causing 
problems when the driver loads, this keyword can be used to turn 
the feature off."

[NOLED]
Display   = "Disable LEDs?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter is used to turn the dongle LEDs off. 
This might be helpful on a mobile computer and may result 
in a modest increase in battery life."

[TXBUFFERSIZE]
Display   = "Transmit buffers size (in packets)"
Type      = Decimal
Range     = 1-20
Optional  = Yes
help = "This parameter sets the size of the adapters transmit 
packet buffer.  This is the number of transmit packets in decimal 
in the range 1-20.  Each packet adds approximately 1520 bytes to 
the resident size of the driver."

[NOEARLYRX]
Display   = "Disable faster receives?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter disables Advanced Look-ahead Pipelining 
features of the Xircom CreditCard Ethernet Adapter IIps.  You may 
need this keyword for NDIS drivers that do not fully support 
the "early RX" feature."

[NOEARLYTX]
Display   = "Disable faster transmits?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter disables early transmit features of Xircom 
CreditCard Ethernet Adapter IIps.  Try using this keyword if you are 
experiencing a large number of transmit overruns."

[LINESPEED]
Display   = "Force operation at 10 or 100 Mbps."
Type      = Decimal
Set       = 10, 100
Optional  = Yes
Help = "This parameter forces operation at 10 or 100 Mbps.  If the
keyword is not stated, the line speed will be automatically detected."

[LINEMODE]
Display   = "Line duplex mode"
Type      = String
StrLength = 4
Set       = HALF, FULL
Optional  = Yes
help = "This parameter selects either half-duplex or full-duplex
mode for the network.  Valid parameters are HALF or FULL.
Selecting full-duplex enables the adapter to send and receive
data simultaneously when connected to a full-duplex hub.  If
left blank the line mode will be determined automatically using
N-Way autonegotiation."

[LINKDISABLE]
Display   = "Disable link integrity?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter is used to turn link integrity checking
off.  Some older network configurations may require this parameter
to be set."

[COAX]
Display   = "Force Coaxial cabling?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter is used to force coaxial (10BASE-2)connection."

[TP]
Display   = "Force Twisted Pair cabling?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter is used to force Twisted Pair connection."

[VERBOSE]
Display   = "Enable verbose messages?"
Type      = None
Set       = "Yes", "No"
Optional  = Yes
help = "This parameter is used to turn on detailed information when
the driver initializes.  This information includes the type of PCI
bridge controller found."

