; Xircom Ethernet Adapter 10/100 ODI LDI File
; (c) Copyright 1999 by Xircom, Inc.  All rights reserved
VER: 1.00
SYN: 1.00

DR CE3ODI
{
   DES:  $CE3ODI_DES
   HELP: $CE3ODI_HELP
   PAR:  1.00
   FILE: CE3ODI.LAN
   ;@#   SPROD: 'Xircom~Ethernet Adapter 10/100'
   ;@#   CLIENT: CE3ODI.COM, CE3ODI.LAN
   ;@#   ALIAS: CE3ODI.LAN

   FR FrameSelect
   {
      CH:  'Ethernet_802.2'
      CH:  'Ethernet_802.3'
      CH:  'Ethernet_SNAP'
      CH:  'Ethernet_II'
      DEF: 1,2
   }

   PR IRQ OPTIONAL
   {
      VAL:      3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15
      TYP:      DECIMAL(2)
      OUT:      'IRQ=%s'
      HELP:     $CE3ODI_IRQ_HELP
   }

   PR PORT OPTIONAL
   {
      DES:      'IO Address'
      VAL:      280-380
      TYP:      HEX(3)
      RES:      20
      OUT:      'PORT=%s'
      HELP:     $CE3ODI_PORT_HELP
   }

   PR MEMORY OPTIONAL
   {
      DES:      'Memory Address'
      VAL:      C0000-EFFFF
      TYP:      HEX(8)
      RES:      1000
      OUT:      'MEM=%s'
      HELP:     $CE3ODI_MEMORY_HELP
   }

   PR NODE
   {
   }

   PR SOCKET
   {
      DES:  "PC Card Socket Number"
      VAL:  1-4
      TYP:  DECIMAL(1)
      OUT:      "SOCKET=%s"
      HELP:     $CE3ODI_SOCKET_HELP
   }

   LI NOCHECK
   {
      DES:      'Disable resource checking?'
      CD:       $YES
      CH:       'NOCHECK'
      CD:       $NO
      CH:       ''
      DEF:      2
      OUT:      '%s'
      HELP:     $CE3ODI_NOCHECK_HELP
   }

   LI VERBOSE
   {
      DES:      'Enable verbose messages?'
      CD:       $YES
      CH:       'VERBOSE'
      CD:       $NO
      CH:       ''
      DEF:      2
      OUT:      '%s'
      HELP:     $CE3ODI_VERBOSE_HELP
   }

   PR TXBUFFERSIZE
   {
      DES:      'Transmit buffer size'
      TYP:      DECIMAL(2)
      VAL:      1-20
      OUT:      'TXBUFFERSIZE=%s'
      HELP:     $CE3ODI_TXBUFFERSIZE_HELP
   }

  LI NOEARLYRX
   {
      DES:      'Disable early receives?'
      CD:       $YES
      CH:       'NOEARLYRX'
      CD:       $NO
      CH:       ''
      DEF:      2
      OUT:      '%s'
      HELP:     $CE3ODI_NOEARLYRX_HELP
   }

   LI NOEARLYTX
   {
      DES:      'Disable early transmits?'
      CD:       $YES
      CH:       'NOEARLYTX'
      CD:       $NO
      CH:       ''
      DEF:      2
      OUT:      '%s'
      HELP:     $CE3ODI_NOEARLYTX_HELP
   }

   LI LINESPEED
   {
      DES:      'Line speed'
      CD:       '10 Mbits per second'
      CH:       'LINESPEED=10'
      CD:       '100 Mbits per second'
      CH:       'LINESPEED=100'
      CD:       'AUTO'
      CH:       ''
      DEF:      3
      OUT:      '%s'
      HELP:     $CE3ODI_LINESPEED_HELP
   }

   LI LINEMODE
   {
      DES:      'Line duplex mode'
      CD:       'FULL'
      CH:       'LINEMODE=FULL'
      CD:       'HALF'
      CH:       'LINEMODE=HALF'
      CD:       'AUTO'
      CH:       ''
      DEF:      3
      OUT:      '%s'
      HELP:     $CE3ODI_LINEMODE_HELP
   }

   LI NOLED
   {
      DES:      'Disable LEDs?'
      CD:       $YES
      CH:       'NOLED'
      CD:       $NO
      CH:       ''
      DEF:      2
      OUT:      '%s'
      HELP:     $CE3ODI_NOLED_HELP
   }

   LI LINKDISABLE
   {
      DES:      'Disable link integrity?'
      CD:       $YES
      CH:       'LINKDISABLE'
      CD:       $NO
      CH:       ''
      DEF:      2
      OUT:      '%s'
      HELP:     $CE3ODI_LINKDISABLE_HELP
   }

}

;English
DLANG: 4
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."

$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in hexadecimal 
		   notation. The adapter supports 16-bits of I/O address
		   space, and requires 128 contiguous I/O addresses if run
		   in I/O mode. If using memory-mapped I/O mode, no I/O 
		   ports are necessary and this field should be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;French
LANG: 6
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;German
LANG: 7
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;Italian
LANG: 8
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;Spanish
LANG: 14
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."
                        


;Portugese
LANG: 12
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."

$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in hexadecimal 
		   notation. The adapter supports 16-bits of I/O address
		   space, and requires 128 contiguous I/O addresses if run
		   in I/O mode. If using memory-mapped I/O mode, no I/O 
		   ports are necessary and this field should be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;Japanese
LANG: 9
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;Korean
LANG: 10
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;Chinese (Simplified)
LANG: 1
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."

;Chinese (Traditional)
LANG: 16
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."
;Russian
LANG: 13
$CE3ODI_DES =  "Xircom Ethernet Adapter 10/100"

$YES = "YES"
$NO = "NO"


$CE3ODI_HELP = "This driver supports CE3ODI adapters for computers that have
	     a PC Card slot. This driver will support up to four adapters
	     as long as the MEMORY, IRQ, and optionally IOADDRESS, keywords
	     are set to different values"

$CE3ODI_IRQ_HELP =        "Selects a hardware interrupt for use by the adapter."
		
$CE3ODI_PORT_HELP = "Sets the base I/O address of the adapter in
		 hexadecimal notation. The adapter supports
		16-bits of I/O address space, and requires 128 contiguous
		I/O addresses if run in I/O mode. If using memory-mapped
		I/O mode, no I/O ports are necessary and this field should
		be left blank."

$CE3ODI_MEMORY_HELP = "Sets the base memory address of the adapter in
		   hexadecimal notation."

$CE3ODI_SOCKET_HELP = "Forces the driver to use a particular PC Card socket
		   (or slot). Overrides automatic detection."

$CE3ODI_NOCHECK_HELP = "Disables verification of adapter resources."

$CE3ODI_VERBOSE_HELP = "Turns on detailed initialization information,
		    including the type of PCMCIA controller found."

$CE3ODI_TXBUFFERSIZE_HELP = "Sets the size of the adapter's transmit
			 packet buffer. Each packet adds approximately
			 1520 bytes to the resident size."

$CE3ODI_NOEARLYRX_HELP = "Disables Advanced Look-ahead Pipelining features of the adapter.
		      Using this keyword may negatively impact performance."

$CE3ODI_NOEARLYTX_HELP = "Disables early transmit.
		      Using this keyword may negatively impact performance."

$CE3ODI_LINESPEED_HELP = "Forces operation to 10 or 100 Mbps.
		       If AUTO is selected the line speed will be
		       automatically detected (default)."

$CE3ODI_LINEMODE_HELP = "Forces half-duplex or full-duplex mode for the network.
		     If AUTO is selected the line mode will
		     be determined automatically."

$CE3ODI_NOLED_HELP = "Turns the dongle LEDs off.
		  This might be helpful on a mobile computer
		  and may result in a modest increase in battery life."

$CE3ODI_LINKDISABLE_HELP = "Turns link integrity checking off.
			Some older network configurations may require
			this parameter to be set."
                        
