InS_StArT
CE3ODI.COM
^Xircom Ethernet Adapter 10/100,CE3ODI.COM,IEM
?Installation for the Xircom Ethernet Adapter 10/100.
!OIEM(INT) Hardware Interrupt
?The default hardware interrupt is 5.
3  
4
@5
6
7
8
9
10
11
12
13
14
15
!OIEM(PORT) Base I/O Port Address
?The default base I/O port address value is 320.
240
260
280
2A0
2C0
2E0
300
@320
340
360
380
!OIEM(MEM) Memory I/O Address
?The default memory I/O address value is D2000.
C0000
@D2000
E8000
*OIEM(FRAME) Frame type
?The latest ODI Specification uses Ethernet_802.2 as the default frame type.  If your network requires something other than Ethernet_802.2, then make sure to specify the correct frame type.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
