#

Table of Contents | Previous Page | Next Page

# Ethernet 10/100+Modem 56
Regulatory and Safety Notices

This section provides the following notices:

- FCC Regulations
- Canadian Department of Communications
- European Community - CE Mark
- Japan Regulatory Notices
- New Zealand Telepermit
- Safety Notices

### FCC Regulations - Part 15

#### Declaration of Conformity (DoC)

Xircom, Inc. declares that the equipment described in this document is within the requirements of the Code of Federal Regulations listed below:

Title 47 Part 15, Subpart B, Class B for a digital device.

This declaration is based upon compliance of the Xircom RealPort Ethernet 10/100+Modem 56 model REM56G-100 or CreditCard Ethernet 10/100+Modem 56 model CEM56-100 to the above standards. Xircom has determined that these models have been shown to comply with the applicable technical standards if no unauthorized change is made in the equipment and if the equipment is properly maintained and operated.

These units are identical to the units tested and found acceptable with the applicable standards. Records maintained by Xircom continue to reflect that units being produced under this Declaration of Conformity, within the variation that can be expected due to quantity production and tested on a statistical basis, continue to comply with the applicable technical standards.

R.W. Bass
Vice President, Operations
Xircom, Inc.
2300 Corporate Center Drive
Thousand Oaks, California 91320 U.S.A.

#### FCC Rules and Regulations - Part 15

This device complies with part 15 of the FCC Rules. Operation is subject to the following two conditions: (1) this device may not cause harmful interference, and (2) This device must accept any interference received, including interference that may cause undesired operation.

The Xircom RealPort Ethernet 10/100+Modem 56 model REM56G-100 and CreditCard Ethernet 10/100+Modem 56 model CEM56-100 complies with the FCC Rules for Class B digital devices. As required by FCC Rules and Regulations, the following Class B information is provided for the guidance of the user.

WARNING: This equipment has been tested and found to comply with the limits for Class B digital devices pursuant to Part 15 of the FCC Rules. These limits are designed to provide reasonable protection against harmful interference in a residential installation. This equipment generates, uses, and can radiate radio frequency energy and, if not installed and used in accordance with the instructions, may cause harmful interference to radio communications. However, there is no guarantee that interference will not occur in a particular installation. If this equipment does cause harmful interference to radio or television reception, which can be determined by turning the equipment off and on, the user is encouraged to try to correct the interference by one or more of the following measures:

- Reorient or relocate the receiving antenna.
- Increase the separation between the equipment and the receiver.
- Connect the equipment into an outlet on a circuit different from that to which the receiver is connected.
- Consult the dealer or an experienced radio/TV technician for help.

Changes or modifications to the digital device not expressly approved by Xircom Inc. could void the user's authority to operate the equipment.

It is suggested that only shielded and grounded cables be used with the equipment to ensure compliance with FCC rules.

  NOTE: When the Ethernet 10Base-2 (B2) adapter cable supplied with model CEM56-100BC, or as a separately purchased accessory, is connected to the CreditCard Ethernet 10/100+Modem 56, the unit complies with FCC Part 15 Class A requirements for office use. As required by FCC Rules and Regulations, the following information is provided for the guidance of the user.
  WARNING: This equipment has been tested and found to comply with the limits for Class A digital devices pursuant to Part 15 of the FCC Rules. These limits are designed to provide reasonable protection against harmful interference when the equipment is operated in a commercial environment. This equipment generates, uses, and can radiate radio frequency energy and, if not installed and used in accordance with the instruction manual, may cause interference to radio communications. Operation of this equipment in a residential area is likely to cause interference, in which case the user will be required to correct the interference at his own expense.
  Changes or modifications to the digital device not expressly approved by Xircom Inc. could void the user’s authority to operate the equipment.
  It is suggested that only shielded and grounded cables be used with the equipment to ensure compliance with FCC rules.

### FCC Regulations - Part 68

To comply with the Federal Communications Commission (FCC) Rules and Regulations, Parts 68, these instructions must be followed:

1. Your modem must not be connected to a party line or coin-operated telephone.
2. If a problem occurs on the telephone line, your modem must be disconnected from the telephone line until it has been determined that your modem is not the cause of the problem.
3. All repairs to your modem must be made by Xircom, Inc. Unauthorized or unorthodox repair methods can alter the modem's radio frequency emissions and other characteristics sufficiently to void your authority to operate the modem over a public telephone network.
4. If requested, you must be prepared to provide the telephone company with the following information:

Equipment Manufacturer: Xircom, Inc.
2300 Corporate Center Drive
Thousand Oaks, CA 91320-1420 U.S.A.
Models: REM56G-100, CEM56-100
FCC Registration Number: See the unit.
Ringer Equivalency No.: See the unit.

This equipment complies with Part 68 of the FCC Rules. On the back of the unit is a label that contains, among other information, the FCC Registration Number and Ringer Equivalency Number (REN) for this equipment. You must, upon request, provide this information to your telephone company.

This equipment uses the following USOC jacks: RJ-11, RJ-45.

An FCC compliant telephone cord and modular plug are provided with this equipment. This equipment is designed to be connected to the telephone network or premises wiring using a compatible modular jack which is Part 68 compliant. See installation instructions for details.

The REN is useful to determine the quantity of devices you may connect to your telephone line and still have all those devices ring when your telephone number is called. In most but not all areas, the sum of the RENs of all devices connected to one line should not exceed five (5.0). To be certain of the number of devices you may connect to your line, as determined by the REN, you should contact your local telephone company to determine the maximum REN for your calling area.

If the Xircom terminal equipment causes harm to the telephone network, the telephone company may discontinue your service temporarily. If possible, they will notify you in advance. But if advance notice is not practical, you will be notified as soon as possible. You will be informed of your right to file a complaint with the FCC.

The telephone company may make changes in its facilities, equipment, operations or procedures that could affect the operation of the equipment. If this happens, the telephone company will provide advance notice in order for you to make necessary modifications to maintain uninterrupted service.

If you experience trouble with this telephone equipment, please contact Xircom, Inc. at (805) 376-9200 for information on obtaining service or repairs. If the equipment is causing harm to the telephone network, the telephone company may request you to disconnect the equipment until the problem is resolved.

There are no user serviceable parts contained in this equipment.

This equipment may not be used on public coin phone service provided by the telephone company. Connection to party line service is subject to state tariffs.

The Telephone Consumer Protection Act of 1991 makes it unlawful for any person to use a computer or other electronic device, including fax machines, to send any message unless such message clearly contains in a margin at the top or bottom of each transmitted page or on the first page of the transmission, the date and time it is sent and an identification of the business or other entity, or other individual sending the message and the telephone number of the sending machine or such business, other entity, or individual. (The telephone number provided may not be a 900 number or any other for which charges exceed local or long-distance transmission charges.)

In order to program this information into your fax software, you should refer to the manual of the fax software being used.

### Canadian Department Of Communications

#### Industry Canada (IC) Notice

This digital apparatus does not exceed the Class B limits for radio noise emissions from digital apparatus set out in the Radio Interference Regulations of the Canadian Department of Communications.

Le présent appareil numérique n'émet pas de bruits radioélectriques dépassant les limites applicables aux appareils numériques de Classe B prescrites dans le règlement sur le brouillage radioélectrique édicté par le Ministère des Communications du Canada.

  NOTE: When the Ethernet 10Base-2 (B2) adapter cable supplied with model CEM56-100BC, or as a separately purchased accessory, is connected to the CreditCard Ethernet 10/100+Modem 56, the unit complies with Class A requirements for office use. As required by IC Rules and Regulations, the following information is provided for the guidance of the user.
  This digital apparatus does not exceed the Class A limits for radio noise emissions from digital apparatus set out in the Radio Interference Regulations of the Canadian Department of Communications.
  Le présent appareil numérique n'émet pas de bruits radioélectriques dépassant les limites applicables aux appareils numériques de Classe A prescrites dans le règlement sur le brouillage radioélectrique édicté par le Ministère des Communications du Canada.

NOTICE: The Industry Canada (IC) label identifies certified equipment. This certification means that the equipment meets telecommunications network protective, operational and safety requirements as prescribed in the appropriate Terminal Equipment Technical Requirements document(s). The department does not guarantee the equipment will operate to the user's satisfaction.

Before installing this equipment, users should ensure that it is permissible to be connected to the facilities of the local telecommunications company. The equipment must also be installed using an acceptable method of connection. The customer should be aware that compliance with the above conditions may not prevent degradation of service in some situations.

Repairs to certified equipment should be coordinated by a representative designated by the supplier. Any repairs or alterations made by a user to this equipment, or equipment malfunctions, may give the telephone communications company cause to request the user to disconnect the equipment.

Users should ensure for their own protection, that the electrical ground connections of the power utility, telephone lines and internal metallic water pipe system, if present, are connected together. This precaution may be particularly important in rural areas.

Caution: Users should not attempt to make such connections themselves, but should contact the appropriate electric inspection authority, or electrician, as appropriate.

NOTICE: The Ringer Equivalence Number (REN) assigned to each terminal device provides an indication of the maximum number of terminals allowed to be connected to a telephone interface. The termination on an interface may consist of any combination of devices subject only to the requirement that the sum of the Ringer Equivalence Numbers of all the devices does not exceed 5.

REN: See back of unit.

Warranty and Repair Service Center:

Xircom, Inc.
2300 Corporate Center Drive
Thousand Oaks, CA 91320-1420 U.S.A.
Phone: (805) 376-9200

## European Community - CE Mark

#### Declaration of Conformity

Xircom, Inc. declares that the equipment described in this document is in conformance with the requirements of the European Council Directive listed below:

73/23/EEC Low Voltage Directive with Amendment 93/68/EEC
89/336/EEC EMC Directive with Amendments 92/31/EEC and 93/68/EEC
1999/5/EC Radio and Telecommunications Terminal Equipment Directive

This declaration is based upon compliance of the product to the following standards:

EN 55022 Class B (CISPR 22 Class B) RF Emissions Control
EN 50082-1 (IEC 801-2, 3, 4) Immunity to Electromagnetic Disturbance
EN 60950 2nd Edition (A1 - A4) Safety of Information Technology Equipment, Including Electrical Business Equipment
TBR21 Analogue PSTN Standard with Advisory Notes in ETSI Guides EG 201 120 and EG 201 121

Product Descriptions: Xircom RealPort Ethernet 10/100+Modem 56 model REM56G-100 and CreditCard Ethernet 10/100+Modem 56 model CEM56-100

R.W. Bass,
Vice President, Operations
Xircom, Inc.
2300 Corporate Center Drive
Thousand Oaks, California 91320 U.S.A.

The CE Mark approval is indicated on your Xircom modem by the CE Mark logo on the back of the card. Country-specific approval numbers are no longer required. The CE Mark logo indicates that the Xircom product has been tested and found to be compliant with the appropriate regulations as listed in the Declaration of Conformity above, and therefore can be used in any of the countries of the EU.

NOTE: These regulations do not affect GlobalACCESS features of the Xircom modem, including use on networks of countries outside the European Union.

#### Compliance Notice

The equipment has been approved in accordance with Council Decision 1999/5/EC on radio equipment and telecommunications terminal equipment and the mutual recognition of their conformity. This device is telecommunications terminal equipment intended to be connected directly to the public telecommunications network (PSTN). However, due to differences between the individual PSTNs provided in different countries, the approval does not, of itself, give an unconditional assurance of successful operation on every PSTN network termination point. In the event of problems, contact your equipment supplier in the first instance.

#### Network Compatibility Declaration

The manufacturer: Xircom Inc, 2300 Corporate Center Drive Thousand Oaks, California 91320 USA, declares its awareness of the Advisory Notes contained in ETSI Guides EG 201 120 and EG 201 121, including any amendments thereto, and indicates below the networks with which the products are designed to work and any notified networks with which there may be interworking difficulties.

These products are designed to work on PSTNs in the following countries: Austria, Belgium, Denmark, Finland, France, Germany, Greece, Iceland, Ireland, Italy, Luxembourg, Norway, Portugal, Spain, Sweden, Switzerland, The Netherlands, United Kingdom. Use the CountrySelect utility supplied with the product to configure your modem for these countries.

#### Declaration of Conformity (Model CABLE-ETH212)

Xircom, Inc. declares that the equipment described in this document is in conformance with the requirements of the European Council Directive listed below:

73/23/EEC Low Voltage Directive with Amendment 93/68/EEC
89/336/EEC EMC Directive with Amendments 92/31/EEC and 93/68/EEC

This declaration is based upon compliance of the product to the following standards:

EN 55022 Class B (CISPR 22 Class B) RF Emissions Control
EN 50082-1 (IEC 801-2, 3, 4) Immunity to Electromagnetic Disturbance
EN 60950 2nd Edition (A1 - A4) Safety of Information Technology Equipment, Including Electrical

Product Description: Xircom CreditCard Ethernet 10/100+Modem 56 10Base-2 Ethernet Cable, Model CABLE-ETH212

R.W. Bass,
Vice President, Operations
Xircom, Inc.
2300 Corporate Center Drive
Thousand Oaks, California 91320 U.S.A.

## Japan Regulatory Notices

Caution: The modem should be set to Japan mode (the default setting for units sold in Japan) when the equipment is used in Japan.

## New Zealand Telepermit Compliance Notes

General

The grant of a Telepermit for any item of terminal equipment indicates only that Telecom has accepted that the item complies with minimum conditions for connection to its network. It indicates no endorsement of the product by Telecom, nor does it provide any sort of warranty. Above all, it provides no assurance that any item will work correctly in all respects with another item of Telepermitted equipment of a different make or model, nor does it imply that any product is compatible with all of Telecom's network services.

Important Notice

Under power failure conditions, this telephone may not operate. Please ensure that a separate telephone, not dependent on local power, is available for emergency use.

Some parameters required for compliance with Telecom's Telepermit requirements are dependent on the equipment (PC) associated with this device. The associated equipment shall be set to operate within the following limits for compliance with Telecom's Specification:-

- There shall be no more than 10 call attempts to the same number within any 30 minute period for any single manual call initiation, and
- The equipment shall go on-hook for a period of not less than 30 seconds between the end of one attempt and the beginning of the next attempt.
- Where automatic calls are made to different numbers, the equipment shall go on-line for a period of not less than 5 seconds between the end of one attempt and the beginning of the next attempt.
- The equipment shall be set to ensure that calls are answered between 3 and 30 seconds of receipt of ringing.

### Safety Notices

This card is intended for use with UL 1950/EN60950/IEC950 (or other NRTL) listed ITE computers that contain operator-accessible PC Card slots.

Table of Contents | Previous Page | Next Page