Before flashing your phone must have SuperCID and SPL v1.01.0109!

1. Unzip wm5xxxxx.bin file from archive to C:\ and rename it to wm5.bin.
2. Disable USB connections in ActiveSync Connection Settings.
3. Turn off the phone and disconnect USB.
4. Press Camera button and holding it insert USB connector (or holding Camera button press Power button for 1-2 seconds)
5. When "Need an UI (0)?" appears on the screen press [0] immediately.
6. You will see tricolor screen, in the blue zone there will be "Typhoon IU" message, if you see "Typhoon XIP" you were late to press [0], start from beginning.
7. Run mtty1.42.exe, press Enter and you will see a prompt.
8. Type "l c:\wm5.bin" without quotes and press Enter.
9. Wait untill the phone flashed and the prompt appeared again, type "ResetDevice", press Enter to restart the phone or just turn the phone off and on.

If you need Java Manager copy target.img.zip to \Windows folder on the phone.


Look for news and updates at http://opencodesolutions.com/~ronswens/