API Guide Home (Online version only) |

# tagIOTANotificationEventType Struct Reference

## Detailed Description

Structure passed to the callbacks registered for incoming IOTA notifications

Definition at line 318 of file HsPhoneIOTATypes.h.

## Data Fields

- UInt16 version
- void * headerP
- UInt8 headerLen
- void * dataP
- UInt8 dataLen
- UInt32 msgID
- UInt32 datetime
- Int32 reserved2
- Int32 reserved3

## Field Documentation

UInt16 version

version number to provide future backwards compatibility

Definition at line 320 of file HsPhoneIOTATypes.h.

void* headerP

pointer to raw header

Definition at line 322 of file HsPhoneIOTATypes.h.

UInt8 headerLen

length of headerP

Definition at line 323 of file HsPhoneIOTATypes.h.

void* dataP

pointer to data body

Definition at line 324 of file HsPhoneIOTATypes.h.

UInt8 dataLen

length of dataP

Definition at line 325 of file HsPhoneIOTATypes.h.

UInt32 msgID

SMS related fields ID into the SMS database to reference this message this ID is not gauranteed to be valid once the notification callback returns. Users should make a copy of the msg if they want to work on it after the callback returns.

Definition at line 328 of file HsPhoneIOTATypes.h.

UInt32 datetime

date/time stamp

Definition at line 335 of file HsPhoneIOTATypes.h.

Int32 reserved2

reserved

Definition at line 336 of file HsPhoneIOTATypes.h.

Int32 reserved3

reserved

Definition at line 337 of file HsPhoneIOTATypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:32 2008 for Palm API Guide