API Guide Home (Online version only) |

# PhnRadioStateType Struct Reference

## Detailed Description

Radio state

Definition at line 86 of file HsPhoneMiscTypes.h.

## Data Fields

- UInt16 version
- UInt32 size
- UInt16 maxConnections
- Boolean alsSupported
- Int16 activeLineNumber

## Field Documentation

UInt16 version

Definition at line 88 of file HsPhoneMiscTypes.h.

UInt32 size

Definition at line 89 of file HsPhoneMiscTypes.h.

UInt16 maxConnections

Definition at line 90 of file HsPhoneMiscTypes.h.

Boolean alsSupported

GSM only feature. if False activeLineNumber should always be 1

Definition at line 91 of file HsPhoneMiscTypes.h.

Int16 activeLineNumber

Definition at line 92 of file HsPhoneMiscTypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:25 2008 for Palm API Guide