API Guide Home (Online version only) |

# UPNotificationEventType Struct Reference

## Detailed Description

Structure passed to the callbacks registered for incoming UP notifications

Definition at line 1327 of file HsPhoneEvent.h.

## Data Fields

- UInt16 version
- void * headerP
- UInt8 headerLen
- char UPData [UPDataSize+1]
- UInt8 _filler100_
- UInt32 msgID
- UInt32 datetime
- Int32 reserved2
- Int32 reserved3

## Field Documentation

UInt16 version

version number to provide future backwards compatibility

Definition at line 1329 of file HsPhoneEvent.h.

void* headerP

pointer to raw header

Definition at line 1331 of file HsPhoneEvent.h.

UInt8 headerLen

length of headerP

Definition at line 1332 of file HsPhoneEvent.h.

char UPData[UPDataSize+1]

Network wakeup fields stores the raw data

Definition at line 1335 of file HsPhoneEvent.h.

UInt8 _filler100_

Definition at line 1336 of file HsPhoneEvent.h.

UInt32 msgID

SMS related fields ID into the SMS database to reference this message this ID is not gauranteed to be valid once the notification callback returns. Users should make a copy of the msg if they want to work on it after the callback returns.

Definition at line 1339 of file HsPhoneEvent.h.

UInt32 datetime

date/time stamp

Definition at line 1346 of file HsPhoneEvent.h.

Int32 reserved2

reserved

Definition at line 1347 of file HsPhoneEvent.h.

Int32 reserved3

reserved

Definition at line 1348 of file HsPhoneEvent.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:32 2008 for Palm API Guide