API Guide Home (Online version only) |

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - p -

- pad : PhnSATEventGetInput , PhnSATEventPlayTone , PhnSATEventRefresh
- padding1 : FrmNavHeaderTag , vpnNotifyVPNLibTag
- padding2 : vpnNotifyVPNLibTag
- padding3 : vpnNotifyVPNLibTag
- pageNum : _HelperServiceMMSObjectType
- param1 : HsSndMidiProgressMsg
- param2 : HsSndMidiProgressMsg
- params : PhnEventType::Data
- parsedType : ParsedInfo
- passwdNeeded : PhnSATEventDataSvc
- password : WUNotificationEventType , PhnEventType::Data
- passwordAccepted : PhnIndicationType
- PDDataInfo : PhnEventType::Data
- pdp_services : PhnPDPWrite , PhnPDPPayload
- pdpAddr : PhnGPRSPDPContextType
- pdpDataCompression : PhnGPRSPDPContextType , NetPrefGPRSQOSType
- pdpHdrCompression : PhnGPRSPDPContextType
- pdpHeaderCompression : NetPrefGPRSQOSType
- pdpType : PhnGPRSPDPContextType
- pdSessionStatus : PhnOneXStatus
- phn_pd_svc_mask : PhnPDDataType
- PhnOnxMipRRQ : PhnEventType::Data
- phoneBookIndex : Address
- phoneEquipmentMode : PhnEventType::Data
- phoneSoundPrefs : SoundPreference::_tonePrefs
- picHeight : PalmVideoAVCCustomGetDecodedFrameType
- picHeightCropped : PalmVideoAVCCustomGetDecodedFrameType
- picWidth : PalmVideoAVCCustomGetDecodedFrameType
- picWidthCropped : PalmVideoAVCCustomGetDecodedFrameType
- pin : PhnPasswordEventType
- pix_place_server : _PhnLibMMSServerInfo
- planarData : PalmVideoAVCCustomGetDecodedFrameType
- planeCount : PalmImagePlanarType
- planeP : PalmImagePlanarType
- planeWidth : PalmImagePlanarType
- playbackCount : tagSndFileStreamData
- playSoundTimes : SoundPreferenceCalendar
- portID : HsSndPortInfo
- position : LocationDataTag
- power : PhnEventType::Data
- powerOnOffContinueCallback : PhnIndicationType
- preambleType : NetServicesProfileV1 , NetServicesProfile
- prefix4DigitCtl : HsDialPrefsUSDialingRulesType
- prefix5DigitCtl : HsDialPrefsUSDialingRulesType
- prefix6DigitCtl : HsDialPrefsUSDialingRulesType
- preSelect : LocsLibSelLocsTag
- presetTime : SoundPreferenceCalendar
- presetTimeUnit : SoundPreferenceCalendar
- prevType : PhnPasswordEventType
- prim_dns_addr : PhnPDPWrite , PhnPDPPayload
- prim_ha_addr : PhnPDPWrite , PhnPDPPayload
- priority : PhnMsgBoxDataType , PhnSMSParams , PhnSATEventDisplayText
- privacy : PhnSMSParams , SoundPreferenceSMS
- profile : PalmAudioAACParamType , PalmVideoMPEG4EncodeParamType , PalmVideoMPEG4DecodeParamType
- profileEntrySize : NetServicesProfileInfo
- profileName : NetServicesProfile , NetServicesProfileV1
- profileRev : NetServicesProfileInfo
- profiles : PhnRingingInfoType
- progress : PhnProgressEventType , PhnEventType::Data
- progress_callback : HsSndBufferData
- progress_userdata : HsSndBufferData
- promptOffset : PhnSATEventSetupCall
- protectedTone : ToneItemType
- protocolErr : BGResult
- protocolErrString : BGResult
- provOffset : PhnSATEventLaunchBrowser
- proxyAddr : _PhnCDMAMediaTVSettings
- proxyPort : _PhnCDMAMediaTVSettings
- ptr : _pluginSendParams
- puk : PhnPasswordEventType
- pwd : PhnMMIEntryType

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:08 2008 for Palm API Guide