API Guide Home (Online version only) |

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - m -

- mainParams : MailAddRecordParamsTypePlus
- majorResult : BGResult
- mapArr : PmSysGadgetBbutResourceType , HsBigButtonReourceType
- matchFound : AddrHsLookupUserDataType , AddrHsLookupUserDataV2Type
- max_message_size : _PhnLibMMSServerInfo
- maxConnections : PhnRadioStateType
- maximumBytes : tagSndFileStreamData
- maximumMilliseconds : tagSndFileStreamData
- maxNameLength : PhnPhoneBookInfoType
- maxNum : NBSNotificationEventType
- maxNumberLength : PhnPhoneBookInfoType
- maxRate : PalmAudioQCELPParamType
- maxRetries : _PhnLibMMSServerInfo
- maxSize : ParsedInfoList , PhnSATEventGetInput
- maxSockets : HS_HTTPLibAppinfo_
- maxValue : LcdOverlayLibSettingTag , CamLibSettingTag
- maxVol : HsSndPortInfo
- mData : AddressAppRecord
- MemoryFile : _PalmPhotoFileLocation
- message : _HelperServiceMMSDetailsType
- messageCount : PhnMsgBoxDataType
- messageTone : SoundPreferenceIM , SoundPreferenceSMS , SoundPreferenceMMS
- mHeader : AddressAppRecord
- mID : AddressAppRecord
- MIMEtype : _pluginExtendedQueryParams , _pluginParams , _pluginQueryParams
- mimeType : _HelperServiceMMSObjectType
- MIMEtype : _pluginSendParams
- minRate : PalmAudioQCELPParamType
- minSize : PhnSATEventGetInput
- minute : Coordinate
- minValue : CamLibSettingTag , LcdOverlayLibSettingTag
- minVol : HsSndPortInfo
- mipSessionFailReason : PhnEventType::Data
- mipSessionType : PhnOneXStatus
- miscData : ParsedInfo
- miscDbgRpt : PhnEventType::Data
- miscUpdate : PhnMiscDbgRptType
- mLocked : AddressAppRecord
- mmiBarring : PhnMMIEntryType , PhnMMIResultType
- mmiCallControl : PhnMMIEntryType
- mmiCallerID : PhnMMIResultType
- mmiCallWaiting : PhnMMIEntryType , PhnMMIResultType
- mmiColp : PhnMMIResultType
- mmiColr : PhnMMIResultType
- mmiForwarding : PhnMMIEntryType , PhnMMIResultType
- mmiIMEI : PhnMMIResultType
- mmiNumberSent : PhnMMIResultType
- mmiPassword : PhnMMIEntryType
- mmiPhoneNumber : PhnMMIEntryType
- mml_server_name : _PhnLibMMSServerInfo
- mms_server_name : _PhnLibMMSServerInfo
- mmsSoundPrefs : SoundPreference::_tonePrefs
- mn_aaa_spi : PhnPDPPayload , PhnPDPWrite
- mn_aaa_ss : PhnPDPWrite , PhnPDPPayload
- mn_aaa_ss_length : PhnPDPPayload , PhnPDPWrite
- mn_ha_spi : PhnPDPWrite , PhnPDPPayload
- mn_ha_ss : PhnPDPWrite , PhnPDPPayload
- mn_ha_ss_length : PhnPDPPayload , PhnPDPWrite
- mode : PhnMMIEntryType , PalmAudioAMRParamType , PhnPhoneEquipmentMode
- modifiers : PhnKeyPressedParams
- month : DSTDataTag
- moreData : _pluginParams , _pluginSendParams , MMProAttachStruct2
- moved : PhnEventType::Data
- moveMessages : PhnIndicationType
- moveRequested : PhnSMSParams
- msec : HS_HTTPLibTime_
- msgAlert : SoundPreferenceSMS , PhnRingingProfileType
- msgBox : PhnEventType::Data
- msgClass : PhnSMSParams
- msgCount : PmBroadcastNewMsgCountNotifyParamType
- msgID : WUNotificationEventType , UPNotificationEventType , tagIOTANotificationEventType , PhnMovedMsgDescType , NBSNotificationEventType
- msgInd : PhnSMSParams
- msgNumber : ParsedInfo
- msgOwner : PhnMovedMsgDescType
- msgType : PhnSMSParams , HsSndMidiProgressMsg
- mSIMMessagesAcknowledge : PhnIndicationType
- multiparty : PhnConnectionType
- mutexSticky : NetPrefFallbackInfoType

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:08 2008 for Palm API Guide