API Guide Home (Online version only) |

# common/system/palmOneChars.h File Reference

Include dependency graph for common/system/palmOneChars.h:

Go to the source code of this file.

## Defines

- #define vchrHard5 0x0214
- #define vchrHard6 0x0215
- #define keyBitHard5 0x2000
- #define vchrRockerSelect vchrRockerCenter

- #define vchrSilkClock (vchrPalmMin + 0)
- #define vchrClock (vchrPalmMin + 1)
- #define vchrPopupBrightness (vchrPalmMin + 2)
- #define vchrNavChange (vchrPalmMin + 3)
- #define vchrCameraShutter (vchrPalmMin + 8)
- #define vchrHardRecord (vchrHard5)

The following group of characters are specific for Tungsten W

- #define vchrDeviceSpecificChar (vchrPalmMin+20)
- #define vchrHard3Down (vchrDeviceSpecificChar + 0)
- #define vchrHard4Down (vchrDeviceSpecificChar + 1)
- #define vchrDeviceIncomingCall (vchrDeviceSpecificChar + 2)
- #define vchrTelDevicePowerOn (vchrDeviceSpecificChar + 3)
- #define vchrMyFavoriteApplication (vchrDeviceSpecificChar + 4)
- #define vchrTelDevicePowerFinished (vchrDeviceSpecificChar + 5)
- #define vchrBacklightToggled (vchrDeviceSpecificChar + 6)
- #define vchrKeyboardSymbol (vchrDeviceSpecificChar + 9)
- #define vchrReplaceLastChar (vchrDeviceSpecificChar + 10)
- #define vchrFunctionFiveWay (vchrDeviceSpecificChar + 11)
- #define vchrEmergencyCall (vchrDeviceSpecificChar + 12)
- #define vchrPowerOnPhone (vchrDeviceSpecificChar + 14)

Character codes for thumb-wheel keys

- #define vchrThumbWheelUp 0x012E
- #define vchrThumbWheelDown 0x012F
- #define vchrThumbWheelPush 0x0130
- #define vchrThumbWheelBack 0x0131

Character codes for rocker keys

- #define vchrRockerUp 0x0132
- #define vchrRockerDown 0x0133
- #define vchrRockerLeft 0x0134
- #define vchrRockerRight 0x0135
- #define vchrRockerCenter 0x0136

## Define Documentation

#define keyBitHard5 0x2000

The keyBit mask used for polling the 5th hard key.

Definition at line 44 of file common/system/palmOneChars.h.

#define vchrBacklightToggled (vchrDeviceSpecificChar + 6)

Tungsten W virtual character. < This character indicates that the backlight has been toggled.

Definition at line 110 of file common/system/palmOneChars.h.

#define vchrCameraShutter (vchrPalmMin + 8)

Camera shutter virtual character. < Generated by the camera shutter button. Currently only available on Zire71.

Definition at line 68 of file common/system/palmOneChars.h.

#define vchrClock (vchrPalmMin + 1)

Clock virtual character. < When handled by the system, it will launch the clock pop-up dialog.

Definition at line 56 of file common/system/palmOneChars.h.

#define vchrDeviceIncomingCall (vchrDeviceSpecificChar + 2)

Tungsten W virtual character. < This character indicates that there is an incoming call.

Definition at line 93 of file common/system/palmOneChars.h.

#define vchrDeviceSpecificChar (vchrPalmMin+20)

Definition at line 83 of file common/system/palmOneChars.h.

#define vchrEmergencyCall (vchrDeviceSpecificChar + 12)

Tungsten W virtual character. < This character indicates that an emergency call is being placed. < This occurs when the 4 hard keys are all pressed at once.

Definition at line 127 of file common/system/palmOneChars.h.

#define vchrFunctionFiveWay (vchrDeviceSpecificChar + 11)

Tungsten W virtual character. < This character indicates that a 5-way event has been triggered.

Definition at line 123 of file common/system/palmOneChars.h.

#define vchrHard3Down (vchrDeviceSpecificChar + 0)

Tungsten W virtual character. < This character indicates that 3rd Hard key is down. Used to check for press and hold event.

Definition at line 85 of file common/system/palmOneChars.h.

#define vchrHard4Down (vchrDeviceSpecificChar + 1)

Tungsten W virtual character. < This character indicates that 4th Hard key is down. Used to check for press and hold event.

Definition at line 89 of file common/system/palmOneChars.h.

#define vchrHard5 0x0214

To match PalmOS 5.1 definition in Chars.h.

Definition at line 36 of file common/system/palmOneChars.h.

#define vchrHard6 0x0215

Definition at line 40 of file common/system/palmOneChars.h.

#define vchrHardRecord (vchrHard5)

Record button virtual character. < On Tungsten T, this button is located below the microphone. On Tungsten W < and Tungsten C, the button is generally placed on the headset.

Definition at line 72 of file common/system/palmOneChars.h.

#define vchrKeyboardSymbol (vchrDeviceSpecificChar + 9)

Tungsten W virtual character. < This character indicates that the space key has been pressed with the function key.

Definition at line 114 of file common/system/palmOneChars.h.

#define vchrMyFavoriteApplication (vchrDeviceSpecificChar + 4)

Tungsten W virtual character. < This character indicates that the Favorite Application button has been pressed. < The button is UP at this point.

Definition at line 101 of file common/system/palmOneChars.h.

#define vchrNavChange (vchrPalmMin + 3)

Five way navigation virtual character. < This character indicates that the five way navigation states have changed.

Definition at line 64 of file common/system/palmOneChars.h.

#define vchrPopupBrightness (vchrPalmMin + 2)

Pop-up brightness virtual character. < When handled by the system, it will launch the brightness pop-up dialog.

Definition at line 60 of file common/system/palmOneChars.h.

#define vchrPowerOnPhone (vchrDeviceSpecificChar + 14)

Tungsten W virtual character. < This character indicates that a request to toggle the phone on or off has been made.

Definition at line 132 of file common/system/palmOneChars.h.

#define vchrReplaceLastChar (vchrDeviceSpecificChar + 10)

Tungsten W virtual character. < This character indicates that a replace last char event has been triggered. < This occurs when an alpha numeric key is pressed and held.

Definition at line 118 of file common/system/palmOneChars.h.

#define vchrRockerCenter 0x0136

5-way rocker center/press

Definition at line 170 of file common/system/palmOneChars.h.

#define vchrRockerDown 0x0133

5-way rocker down

Definition at line 167 of file common/system/palmOneChars.h.

#define vchrRockerLeft 0x0134

5-way rocker left

Definition at line 168 of file common/system/palmOneChars.h.

#define vchrRockerRight 0x0135

5-way rocker right

Definition at line 169 of file common/system/palmOneChars.h.

#define vchrRockerSelect vchrRockerCenter

Definition at line 176 of file common/system/palmOneChars.h.

#define vchrRockerUp 0x0132

5-way rocker up

Definition at line 166 of file common/system/palmOneChars.h.

#define vchrSilkClock (vchrPalmMin + 0)

Silk screen clock button virtual character. < When handled by the system, it will launch the clock pop-up dialog.

Definition at line 52 of file common/system/palmOneChars.h.

#define vchrTelDevicePowerFinished (vchrDeviceSpecificChar + 5)

Tungsten W virtual character. < This character indicates that the backlight has been toggled.

Definition at line 106 of file common/system/palmOneChars.h.

#define vchrTelDevicePowerOn (vchrDeviceSpecificChar + 3)

Tungsten W virtual character. < This character indicates that the phone has been powered on

Definition at line 97 of file common/system/palmOneChars.h.

#define vchrThumbWheelBack 0x0131

optional thumb-wheel cluster back

Definition at line 155 of file common/system/palmOneChars.h.

#define vchrThumbWheelDown 0x012F

optional thumb-wheel down

Definition at line 153 of file common/system/palmOneChars.h.

#define vchrThumbWheelPush 0x0130

optional thumb-wheel press/center

Definition at line 154 of file common/system/palmOneChars.h.

#define vchrThumbWheelUp 0x012E

optional thumb-wheel up

Definition at line 152 of file common/system/palmOneChars.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:07:46 2008 for Palm API Guide