API Guide Home (Online version only) |

# CamLibStreamTag Struct Reference

## Detailed Description

Video stream structure. Used for capturing a video stream.

When used with WaitfForFram, bufP will contain the full frame buffer.

Definition at line 211 of file palmOneCameraCommon.h.

## Data Fields

- void * lock
- void * bufP
- UInt32 size
- UInt32 frameTime
- UInt32 frameNum

## Field Documentation

void* lock

Reserved.

Definition at line 213 of file palmOneCameraCommon.h.

void* bufP

Pointer to base of frame buffer content.

Definition at line 214 of file palmOneCameraCommon.h.

UInt32 size

Size in bytes of frame buffer.

Definition at line 215 of file palmOneCameraCommon.h.

UInt32 frameTime

Time-stamp when frame was captured.

Definition at line 216 of file palmOneCameraCommon.h.

UInt32 frameNum

Number of frames (relative to start) in stream.

Definition at line 217 of file palmOneCameraCommon.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:11 2008 for Palm API Guide