API Guide Home (Online version only) |

# PalmVideoAVCCustomGetInfoType Struct Reference

## Detailed Description

AVC/H264 Custom Control API structure for GetInfo about frame.

Definition at line 608 of file palmOneCodecFormat.h.

## Data Fields

- UInt16 frameWidth
- UInt16 frameHeight
- UInt16 frameWidthCropped
- UInt16 frameHeightCropped
- UInt16 horizontalOffset
- UInt16 verticalOffset
- UInt32 chromaFormat

## Field Documentation

UInt16 frameWidth

width of lum. plane in pixels

Definition at line 609 of file palmOneCodecFormat.h.

UInt16 frameHeight

Ht of lum. plane in pixels

Definition at line 610 of file palmOneCodecFormat.h.

UInt16 frameWidthCropped

Width of cropped lum. plane in pixels

Definition at line 611 of file palmOneCodecFormat.h.

UInt16 frameHeightCropped

height of cropped lum. plane in pixels

Definition at line 612 of file palmOneCodecFormat.h.

UInt16 horizontalOffset

Horizontal offset of cropped lum. plane

Definition at line 613 of file palmOneCodecFormat.h.

UInt16 verticalOffset

Vertical offset of cropped lum. plane

Definition at line 614 of file palmOneCodecFormat.h.

UInt32 chromaFormat

Chroma format, only YUV420 for now

Definition at line 615 of file palmOneCodecFormat.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:17 2008 for Palm API Guide