API Guide Home (Online version only) |

# _PhnLibMMSServerInfo Struct Reference

## Detailed Description

Definition at line 482 of file HsPhoneSMSTypes.h.

## Data Fields

- UInt32 version
- UInt32 max_message_size
- UInt8 mms_server_name [kMMSStringMaxLen+1]
- UInt8 mml_server_name [kMMSStringMaxLen+1]
- UInt8 pix_place_server [kMMSPixPlaceMaxLen+1]
- UInt8 user_agent [kMMSStringMaxLen+1]
- UInt8 maxRetries
- UInt8 timeout
- Boolean deliveryAck

## Field Documentation

UInt32 version

must be set to PhnLibMMSServerInfoVersion

Definition at line 484 of file HsPhoneSMSTypes.h.

UInt32 max_message_size

max message size kB

Definition at line 485 of file HsPhoneSMSTypes.h.

UInt8 mms_server_name[kMMSStringMaxLen+1]

MMS server [NULL terminated string]

Definition at line 486 of file HsPhoneSMSTypes.h.

UInt8 mml_server_name[kMMSStringMaxLen+1]

MML server [NULL terminated string]

Definition at line 487 of file HsPhoneSMSTypes.h.

UInt8 pix_place_server[kMMSPixPlaceMaxLen+1]

MMS Pix place address [NULL terminated string]

Definition at line 488 of file HsPhoneSMSTypes.h.

UInt8 user_agent[kMMSStringMaxLen+1]

user agent string [NULL terminated string]

Definition at line 489 of file HsPhoneSMSTypes.h.

UInt8 maxRetries

number of retry attempts

Definition at line 490 of file HsPhoneSMSTypes.h.

UInt8 timeout

MMSC timeout

Definition at line 491 of file HsPhoneSMSTypes.h.

Boolean deliveryAck

delivery ack setting

Definition at line 492 of file HsPhoneSMSTypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:09 2008 for Palm API Guide