API Guide Home (Online version only) |

# PalmVideoAVCCustomGetDecodedFrameType Struct Reference

Collaboration diagram for PalmVideoAVCCustomGetDecodedFrameType:

[legend]

## Detailed Description

AVC/H264 Custom Control API structure for getting a decoded frame.

Definition at line 621 of file palmOneCodecFormat.h.

## Data Fields

- PalmImagePlanarType planarData
- Int32 framesReady
- UInt16 picWidth
- UInt16 picWidthCropped
- UInt16 picHeight
- UInt16 picHeightCropped
- UInt16 stride
- UInt32 compositionTimestamp
- double compositionTime

## Field Documentation

PalmImagePlanarType planarData

Definition at line 622 of file palmOneCodecFormat.h.

Int32 framesReady

Definition at line 623 of file palmOneCodecFormat.h.

UInt16 picWidth

width of lum. plane in pixels

Definition at line 624 of file palmOneCodecFormat.h.

UInt16 picWidthCropped

Width of cropped lum. plane in pixels

Definition at line 625 of file palmOneCodecFormat.h.

UInt16 picHeight

Ht of lum. plane in pixels

Definition at line 626 of file palmOneCodecFormat.h.

UInt16 picHeightCropped

height of cropped lum. plane in pixels

Definition at line 627 of file palmOneCodecFormat.h.

UInt16 stride

offset from start of one line of from to start of next

Definition at line 628 of file palmOneCodecFormat.h.

UInt32 compositionTimestamp

timestamp moment in time decoded data to be played back

Definition at line 629 of file palmOneCodecFormat.h.

double compositionTime

time describing moment in time decoded data to be played back

Definition at line 630 of file palmOneCodecFormat.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:17 2008 for Palm API Guide