API Guide Home (Online version only) |

# PhnOperatorType Struct Reference

## Detailed Description

Definition at line 146 of file HsPhoneNetworkTypes.h.

## Data Fields

- PhnOperatorStatus status
- PhnOperatorID id
- char longname [MAX_LONGOPERATORNAME_LENGTH+1]
- char shortname [MAX_SHORTOPERATORNAME_LENGTH+1]
- Boolean isRoaming

## Field Documentation

PhnOperatorStatus status

Definition at line 148 of file HsPhoneNetworkTypes.h.

PhnOperatorID id

Not really used since CDMA just allows one service provider

Definition at line 149 of file HsPhoneNetworkTypes.h.

char longname[MAX_LONGOPERATORNAME_LENGTH+1]

name + terminating NULL char

Definition at line 150 of file HsPhoneNetworkTypes.h.

char shortname[MAX_SHORTOPERATORNAME_LENGTH+1]

name + terminating NULL char

Definition at line 151 of file HsPhoneNetworkTypes.h.

Boolean isRoaming

in sync with the current roaming status

Definition at line 152 of file HsPhoneNetworkTypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:23 2008 for Palm API Guide