API Guide Home (Online version only) |

# NetPrefLibFieldInfoTable.h File Reference

## Detailed Description

This header file contains record field information for NetPref settings.

Version:
  1.0

Date:
  01/11/2002

Definition in file NetPrefLibFieldInfoTable.h.

Go to the source code of this file.

## Functions

- NetPrefRecFieldInfoPreamble () NetPrefRecFieldInfoFIRST(netPrefRecFieldUnknown
- NetPrefRecFieldInfoGrpStart (netPrefRecFieldExtendedSTART, 1) NetPrefRecFieldInfoExtended(netPrefRecFieldUInt32Reserved1
- NetPrefRecFieldInfoExtended (netPrefRecFieldSvcMediumAlias, 3, netPrefFieldTypeUInt16, 0, 0,< 3:medium >, 10) NetPrefRecFieldInfoExtended(netPrefRecFieldBinding
- < 4:bind > NetPrefRecFieldInfoExtended (netPrefRecFieldBindingIndex, 5, netPrefFieldTypeUInt16, 0, 0,< 5:bindidx >, 11) NetPrefRecFieldInfoExtended(netPrefRecFieldSvcGatewayType
- < 4:bind >< 6:gtwytyp > NetPrefRecFieldInfoExtended (netPrefRecFieldFallbackID, 7, netPrefFieldTypeUInt32, 0, 0,< 7:fback >, 9) NetPrefRecFieldInfoExtended(netPrefRecFieldAPN
- < 4:bind >< 6:gtwytyp ><
  8:apn > NetPrefRecFieldInfoExtended (netPrefRecFieldMdmInitStr, 9, netPrefFieldTypeStr, 0, 0,< 9:mdmins >, 10) NetPrefRecFieldInfoExtended(netPrefRecFieldIsMobileIP
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip > NetPrefRecFieldInfoExtended (netPrefRecFieldHAAddrPrimary, 11, netPrefFieldTypeUInt32, 0, 0,< 11:ha1 >, 8) NetPrefRecFieldInfoExtended(netPrefRecFieldHAAddrSecondary
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 > NetPrefRecFieldInfoExtended (netPrefRecFieldMnHaSS, 13, netPrefFieldTypeBin, 0, 0,< 13:hapsw >, 10) NetPrefRecFieldInfoExtended(netPrefRecField1xRTTTunneling
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl > NetPrefRecFieldInfoExtended (netPrefRecFieldMnHaSpi, 15, netPrefFieldTypeUInt32, 0, 0,< 15:haspi >, 10) NetPrefRecFieldInfoExtended(netPrefRecFieldMnAaaSpi
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp > NetPrefRecFieldInfoExtended (netPrefRecFieldDialStr, 17, netPrefFieldTypeStr, 0, 0,< 17:dials >, 10) NetPrefRecFieldInfoExtended(netPrefRecFieldRecProtection
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect > NetPrefRecFieldInfoExtended (netPrefRecFieldPDPIndex, 19, netPrefFieldTypeUInt32, 0, 0,< 19:pdpidx >, 11) NetPrefRecFieldInfoExtended(netPrefRecFieldPDPChangeID
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg > NetPrefRecFieldInfoExtended (netPrefRecFieldCreatorID, 21, netPrefFieldTypeUInt32, 0, 0,< 21:crid >, 9) NetPrefRecFieldInfoExtended(netPrefRecFieldCreatorData
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata > NetPrefRecFieldInfoExtended (netPrefRecFieldGPRSQOS, 23, netPrefFieldTypeBin, 0, 0,< 23:gprsqos >, 12) NetPrefRecFieldInfoExtended(netPrefRecField1xRTTQOS
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos > NetPrefRecFieldInfoExtended (netPrefRecFieldBinReserved1, 25, netPrefFieldTypeBin, 0, 0,< 25:binrsvd1 >, 13) NetPrefRecFieldInfoExtended(netPrefRecFieldNaiStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai > NetPrefRecFieldInfoExtended (netPrefRecFieldMnAaaSs, 27, netPrefFieldTypeBin, 0, 0,< 27:mnaaass >, 12) NetPrefRecFieldInfoExtended(netPrefRecFieldVJCompSlots
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots > NetPrefRecFieldInfoExtended (netPrefRecFieldFallbackInfo, 29, netPrefFieldTypeBin, 0, 0,< 29:fbkinfo >, 12) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyPrimaryHttpServer
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyPrimaryHttpPort, 31, netPrefFieldTypeUInt32, 0, 0,< 31:HttpPt >, 11) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyPrimaryHttpsServer
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyPrimaryHttpsPort, 33, netPrefFieldTypeUInt32, 0, 0,< 33:HttpsPt >, 12) NetPrefRecFieldInfoExtended(netPrefRecFieldProxySecondaryHttpServer
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 > NetPrefRecFieldInfoExtended (netPrefRecFieldProxySecondaryHttpPort, 35, netPrefFieldTypeUInt32, 0, 0,< 35:HttpP2 >, 11) NetPrefRecFieldInfoExtended(netPrefRecFieldProxySecondaryHttpsServer
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 > NetPrefRecFieldInfoExtended (netPrefRecFieldProxySecondaryHttpsPort, 37, netPrefFieldTypeUInt32, 0, 0,< 37:HttpsP2 >, 12) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyExcludedHostsString
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyUsernameNew, 39, netPrefFieldTypeStr, 0, 0,< 39:User2 >, 10) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyPasswordNew
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyReqCustomUaProf, 41, netPrefFieldTypeUInt8, 0, 0,< 41:CustUa >, 11) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyDefaultHomePage
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyUaProfHostedOnOwnServers, 43, netPrefFieldTypeUInt8, 0, 0,< 43:UaOwnSv >, 12) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyUrlOfUaProfFile
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyEncryptedMsisdn, 45, netPrefFieldTypeUInt8, 0, 0,< 45:EncrMSI >, 12) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyMsisdnFormat
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyMsisdnStaticString, 47, netPrefFieldTypeStr, 0, 0,< 47:MSIStr >, 11) NetPrefRecFieldInfoExtended(netPrefRecFieldProxyReqStaticHeaderString
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat > NetPrefRecFieldInfoExtended (netPrefRecFieldProxyStaticHeaderString, 49, netPrefFieldTypeStr, 0, 0,< 49:StatHStr >, 13) NetPrefRecFieldInfoExtended(netPrefRecFieldDomain01
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 > NetPrefRecFieldInfoExtended (netPrefRecFieldDomain02, 51, netPrefFieldTypeStr, 0, 0,< 51:domain02 >, 13) NetPrefRecFieldInfoExtended(netPrefRecFieldDomain03
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 > NetPrefRecFieldInfoExtended (netPrefRecFieldDomain04, 53, netPrefFieldTypeStr, 0, 0,< 53:domain04 >, 13) NetPrefRecFieldInfoExtended(netPrefRecFieldDomain05
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 > NetPrefRecFieldInfoExtended (netPrefRecFieldDomain06, 55, netPrefFieldTypeStr, 0, 0,< 55:domain06 >, 13) NetPrefRecFieldInfoExtended(netPrefRecFieldDomain07
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 > NetPrefRecFieldInfoExtended (netPrefRecFieldDomain08, 57, netPrefFieldTypeStr, 0, 0,< 57:domain08 >, 13) NetPrefRecFieldInfoExtended(netPrefRecFieldDomain09
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 > NetPrefRecFieldInfoExtended (netPrefRecFieldDomain10, 59, netPrefFieldTypeStr, 0, 0,< 59:domain10 >, 13) NetPrefRecFieldInfoGrpEnd(netPrefRecFieldExtendedEND) NetPrefRecFieldInfoGrpStart(netPrefRecFieldLegacySTART
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 > NetPrefRecFieldInfoLegacy (netPrefRecFieldInterfaceID, 1001, netPrefFieldTypeUInt32, 0, 0,< 1001:ifid >, 11) NetPrefRecFieldInfoLegacy(netPrefRecFieldIPAddrIsDynamic
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip > NetPrefRecFieldInfoLegacy (netPrefRecFieldIPAddr, 1003, netPrefFieldTypeUInt32, 0, 0,< 1003:ipaddr >, 13) NetPrefRecFieldInfoLegacy(netPrefRecFieldDNSAddrIsDynamic
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns > NetPrefRecFieldInfoLegacy (netPrefRecFieldDNSAddrPrimary, 1005, netPrefFieldTypeUInt32, 0, 0,< 1005:pridns >, 13) NetPrefRecFieldInfoLegacy(netPrefRecFieldDNSAddrSecondary
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns > NetPrefRecFieldInfoLegacy (netPrefRecFieldCloseWaitTime, 1007, netPrefFieldTypeUInt32, 0, 0,< 1007:cwtm >, 11) NetPrefRecFieldInfoLegacy(netPrefRecFieldInactivityTimer
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm > NetPrefRecFieldInfoLegacy (netPrefRecFieldEstablishmentTimeout, 1009, netPrefFieldTypeUInt16, 0, 0,< 1009:estbtm >, 13) NetPrefRecFieldInfoLegacy(netPrefRecFieldVJCompEnable
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr > NetPrefRecFieldInfoLegacy (netPrefRecFieldUseModem, 1011, netPrefFieldTypeUInt8, 0, 0,< 1011:usemdm >, 13) NetPrefRecFieldInfoLegacy(netPrefRecFieldServiceName
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam > NetPrefRecFieldInfoLegacy (netPrefRecFieldUsername, 1013, netPrefFieldTypeStr, 0, 0,< 1013:usrnam >, 13) NetPrefRecFieldInfoLegacy(netPrefRecFieldPassword
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw > NetPrefRecFieldInfoLegacy (netPrefRecFieldDomainName, 1015, netPrefFieldTypeStr, 0, 0,< 1015:domain >, 13) NetPrefRecFieldInfoLegacy(netPrefRecFieldHostTable
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab > NetPrefRecFieldInfoLegacy (netPrefRecFieldSMTPHost, 1017, netPrefFieldTypeStr, 0, 0,< 1017:smtphst >, 14) NetPrefRecFieldInfoLegacy(netPrefRecFieldPOPHost
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst > NetPrefRecFieldInfoLegacy (netPrefRecFieldNewsServer, 1019, netPrefFieldTypeStr, 0, 0,< 1019:newssrv >, 14) NetPrefRecFieldInfoLegacy(netPrefRecFieldLoginScript
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script > NetPrefRecFieldInfoLegacy (netPrefRecFieldConnection, 1021, netPrefFieldTypeStr, 0, 0,< 1021:connnam >, 14) NetPrefRecFieldInfoLegacy(netPrefRecFieldDialPrefixEnable
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script >< 1022:enprefx > NetPrefRecFieldInfoLegacy (netPrefRecFieldCallWaitingEnable, 1023, netPrefFieldTypeUInt8, 0, 0,< 1023:encalwt >, 14) NetPrefRecFieldInfoLegacy(netPrefRecFieldCallingCardEnable
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script >< 1022:enprefx >< 1024:encalcd > NetPrefRecFieldInfoLegacy (netPrefRecFieldPulseDialEnable, 1025, netPrefFieldTypeUInt8, 0, 0,< 1025:enpulse >, 14) NetPrefRecFieldInfoLegacy(netPrefRecFieldPhoneNumber
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script >< 1022:enprefx >< 1024:encalcd >< 1026:phone > NetPrefRecFieldInfoLegacy (netPrefRecFieldDialPrefix, 1027, netPrefFieldTypeStr, 0, 0,< 1027:dlprefx >, 14) NetPrefRecFieldInfoLegacy(netPrefRecFieldCallWaitingString

## Variables

- netPrefFieldTypeUInt32
- netPrefFieldTypeUInt16
- < 4:bind > netPrefFieldTypeUInt32
- < 4:bind >< 6:gtwytyp > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip > netPrefFieldTypeUInt32
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 > netPrefFieldTypeUInt16
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl > netPrefFieldTypeUInt32
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp > netPrefFieldTypeUInt32
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect > netPrefFieldTypeBin
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg > netPrefFieldTypeBin
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata > netPrefFieldTypeBin
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns > netPrefFieldTypeUInt32
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns > netPrefFieldTypeUInt16
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst > netPrefFieldTypeZStrList
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script >< 1022:enprefx > netPrefFieldTypeUInt8
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script >< 1022:enprefx >< 1024:encalcd > netPrefFieldTypeStr
- < 4:bind >< 6:gtwytyp ><
  8:apn >< 10:mip >< 12:ha2 >< 14:1xtnl >< 16:aaasp >< 18:protect >< 20:pdpchg >< 22:crdata >< 24:1xrttqos >< 26:nai >< 28:vjslots >< 30:HttpSv >< 32:HttpsSv >< 34:HttpS2 >< 36:HttpsS2 >< 38:ExclHst >< 40:Pass2 >< 42:HomePg >< 44:UrlUa >< 46:MSIfmt >< 48:ReqStat >< 50:domain01 >< 52:domain03 >< 54:domain05 >< 56:domain07 >< 58:domain09 >< 1002:dynip >< 1004:dyndns >< 1006:secdns >< 1008:inactm >< 1010:vjcmpr >< 1012:svcnam >< 1014:usrpsw >< 1016:hosttab >< 1018:pophst >< 1020:script >< 1022:enprefx >< 1024:encalcd >< 1026:phone > netPrefFieldTypeStr

## Function Documentation

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldDomain10 | ,
|  | 59 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 59:domain10 > | ,
|  | 13 |  |
| ) |  |  |

START OF LEGACY FIELDS

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldDomain08 | ,
|  | 57 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 57:domain08 > | ,
|  | 13 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldDomain06 | ,
|  | 55 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 55:domain06 > | ,
|  | 13 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldDomain04 | ,
|  | 53 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 53:domain04 > | ,
|  | 13 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldDomain02 | ,
|  | 51 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 51:domain02 > | ,
|  | 13 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyStaticHeaderString | ,
|  | 49 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 49:StatHStr > | ,
|  | 13 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyMsisdnStaticString | ,
|  | 47 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 47:MSIStr > | ,
|  | 11 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyEncryptedMsisdn | ,
|  | 45 | ,
|  | netPrefFieldTypeUInt8 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 45:EncrMSI > | ,
|  | 12 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyUaProfHostedOnOwnServers | ,
|  | 43 | ,
|  | netPrefFieldTypeUInt8 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 43:UaOwnSv > | ,
|  | 12 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyReqCustomUaProf | ,
|  | 41 | ,
|  | netPrefFieldTypeUInt8 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 41:CustUa > | ,
|  | 11 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyUsernameNew | ,
|  | 39 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 39:User2 > | ,
|  | 10 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxySecondaryHttpsPort | ,
|  | 37 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 37:HttpsP2 > | ,
|  | 12 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxySecondaryHttpPort | ,
|  | 35 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 35:HttpP2 > | ,
|  | 11 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyPrimaryHttpsPort | ,
|  | 33 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 33:HttpsPt > | ,
|  | 12 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldProxyPrimaryHttpPort | ,
|  | 31 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 31:HttpPt > | ,
|  | 11 |  |
| ) |  |  |

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldFallbackInfo | ,
|  | 29 | ,
|  | netPrefFieldTypeBin | ,
|  | 0 | ,
|  | 0 | ,
|  | < 29:fbkinfo > | ,
|  | 12 |  |
| ) |  |  |

<chg 2006-01-18 kos> Feature for Camino|Microwave: Per-APN proxy settings (9.1.2) deprecates the old "browser settings" normally stored in the carrier record

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldMnAaaSs | ,
|  | 27 | ,
|  | netPrefFieldTypeBin | ,
|  | 0 | ,
|  | 0 | ,
|  | < 27:mnaaass > | ,
|  | 12 |  |
| ) |  |  |

UInt8, -- initial number of VJ Compression slots if VJ compression is enabled; used to set NetLib's netIFSettingVJCompSlots setting (see also netPrefRecFieldVJCompEnable).

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldBinReserved1 | ,
|  | 25 | ,
|  | netPrefFieldTypeBin | ,
|  | 0 | ,
|  | 0 | ,
|  | < 25:binrsvd1 > | ,
|  | 13 |  |
| ) |  |  |

char*, 1xRTT NAI field (CDMA/1xRTT)

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldGPRSQOS | ,
|  | 23 | ,
|  | netPrefFieldTypeBin | ,
|  | 0 | ,
|  | 0 | ,
|  | < 23:gprsqos > | ,
|  | 12 |  |
| ) |  |  |

NetPref1xRTTQOSType -- 1xRTT Quality of Service parameters. UNDEFINED/RESERVED BY HANDSPRING

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldCreatorID | ,
|  | 21 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 21:crid > | ,
|  | 9 |  |
| ) |  |  |

void*, Creator-specific binary data field; applications that set the netPrefRecFieldCreatorID field may also save application-specific data inside this field. see also netPrefRecFieldCreatorID.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldPDPIndex | ,
|  | 19 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 19:pdpidx > | ,
|  | 11 |  |
| ) |  |  |

void*, -- Unique ID/Change number of the PDP slot in radio's NV table. Presently used for CDMA/1xRTT IOTA-bound profiles. For internal use only!

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldDialStr | ,
|  | 17 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 17:dials > | ,
|  | 10 |  |
| ) |  |  |

UInt32, NetPrefRecProtectionType -- record protection options

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldMnHaSpi | ,
|  | 15 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 15:haspi > | ,
|  | 10 |  |
| ) |  |  |

UInt32, SPI for MN-AAA authentication, if Mobile-IP (CDMA/1xRTT)

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldMnHaSS | ,
|  | 13 | ,
|  | netPrefFieldTypeBin | ,
|  | 0 | ,
|  | 0 | ,
|  | < 13:hapsw > | ,
|  | 10 |  |
| ) |  |  |

UInt16, NetPref1xRTTTunnelingEnum; Tunneling, if Mobile-IP (CDMA/1xRTT)

<4:bind><6:gtwytyp><8:apn><10:mip> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldHAAddrPrimary | ,
|  | 11 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 11:ha1 > | ,
|  | 8 |  |
| ) |  |  |

UInt32, Secondary HA Address, if Mobile-IP (CDMA/1xRTT)

<4:bind><6:gtwytyp><8:apn> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldMdmInitStr | ,
|  | 9 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 9:mdmins > | ,
|  | 10 |  |
| ) |  |  |

UInt8; Is Mobile-IP; non-zero=true (0x01), zero=false (CDMA/1xRTT only)

<4:bind><6:gtwytyp> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldFallbackID | ,
|  | 7 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 7:fback > | ,
|  | 9 |  |
| ) |  |  |

char*, APN name for GPRS services

<4:bind> NetPrefRecFieldInfoExtended | ( | netPrefRecFieldBindingIndex | ,
|  | 5 | ,
|  | netPrefFieldTypeUInt16 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 5:bindidx > | ,
|  | 11 |  |
| ) |  |  |

UInt32, NetPrefSvcGatewayType - Internet, WAP, etc. (1 or more netPrefSvcGateway... constants bitwise-or'ed together; if the field is absent, Internet is implied.

NetPrefRecFieldInfoExtended | ( | netPrefRecFieldSvcMediumAlias | ,
|  | 3 | ,
|  | netPrefFieldTypeUInt16 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 3:medium > | ,
|  | 10 |  |
| ) |  |  |

UInt16, NetPrefSvcBindingEnum; not needed in most cases. Handspring internal use only!

NetPrefRecFieldInfoGrpStart | ( | netPrefRecFieldExtendedSTART | ,
|  | 1 |  |
| ) |  |  |

UInt32; reserved for internal Handspring use only

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script><1022:enprefx><1024:encalcd><1026:phone> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldDialPrefix | ,
|  | 1027 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1027:dlprefx > | ,
|  | 14 |  |
| ) |  |  |

char*; corresponds to the Call Waiting setting in the Phone Setup dialog.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script><1022:enprefx><1024:encalcd> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldPulseDialEnable | ,
|  | 1025 | ,
|  | netPrefFieldTypeUInt8 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1025:enpulse > | ,
|  | 14 |  |
| ) |  |  |

char*; phone number; corresponds to the Phone # field in the Phone Setup dialog.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script><1022:enprefx> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldCallWaitingEnable | ,
|  | 1023 | ,
|  | netPrefFieldTypeUInt8 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1023:encalwt > | ,
|  | 14 |  |
| ) |  |  |

UInt8; non-zero=true, zero=false; corresponds to the Calling Card setting in the Phone Setup dialog.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldConnection | ,
|  | 1021 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1021:connnam > | ,
|  | 14 |  |
| ) |  |  |

UInt8; non-zero=true, zero=false; corresponds to the dial prefix setting in the Phone Setup dialog.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldNewsServer | ,
|  | 1019 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1019:newssrv > | ,
|  | 14 |  |
| ) |  |  |

char*; loginScript; scripts contain null terminated strings and end with a double null; ***an empty script is represented with a single null (not double null); used to set NetLib's netIFSettingLoginScript setting for dial-up type of profiles. Refer to Palm for login-script format.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldSMTPHost | ,
|  | 1017 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1017:smtphst > | ,
|  | 14 |  |
| ) |  |  |

char*; presently not used.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldDomainName | ,
|  | 1015 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1015:domain > | ,
|  | 13 |  |
| ) |  |  |

char*; callback username, password; used to set NetLib's netSettingHostTbl setting; might not be used by NetLib.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldUsername | ,
|  | 1013 | ,
|  | netPrefFieldTypeStr | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1013:usrnam > | ,
|  | 13 |  |
| ) |  |  |

char*; password

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldUseModem | ,
|  | 1011 | ,
|  | netPrefFieldTypeUInt8 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1011:usemdm > | ,
|  | 13 |  |
| ) |  |  |

char*; service name

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldEstablishmentTimeout | ,
|  | 1009 | ,
|  | netPrefFieldTypeUInt16 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1009:estbtm > | ,
|  | 13 |  |
| ) |  |  |

UInt8; non-zero=true, zero=false; used to set NetLib's netIFSettingVJCompEnable setting. See also netPrefRecFieldVJCompSlots.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldCloseWaitTime | ,
|  | 1007 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1007:cwtm > | ,
|  | 11 |  |
| ) |  |  |

UInt16; expressed in seconds; see NetPrefNetIdleTimeoutEnum for special values; used to set NetLib interface's netIFSettingInactivityTimeout setting (also known as "idle timeout"). IMPORTANT: This setting is enforced beginning with Palm OS 5.0 and must be used to configure the idle timeout of the TCP/IP stack.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldDNSAddrPrimary | ,
|  | 1005 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1005:pridns > | ,
|  | 13 |  |
| ) |  |  |

UInt32; secondary DNS address if not dynamic

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldIPAddr | ,
|  | 1003 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1003:ipaddr > | ,
|  | 13 |  |
| ) |  |  |

UInt8; non-zero=true (0x01), zero=false

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09> NetPrefRecFieldInfoLegacy | ( | netPrefRecFieldInterfaceID | ,
|  | 1001 | ,
|  | netPrefFieldTypeUInt32 | ,
|  | 0 | ,
|  | 0 | ,
|  | < 1001:ifid > | ,
|  | 11 |  |
| ) |  |  |

UInt8; non-zero=true, zero=false

NetPrefRecFieldInfoPreamble | ( |  | ) |

reserve 0

## Variable Documentation

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata> netPrefFieldTypeBin

Definition at line 214 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg> netPrefFieldTypeBin

Definition at line 204 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect> netPrefFieldTypeBin

Definition at line 187 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script><1022:enprefx><1024:encalcd><1026:phone> netPrefFieldTypeStr

Definition at line 538 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script><1022:enprefx><1024:encalcd> netPrefFieldTypeStr

Definition at line 530 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab> netPrefFieldTypeStr

Definition at line 483 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw> netPrefFieldTypeStr

Definition at line 472 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam> netPrefFieldTypeStr

Definition at line 460 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr> netPrefFieldTypeStr

Definition at line 449 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07> netPrefFieldTypeStr

Definition at line 364 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05> netPrefFieldTypeStr

Definition at line 354 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03> netPrefFieldTypeStr

Definition at line 344 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01> netPrefFieldTypeStr

Definition at line 334 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat> netPrefFieldTypeStr

Definition at line 324 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa> netPrefFieldTypeStr

Definition at line 310 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg> netPrefFieldTypeStr

Definition at line 304 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2> netPrefFieldTypeStr

Definition at line 298 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst> netPrefFieldTypeStr

Definition at line 292 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2> netPrefFieldTypeStr

Definition at line 286 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2> netPrefFieldTypeStr

Definition at line 280 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv> netPrefFieldTypeStr

Definition at line 274 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv> netPrefFieldTypeStr

Definition at line 268 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots> netPrefFieldTypeStr

Definition at line 262 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos> netPrefFieldTypeStr

Definition at line 222 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp> netPrefFieldTypeStr

Definition at line 127 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns> netPrefFieldTypeUInt16

Definition at line 429 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2> netPrefFieldTypeUInt16

Definition at line 155 of file NetPrefLibFieldInfoTable.h.

netPrefFieldTypeUInt16

Definition at line 101 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns> netPrefFieldTypeUInt32

Definition at line 410 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp> netPrefFieldTypeUInt32

Definition at line 175 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl> netPrefFieldTypeUInt32

Definition at line 163 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip> netPrefFieldTypeUInt32

Definition at line 147 of file NetPrefLibFieldInfoTable.h.

<4:bind> netPrefFieldTypeUInt32

Definition at line 116 of file NetPrefLibFieldInfoTable.h.

netPrefFieldTypeUInt32

Definition at line 87 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script><1022:enprefx> netPrefFieldTypeUInt8

Definition at line 522 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst><1020:script> netPrefFieldTypeUInt8

Definition at line 510 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm> netPrefFieldTypeUInt8

Definition at line 441 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip> netPrefFieldTypeUInt8

Definition at line 402 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09> netPrefFieldTypeUInt8

Definition at line 394 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt> netPrefFieldTypeUInt8

Definition at line 316 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai> netPrefFieldTypeUInt8

Definition at line 248 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn> netPrefFieldTypeUInt8

Definition at line 139 of file NetPrefLibFieldInfoTable.h.

<4:bind><6:gtwytyp><8:apn><10:mip><12:ha2><14:1xtnl><16:aaasp><18:protect><20:pdpchg><22:crdata><24:1xrttqos><26:nai><28:vjslots><30:HttpSv><32:HttpsSv><34:HttpS2><36:HttpsS2><38:ExclHst><40:Pass2><42:HomePg><44:UrlUa><46:MSIfmt><48:ReqStat><50:domain01><52:domain03><54:domain05><56:domain07><58:domain09><1002:dynip><1004:dyndns><1006:secdns><1008:inactm><1010:vjcmpr><1012:svcnam><1014:usrpsw><1016:hosttab><1018:pophst> netPrefFieldTypeZStrList

Definition at line 496 of file NetPrefLibFieldInfoTable.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:07:39 2008 for Palm API Guide