API Guide Home (Online version only) |

# PhnDataSessionStateType Struct Reference

## Detailed Description

Definition at line 628 of file HsPhoneNetworkTypes.h.

## Data Fields

- UInt32 version
- PhnDataServiceType availableService
- PhnDataServiceType sessionType
- PhnPacketDataSessionType sessionStatus
- PhnPacketDataEndStatusType disconnectStatus

## Field Documentation

UInt32 version

(1.0) should be set to the structure version that you are requesting

Definition at line 630 of file HsPhoneNetworkTypes.h.

PhnDataServiceType availableService

(1.0) data connection type available

Definition at line 631 of file HsPhoneNetworkTypes.h.

PhnDataServiceType sessionType

(1.0) data connection type (valid only if status is Active or Dormant)

Definition at line 632 of file HsPhoneNetworkTypes.h.

PhnPacketDataSessionType sessionStatus

(1.0) data connection status

Definition at line 633 of file HsPhoneNetworkTypes.h.

PhnPacketDataEndStatusType disconnectStatus

(1.0) data connection end status (only useful after a data call has been terminated)

Definition at line 634 of file HsPhoneNetworkTypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:19 2008 for Palm API Guide