API Guide Home (Online version only) |

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - a -

- aboveObjectID : FrmNavOrderEntryTag
- account : SysVPPILaunchCmdEditAccountType , SysVPPILaunchCmdDeleteAccountType , SysVPPILaunchCmdSetCurrentAccountType
- accountID : VPNAccountType
- accountName : VPNAccountType
- accounts : SysVPPILaunchCmdGetAccountsType
- acknowledge : PhnEventType
- action : PhnMMIEntryType
- Action : P1clRecordDetails
- action : PhnSATEventLaunchBrowser
- actionCode : PalmAudioPlaybackNotifyEventTypeTag , PhnMMIEntryType
- activate : PhnSMSParams
- active_idx : PhnPDPList
- active_idx_set : PhnPDPList
- activeCall : AddrPhonebookAppParamsType
- activeLine : PhnLineStateType
- activeLineNumber : PhnRadioStateType
- add1BeforeAreaCode : HsDialPrefsUSDialingRulesType
- addr : HS_HTTPLibIPAddr_ , PhnIOTAPhnNAISIPEdgeProxyType , PhnIOTAPhnProxyAddrWdpType
- address : AddressType , PhnConnectionType
- addressSize : AddressType
- alarmPreset : SoundPreferenceCalendar
- alarmTone : SoundPreferenceCalendar
- albumID : _PalmPhotoSelectionParam
- alertTone : SoundPreferenceEmail
- algorithm : PalmVideoMPEG4EncodeParamType , NetPrefFallbackInfoType
- alphaIdOffset : PhnSATEventSendDTMF , PhnSATEventLaunchBrowser , PhnSATEventIdleModeText , PhnSATEventRunAT , PhnSATEventDataSvc
- alsSupported : PhnRadioStateType
- altitude : PhnPDDataType
- amplitude : HsSndBufferData
- apiCreator : SndCodecCustomControlType
- apiSelector : SndCodecCustomControlType
- apn : PhnGPRSPDPContextType
- appCreator : HS_HTTPLibAppinfo_
- appId : WAPNotificationEventType
- areaCodeCtl : HsDialPrefsUSDialingRulesType
- ascP : PalmAudioAACDecParamType
- aSize : MMProAttachStruct2 , MMProAttachStruct
- assigned : SysWPPILaunchCmdType
- athenaDeviceCreatorCode : PmConnectorNotifyDataType
- attachData : MailAddRecordAttachment
- attachDBID : MailAddRecordAttachment
- attachDescription : MailAddRecordAttachment
- attachFileName : MailAddRecordAttachment
- attachment : MMProAttachStruct , MMProAttachStruct2
- attachments : MMProLaunchStruct2 , MailAddRecordParamsTypePlus , MMProLaunchStruct
- attachName : MMProAttachStruct2 , MMProAttachStruct
- attachSize : MailAddRecordAttachment
- attachType : MailAddRecordAttachment
- audioAlertEnable : PhnSMSPrefType
- authentication : NetServicesProfile , NetServicesProfileV1
- authenticationMethodID : SysWPPILaunchCmdGetDescriptionType , WiFiAuthenticationMethodType , SysWPPILaunchCmdType
- authenticationMethodName : WiFiAuthenticationMethodType
- authenticationMethods : SysWPPILaunchCmdGetAuthenticationMethodsType
- auto4DigitPrefix : HsDialPrefsUSDialingRulesType
- auto5DigitPrefix : HsDialPrefsUSDialingRulesType
- auto6DigitPrefix : HsDialPrefsUSDialingRulesType
- autoAreaCode : HsDialPrefsUSDialingRulesType
- autoOffWhenClosed : PowerPanelAppPrefs
- autoOnWhenOpened : PowerPanelAppPrefs
- availableService : PhnDataSessionStateType
- avgBytesPerSec : PalmAudioMP2ParamType

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:08 2008 for Palm API Guide