API Guide Home (Online version only) |

# PhnIOTAReportType Struct Reference

## Detailed Description

Definition at line 59 of file HsPhoneIOTATypes.h.

## Data Fields

- PhnIOTAStatus status
- UInt8 namInUse
- PHNErrorCode error

## Field Documentation

PhnIOTAStatus status

the status that the modem changes into

Definition at line 61 of file HsPhoneIOTATypes.h.

UInt8 namInUse

namInUse4IOTA currently

Definition at line 62 of file HsPhoneIOTATypes.h.

PHNErrorCode error

== 0 normally, only != 0 for phnIOTAEnd and phnIOTACommit if Commit failed.

Definition at line 63 of file HsPhoneIOTATypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:22 2008 for Palm API Guide