API Guide Home (Online version only) |

# Net80211DeviceInfo Struct Reference

## Detailed Description

Device information concerning Hardware and Firmware information for the "adapter".

Revision information and product name data is returned.

Definition at line 85 of file PalmNetServices.h.

## Data Fields

- UInt32 validFlags
- UInt32 fwRev [2]
- Int32 serialNumberSize
- UInt8 serialNumber [kNetSerialNumberLength]
- Char driverDate [kNetDriverDateLength]
- Char fwName [kNetFWNameLength]

## Field Documentation

UInt32 validFlags

Bit flag indicating validity of fields.

Definition at line 87 of file PalmNetServices.h.

UInt32 fwRev[2]

Firmware revision. STA/BB (32 bits), PRI/MAC (32 bits). Valid is (validFlags & 1) == 1.

Definition at line 88 of file PalmNetServices.h.

Int32 serialNumberSize

Serial number size. Valid is (validFlags & 8) == 1.

Definition at line 89 of file PalmNetServices.h.

UInt8 serialNumber[kNetSerialNumberLength]

Serial number. Valid is (validFlags & 8) == 1.

Definition at line 90 of file PalmNetServices.h.

Char driverDate[kNetDriverDateLength]

Driver date. Valid is (validFlags & 2) == 1.

Definition at line 91 of file PalmNetServices.h.

Char fwName[kNetFWNameLength]

Firmware name. Valid is (validFlags & 4) == 1.

Definition at line 92 of file PalmNetServices.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:14 2008 for Palm API Guide