API Guide Home (Online version only) |

# hsPhoneLocationTypes.h File Reference

## Detailed Description

File contains Phone Location data types.

Definition in file hsPhoneLocationTypes.h.

Include dependency graph for hsPhoneLocationTypes.h:

Go to the source code of this file.

## Typedefs

- typedef UInt8 PhnPDSessionConfigParamType

## Enumerations

- enum _PhnPDSessionConfigParamType {
  PhnPDConfigIPAddr = 1,
  PhnPDConfigPortID,
  PhnPDConfigGPSLock,
  PhnPDConfigPTLMMode
  }

## Typedef Documentation

typedef UInt8 PhnPDSessionConfigParamType

error codes returned by phone library functions

Definition at line 38 of file hsPhoneLocationTypes.h.

## Enumeration Type Documentation

enum _PhnPDSessionConfigParamType

Enumerator:

  PhnPDConfigIPAddr | Binary value of the Position Determination Entity (PDE) IP Address
  PhnPDConfigPortID | Binary value of the PDE Port ID.
  PhnPDConfigGPSLock | Level of GPS lock set in the modem.
  PhnPDConfigPTLMMode | The protocol transport layer mechanism to be used to talk to the PDE.

Definition at line 44 of file hsPhoneLocationTypes.h.

    00045   {
    00046     PhnPDConfigIPAddr = 1,  /**< Binary value of the Position Determination Entity (PDE) IP Address */
    00047     PhnPDConfigPortID,      /**< Binary value of the PDE Port ID. */
    00048     PhnPDConfigGPSLock,     /**< Level of GPS lock set in the modem. */
    00049     PhnPDConfigPTLMMode     /**< The protocol transport layer mechanism to be used to talk to the PDE. */
    00050   }_PhnPDSessionConfigParamType;

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:07:20 2008 for Palm API Guide