API Guide Home (Online version only) |

# SndCodecCustomControlType Struct Reference

## Detailed Description

Holds Custom Control type information for the Extended Sound Manager.

This structure is used to set/get values specific to a codec. Note that if this custom control comes from a 68K app, it's the responsibility of the 68K app to flip and align the fields of the structure correctly. The fields are defined as being in little-endian format.

Definition at line 75 of file PalmSoundCustomCtrl.h.

## Data Fields

- UInt32 apiCreator
- UInt32 apiSelector
- void * valueP
- UInt16 * valueLenP

## Field Documentation

UInt32 apiCreator

Codec creator. (codecDriverIMAADPCM...)

Definition at line 76 of file PalmSoundCustomCtrl.h.

UInt32 apiSelector

Codec selector. (codecIMAADPCMSetBlockSize...)

Definition at line 77 of file PalmSoundCustomCtrl.h.

void* valueP

Pointer to the parameters to be passed to the codec.

Definition at line 78 of file PalmSoundCustomCtrl.h.

UInt16* valueLenP

Size of the parameters to be passed to the codec.

Definition at line 79 of file PalmSoundCustomCtrl.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:29 2008 for Palm API Guide