API Guide Home (Online version only) |

# HsErrors.h

Go to the documentation of this file.

    00001 /** @ingroup System
    00002  *
    00003  */
    00004 /**
    00005  * @file HsErrors.h
    00006  * Errors that are not part of any particular component but can be returned by
    00007  * many different system components.
    00008  *
    00009  * \license
    00010  *
    00011  *    Copyright (c) 2002 Handspring Inc., All Rights Reserved
    00012  *
    00013  * \author Kiran Prasad
    00014  *
    00015  * $Id: //device/handheld/dev/sdk/2.2.2/incs/common/system/HsErrors.h#1 $
    00016  *
    00017  *****************************************************************************/
    00018
    00019 #ifndef __HS_ERRORS_H__
    00020 #define __HS_ERRORS_H__
    00021
    00022
    00023 #if 0
    00024 #pragma mark -------- Radio Errors --------
    00025 #endif
    00026 /**
    00027  * The radio is currently off and you can not perform the action requested.
    00028  **/
    00029 #define hsErrRadioOff                     (hsOEMRadioErrorClass | 0x01)
    00030
    00031 /**
    00032  * The radio is currently not registered and you can not perform the action
    00033  * reuqested.
    00034  **/
    00035 #define hsErrRadioNotRegistered           (hsOEMRadioErrorClass | 0x02)
    00036
    00037 /**
    00038  * The radio is currently on an active voice call and so your request can not be
    00039  * handled.
    00040  **/
    00041 #define hsErrVoiceCallActive              (hsOEMRadioErrorClass | 0x03)
    00042
    00043 /**
    00044  * For GSM Radio Only,
    00045  *   Your SIM is not ready to perform this action. This can either mean there is
    00046  *   no SIM or it is not fully read yet.
    00047  **/
    00048 #define hsErrSimNotReady                  (hsOEMRadioErrorClass | 0x04)
    00049
    00050 /**
    00051  * Your Radio is currently locked and therefore we can perform the action
    00052  * requested.
    00053  **/
    00054 #define hsErrPhoneLocked                  (hsOEMRadioErrorClass | 0x05)
    00055
    00056 /**
    00057  * Phone is not activated.
    00058  **/
    00059 #define hsErrPhoneNotActivated            (hsOEMRadioErrorClass | 0x06)
    00060
    00061 #endif

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:06:53 2008 for Palm API Guide