API Guide Home (Online version only) |

# PhnSATEventGetInput Struct Reference

## Detailed Description

Definition at line 997 of file HsPhoneEvent.h.

## Data Fields

- UInt32 signature
- UInt32 notificationType
- UInt32 textOffset
- UInt16 format
- UInt16 helpInfo
- UInt16 echoMode
- UInt16 minSize
- UInt32 defaultOffset
- UInt16 maxSize
- UInt16 pad

## Field Documentation

UInt32 signature

Definition at line 998 of file HsPhoneEvent.h.

UInt32 notificationType

Definition at line 999 of file HsPhoneEvent.h.

UInt32 textOffset

Definition at line 1001 of file HsPhoneEvent.h.

UInt16 format

See GSMSATEventInputFormatEnum

Definition at line 1002 of file HsPhoneEvent.h.

UInt16 helpInfo

Definition at line 1003 of file HsPhoneEvent.h.

UInt16 echoMode

Definition at line 1004 of file HsPhoneEvent.h.

UInt16 minSize

Definition at line 1005 of file HsPhoneEvent.h.

UInt32 defaultOffset

offset of default value string at end of cmd block (0 if none) <chg 05-13-2002 TRS> bug # 13829

Definition at line 1006 of file HsPhoneEvent.h.

UInt16 maxSize

Definition at line 1007 of file HsPhoneEvent.h.

UInt16 pad

Definition at line 1008 of file HsPhoneEvent.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:26 2008 for Palm API Guide