API Guide Home (Online version only) |

# PhnSATEventRefresh Struct Reference

## Detailed Description

Definition at line 1082 of file HsPhoneEvent.h.

## Data Fields

- UInt32 signature
- UInt32 notificationType
- UInt32 EFList
- UInt16 refreshType
- UInt16 pad

## Field Documentation

UInt32 signature

Definition at line 1083 of file HsPhoneEvent.h.

UInt32 notificationType

Definition at line 1084 of file HsPhoneEvent.h.

UInt32 EFList

This is a bitmap of the efs to be refreshed

Definition at line 1085 of file HsPhoneEvent.h.

UInt16 refreshType

Definition at line 1086 of file HsPhoneEvent.h.

UInt16 pad

Definition at line 1087 of file HsPhoneEvent.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:27 2008 for Palm API Guide