API Guide Home (Online version only) |

# NetMasterClientEventInfoType Struct Reference

Collaboration diagram for NetMasterClientEventInfoType:

[legend]

## Detailed Description

This structure is passed as the 'detailsP' of the notification.

See also:
  Palm OS Notification Manager

Definition at line 199 of file NetMasterLibTypes.h.

## Data Fields

- UInt16 version
- NetMasterClientEventEnum eventID
- union {
  - void * genericEventDataP
  - NetMasterClientEventVPNConnInstallType * vpnConnInstallP
- } eventData
- UInt32 inReserved1
- UInt32 inReserved2
- UInt32 inReserved3
- UInt32 inReserved4

## Field Documentation

UInt16 version

Version of this structure -- all future versions MUST define backward compatible Event structures. NetMaster Library sets this to netMasterClientCurrentEventVersion at the time the library was built.

Definition at line 209 of file NetMasterLibTypes.h.

NetMasterClientEventEnum eventID

Event ID

Definition at line 212 of file NetMasterLibTypes.h.

void* genericEventDataP

genericEventDataP is for the convenience of the internal code only.

Definition at line 219 of file NetMasterLibTypes.h.

NetMasterClientEventVPNConnInstallType* vpnConnInstallP

For netMasterClientEventVPNConnInstall

Definition at line 222 of file NetMasterLibTypes.h.

union { ... } eventData

Data corresponding to the event ID

UInt32 inReserved1

Reserved values; Set to 0 by NetMaster library

Definition at line 227 of file NetMasterLibTypes.h.

UInt32 inReserved2

Reserved values; Set to 0 by NetMaster library

Definition at line 228 of file NetMasterLibTypes.h.

UInt32 inReserved3

Reserved values; Set to 0 by NetMaster library

Definition at line 229 of file NetMasterLibTypes.h.

UInt32 inReserved4

Reserved values; Set to 0 by NetMaster library

Definition at line 230 of file NetMasterLibTypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:14 2008 for Palm API Guide