API Guide Home (Online version only) |

# CamLibBitmapInfoTag Struct Reference

## Detailed Description

Bitmap info structure for every format except PalmBMPV4. Data starts after the parameters.

Definition at line 175 of file palmOneCameraCommon.h.

## Data Fields

- UInt16 width
- UInt16 height
- UInt32 numBytes
- UInt8 bitsPerPixel
- UInt8 reserved0
- UInt16 reserved1

## Field Documentation

UInt16 width

Width of the bitmap.

Definition at line 177 of file palmOneCameraCommon.h.

UInt16 height

Height of the bitmap.

Definition at line 178 of file palmOneCameraCommon.h.

UInt32 numBytes

Number or Bytes to be streamed.

Definition at line 179 of file palmOneCameraCommon.h.

UInt8 bitsPerPixel

Number of bits per pixel.

Definition at line 180 of file palmOneCameraCommon.h.

UInt8 reserved0

For packing.

Definition at line 181 of file palmOneCameraCommon.h.

UInt16 reserved1

For packing.

Definition at line 182 of file palmOneCameraCommon.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:11 2008 for Palm API Guide