API Guide Home (Online version only) |

# PalmAudioAMRParamType Struct Reference

## Detailed Description

Definition at line 450 of file palmOneCodecFormat.h.

## Data Fields

- UInt32 mode
- UInt32 dtxMode

## Field Documentation

UInt32 mode

Encoding mode (i.e. kBits/second).

Definition at line 451 of file palmOneCodecFormat.h.

UInt32 dtxMode

Discontinuous transmission mode.

Definition at line 452 of file palmOneCodecFormat.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:15 2008 for Palm API Guide