API Guide Home (Online version only) |

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - i -

- id : PhnConnectionType , PhnError , PhnSMSParams , PhnSATEventMenuRec , WAPNotificationEventType , PhnOperatorType , PhnMMIEntryType , ToneIdentifier
- identifier : ToneItemType
- idx : PhnPDPWrite
- idx0_set : PhnPDPList
- idx0_uid : PhnPDPList
- idx1_set : PhnPDPList
- idx1_uid : PhnPDPList
- idx2_set : PhnPDPList
- idx2_uid : PhnPDPList
- idx3_set : PhnPDPList
- idx3_uid : PhnPDPList
- idx4_set : PhnPDPList
- idx4_uid : PhnPDPList
- idx5_set : PhnPDPList
- idx5_uid : PhnPDPList
- idx6_set : PhnPDPList
- idx6_uid : PhnPDPList
- idx7_set : PhnPDPList
- idx7_uid : PhnPDPList
- idx_RSVD8_set : PhnPDPList
- idx_rsvd8_uid : PhnPDPList
- idx_RSVD9_set : PhnPDPList
- idx_rsvd9_uid : PhnPDPList
- ifCreator : SysWPPILaunchCmdPromptAndConfigureType , vpnNotifyVPNLibTag
- ifInstance : SysWPPILaunchCmdPromptAndConfigureType , vpnNotifyVPNLibTag
- imageBits : AddrPhotoCallerIDParamsType
- imageCount : _PalmPhotoSelections
- imageDataP : PalmImageINDEXParamType , PalmImageGIFFrameParamType
- imageDataSize : PalmImageGIFFrameParamType
- imageFormat : _PalmPhotoReadWriteParam
- imageH : _PalmPhotoSelections
- imageHeight : PalmImageGIFFrameParamType
- imageInfo : _PalmPhotoCreateParam , _PalmPhotoCaptureParamV2
- imageQuality : _PalmPhotoImageInfo
- imageWidth : PalmImageGIFFrameParamType
- imei : PhnMMIResultType
- imSoundPrefs : SoundPreference::_tonePrefs
- incoming : PhnConnectionType
- index : PhnIOTAPhnTlsRcUrlType , PhnIOTAPhnNAISIPEdgeProxyType , PhnIOTAPhnProxyAddrWdpType , PhnIOTAPhnNAISIPCfgSvr , PhnIOTAPhnNAIPPGType , PhnIOTAPhnNAISIPDataxchType , PhnIOTAPhnNAISIPDatagwyType , PhnIOTAPhnSIPRetryTimerType , PhnIOTAPhnNAIIMStore , PhnIOTAPhnSIPRetryCntType
- indication : PhnEventType::Data
- indicationCode : PhnIndicationType
- indicator : PhnSMSParams
- indicatorOn : PhnMsgBoxDataType
- indType : PhnSMSParams
- info : PhnEventType::Data , ParsedInfoList
- InfoBuffer : NetworkDeviceQueryData
- InfoBufferLength : NetworkDeviceQueryData
- infoP : _PalmPhotoExtraInfo
- infoSize : _PalmPhotoExtraInfo
- InfoSize : NetworkDeviceQueryData
- InfoSizeRequired : NetworkDeviceQueryData
- infoType : _PalmPhotoExtraInfo
- init_rrq : PhnOnexMipRRQType
- initialObjectIDHint : FrmNavHeaderTag
- inReserved1 : NetMasterClientEventVPNConnInstallType , NetMasterClientEventInfoType
- inReserved2 : NetMasterClientEventVPNConnInstallType , NetMasterClientEventInfoType
- inReserved3 : NetMasterClientEventInfoType
- inReserved4 : NetMasterClientEventInfoType
- interactive : MMProLaunchStruct , MMProLaunchStruct2
- iota_ph_dls_lock : PhnIOTAPhnDlsLockType
- iotaInfo : PhnEventType::Data
- ipAllocType : NetServicesProfile , NetServicesProfileV1
- ipGateway : NetServicesProfile , NetServicesProfileV1
- ipMask : NetServicesProfileV1 , NetServicesProfile
- ipPrimaryDNS : NetServicesProfileV1 , NetServicesProfile
- ipSecondaryDNS : NetServicesProfileV1 , NetServicesProfile
- isForeground : HS_HTTPLibAppinfo_
- isInterlaced : PalmImageGIFFrameParamType
- isRoaming : PhnOperatorType
- isVFSFileName : _HelperServiceMMSObjectType
- item : _pluginSendParams
- itemDescriptors : _pluginQueryParams
- itemLength : ParsedInfo
- itemSizes : _pluginQueryParams
- IVOPQuantization : PalmVideoMPEG4EncodeParamType

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:08 2008 for Palm API Guide