API Guide Home (Online version only) |

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - r -

- rcptAlert : SoundPreferenceSMS
- reasonCode : WUNotificationEventType
- record : PhnSATEventMenu
- recordCount : PhnSATEventMenu
- RecordIndex : P1clRecordDetails
- recordNum : AddrCallerIDParamsType , AddrPhotoCallerIDParamsType
- RecordUId : P1clRecordDetails
- rect : _PalmPhotoDisplayParam
- recvBufferSize : HS_HTTPLibAppinfo_
- reducedRate : PalmAudioQCELPParamType
- ref : AddrCallerIDParamsType
- refNum : NBSNotificationEventType , HS_HTTPLibNetLibInfo_
- refreshType : PhnSATEventRefresh
- registration : PhnEventType::Data
- reminderTone : SoundPreferenceCalendar
- repeatAlarmTimes : SoundPreferenceCalendar
- repeated : PhoneAppLaunchCmdSendDTMFToneType
- repeatInterval : SoundPreferenceCalendar
- repeatNewPwd : PhnMMIEntryType
- reqIP : NetServicesProfile , NetServicesProfileV1
- requestSmsInfo : PhnLibLengthInfoType
- reserved : _PalmPhotoSelectionParam , LocDBRecordTag , LocsLibSelLocsTag , _PalmPhotoReadWriteParam , NetPrefGPRSQOSType , ApptTimeZoneType , _PalmPhotoFileLocation , _PalmPhotoExtraInfo , LocationDataTag
- reserved0 : NBSNotificationEventType , CamLibBitmapInfoTag
- reserved1 : PmConnectorNotifyDataType , AddressAppRecord , PhnPDPWrite , NBSNotificationEventType , HsSndPortInfo , HsSndBufferData , CamLibBitmapInfoTag
- reserved1a : NBSNotificationEventType
- reserved2 : UPNotificationEventType , tagIOTANotificationEventType , PmConnectorNotifyDataType , PhnPDPWrite , HsSndPortInfo , NBSNotificationEventType , HsSndBufferData , WUNotificationEventType
- reserved3 : tagIOTANotificationEventType , NBSNotificationEventType , PhnPDPWrite , WUNotificationEventType , UPNotificationEventType
- reserved4 : PhnPDPWrite
- reserved5 : PhnPDPWrite
- reserved6 : PhnPDPWrite
- response : DevAppLaunchCmdGenericCallType
- restartInterval : PalmImageJPEGEncodeParamType
- restrict_ha_addr : PhnPDPPayload
- restrict_home_addr : PhnPDPPayload
- restrict_mn_aaa_spi : PhnPDPPayload
- restrict_mn_aaa_ss : PhnPDPPayload
- restrict_mn_ha_spi : PhnPDPPayload
- restrict_mn_ha_ss : PhnPDPPayload
- restrict_nai : PhnPDPPayload
- restrict_rev_tunnel_pref : PhnPDPPayload
- result : DialPnlIsDialingAvailableParamsType , PhnUSSDEventType
- resultString : AddrCallerIDParamsType
- ret : _pluginGetInfoParams , _pluginExtendedQueryParams , _pluginSendParams , _pluginQueryParams , _pluginParams
- rev_tunnel_pref : PhnPDPWrite , PhnPDPPayload
- ringerID : PhnRingingProfileType
- roamCallGuardEnable : PhnRoamPrefInfoType
- roamingTone : SoundPreferencePhone
- roamRingerEnable : PhnRoamPrefInfoType
- roamRingerID : PhnRoamPrefInfoType
- rowByte : PalmImageParamType , PalmImageINDEXParamType
- rrq_timer : PhnOnexMipRRQType
- rulesEnabled : HsDialPrefsUSDialingRulesType
- rwCallback : _PalmPhotoReadWriteParam

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:08 2008 for Palm API Guide