API Guide Home (Online version only) |

# _PhnCDMAMediaTVSettings Struct Reference

## Detailed Description

Definition at line 905 of file HsPhoneCDMATypes.h.

## Data Fields

- UInt32 version
- char homePage [phnMaxUrlLen+1]
- UInt32 proxyAddr
- UInt16 proxyPort
- UInt32 streamBufferSize
- UInt32 streamTimeout

## Field Documentation

UInt32 version

(1) should be set to the structure version that you are requesting

Definition at line 907 of file HsPhoneCDMATypes.h.

char homePage[phnMaxUrlLen+1]

NULL terminated string

Definition at line 909 of file HsPhoneCDMATypes.h.

UInt32 proxyAddr

proxy IP address

Definition at line 910 of file HsPhoneCDMATypes.h.

UInt16 proxyPort

proxy port

Definition at line 911 of file HsPhoneCDMATypes.h.

UInt32 streamBufferSize

stream buffer size

Definition at line 912 of file HsPhoneCDMATypes.h.

UInt32 streamTimeout

streaming timeout

Definition at line 913 of file HsPhoneCDMATypes.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:09 2008 for Palm API Guide