e80
; B5C-LB36.INS		Wayne Masters
;  05/05/86		Potpourri, 408-378-7474
;
;  This is an insert, not an overlay, for BYE5 and the Ampro Little-Board
;  running a v3.6, or later, BIOS, which uses a spare CTC channel to main-
;  tain a memory resident date/time clock.
;
;  This routine expects the clock to be initialized to the correct date/time
;  before executing the BYE5 program.
;
;  Set the following equates in BYE5:
;
; CLOCK   EQU	YES	(Same for KMD)
; TIMEON  EQU	YES	(Same for KMD)
; BIN2BCD EQU	YES
;
;  Delete the existing TIME routine in BYE5 and replace it with this insert.
;
;
CENTURY	EQU	19H		; Change this every 100 years
LDIR	EQU	0B0EDH		; Z80 ldir
;
;
TIME:	LDA	CPYFLG
	ORA	A		; See if we have already copied the JMP table
	JNZ	TIME1		; Yes, skip this
;
	LXI	D,WBOOT		; Build BIOS entry table
	LHLD	1		; Get BIOS start
	LXI	B,51		; Bytes to move
	DW	LDIR		; Move it
;
	CALL	GETTBL		; Get address of next JMP table
	LXI	D,NXTTBL	; (HL) has BIOS nxttbl address
	LXI	B,15		;
	DW	LDIR		; Move the table
	MVI	A,0FFH
	STA	CPYFLG		; Set the flag so we only do this once
;
TIME1:	CALL	TOD		; Get clock base address
;
; (HL) now has address of clock data
;
	DI			; Disable interrupts while we do this
	LXI	D,SEC		; Move time/date
	LXI	B,6
	DW	LDIR		; Save time/date
	EI			; Enable interrupts now
;
; Everthing needed has been moved into this program area.
;
	CALL	J2MD		; Convert Julian date to month/day
;
; Now convert and store date/time from binary to bcd and put into BYE5
;
	MVI	A,CENTURY
	STA	RTCBUF+3	; Century
	LDA	CYEAR
	CALL	BINBCD
	STA	RTCBUF+4	; Year
	LDA	TMONTH
	CALL	BINBCD
	STA	RTCBUF+5	; Month
	LDA	TDAY
	CALL	BINBCD
	STA	RTCBUF+6	; Day
	LDA	HOUR
	STA	CCHOUR		; Binary form for cchour
	CALL	BINBCD
	STA	RTCBUF		; BCD form for buffer hours
	LDA	MIN
	STA	CCMIN		; Binary minutes
	CALL	BINBCD
	STA	RTCBUF+1	; BCD minutes
	LDA	SEC
	CALL	BINBCD
	STA	RTCBUF+2	; Seconds
;
	RET			; All done
;
;
;  Convert Julian to month/day
;
J2MD:	LXI	D,MTHS		; Intialize month pointer
	LHLD	JDAY		; Julian day in (HL)
	INX	H		; Adjust for ordinal 0
	XRA	A
	MOV	B,A		; Initialize high byte of sub with 0
	INR	A
	STA	TMONTH		; Initialize month to 1

J2MD1:	LDAX	D
	ORA	A		; Clear carry
	MOV	C,A
	MOV	A,L		; May be day
	DW	42EDH		; SBC HL,BC
	JC	J2MD2
	JZ	J2MD2
	LDA	TMONTH
	INR	A		; Update month
	STA	TMONTH
	INX	D
	JMP	J2MD1

J2MD2:	STA	TDAY		; Set day
	RET
;
	DB	0
MTHS:	DB	31,29,31,30,31,30,31,31,30,31,30,31
CPYFLG:	DB	0		; Flag for JMP table copied?
;
; BIOS JMP table, moved from the BIOS on first call to TIME
;
WBOOT:	DB	0,0,0		; Warm start
	DB	0,0,0		; Console status
	DB	0,0,0		; Console character in
	DB	0,0,0		; Console character out
	DB	0,0,0		; List character out
	DB	0,0,0		; Punch character out
	DB	0,0,0		; Reader character in
	DB	0,0,0		; Seek to home position
	DB	0,0,0		; Select disk
	DB	0,0,0		; Set track number
	DB	0,0,0		; Set sector number
	DB	0,0,0		; Set DMA address
	DB	0,0,0		; Read disk
	DB	0,0,0		; Write disk
	DB	0,0,0		; Return list status
	DB	0,0,0		; Sector translate
;
GETTBL:	DB	0,0,0		; Point to more jumps, =>v3.6 BIOS only
;
NXTTBL:
	DB	0,0,0		; JMP swap
	DB	0,0,0		; Get hd table info
	DB	0,0,0		; Get/set phytab access
	DB	0,0,0		; Get phytab entry address
TOD:	DB	0,0,0		; Get base address of clock tick

; Time/Date counters from BIOS

SEC:	DB	0
MIN:	DB	0
HOUR:	DB	0
JDAY:	DB	0,0		; Julian day 0-366 for leap year
CYEAR:	DB	0

TMONTH:	DB	0		; Temp storage for month
TDAY:	DB	0		; Temp storage for day
;
; End of B5C-LB36
;

0

