Correction to CCRT description (in ILBM docs):

   Comment on "direction" variable should read

   /* 0 = don't cycle, -1 = cycle forwards (1,2,3),
      1 = cycle backwards (3,2,1)                   */
