  +------------------------------------------------------------------------+
  |    This report is created by ASTRA v.7.20     Feb-03-2025 8:48:05 AM   |
  +------------------------------------------------------------------------+
                                       
    Version:                           ASTRA - Advanced Sysinfo Tool 7.20
    Registered To:                     Sysinfo Lab
    License Type:                      Professional for 1 computer
    Home Page:                         www.sysinfolab.com
                                       
    Report Date:                       Feb-03-2025
    Report Time:                       8:48:05 AM
                                       
                  +-----------------------------------------+
                  |              System Summary             |
                  +-----------------------------------------+
  Processor 
    Processor:                         AMD Ryzen 5 5600 3500 MHz
    CPU Clock:                         3500.0 MHz (35.0 x 100.0 MHz)
    Level 1 Cache:                     6 x 32 kB + 6 x 32 kB (data+instr.)
    Level 2 Cache:                     6 x 512 kB
    Level 3 Cache:                     1 x 32 MB
  Motherboard
    System Name:                       Micro-Star International Co., Ltd. MS-7A38
    Board Model:                       Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
    BIOS Version:                      American Megatrends International, LLC. B.L0
    BIOS Version:                      AMI BIOS 08.00.10
    Chipset Name:                      AMD B450 (Promontory)
    Northbridge Vendor:                Advanced Micro Devices (AMD)
    Northbridge:                       Starship/Matisse Root Complex
    Southbridge Vendor:                Advanced Micro Devices (AMD)
    Southbridge:                       B450 Fusion Controller Hub (FCH)
    PCI Bus Version:                   3.0
    PnP Version:                       Not Present
    DMI/SMBIOS Version:                2.8
  Memory
    Base Memory:                       629 kB (582 kB free)
    Extended Memory:                   16700340 kB (16308.93 MB)
    System Memory:                     16310 MB
    Memory Module:                     8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
    Memory Module:                     8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
  Storage
    Disk Size:                         953869 MB (931.51 GB)
    Disk Size:                         953869 MB (931.51 GB)
    Disk Size:                         953869 MB (931.51 GB)
    Disk Size:                         238475 MB (232.89 GB)
  Monitor
    Monitor Vendor:                    AOC International (TPV Technology)
    Monitor Model:                     Q27G2G3 / Q27G2E / 27G2G4 / 27G2G8 / Q27G2G4 / Q27G2WG4 / 27G2G5 / U27P2G6B / 27V2G5 / 27B2 / 27B2G5 (27.0")
  Video Card
    Video Chip Vendor:                 NVIDIA Corporation
    Video Chip:                        GeForce RTX 3060 Ti LHR [GA104]
    VESA OEM String:                   NVIDIA
    Bus Type:                          PCI Express 4.0 x16
    Video Memory Size:                 8 GB GDDR6
  Sound
    Sound Chip Vendor:                 NVIDIA Corporation
    Sound Chip:                        GA104 High Definition Audio Controller
    Audio Codec Name:                  NVidia GPU GA104 HDMI/DP
  Sound 2
    Sound Chip Vendor:                 Advanced Micro Devices (AMD)
    Sound Chip:                        Starship/Matisse HD Audio Controller
    Audio Codec Name:                  Realtek ALC892
  Operating System
    DOS Version:                       FreeDOS 7.10 rev.0 in HMA
  Network
    Network Chip Vendor:               Realtek Semiconductor
    Network Chip:                      RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
  Ports
    Mouse Type:                        PS/2 (version 7.05) 
    LPT Ports:                         LPT1 (0378h) 
    COM Ports:                         COM1 (03F8h) 
    Joystick:                          Not Present
                                       
                  +-----------------------------------------+
                  |               Motherboard               |
                  +-----------------------------------------+
  System
    System Vendor:                     Micro-Star International Co., Ltd.
    Product Name:                      MS-7A38
    Version:                           8.0
    Serial Number:                     To be filled by O.E.M.
    UUID:                              12983CA982A41496AAC82CF05DD2A722
    Wake-up Type:                      Power Switch
    SKU Number:                        To be filled by O.E.M.
    Family:                            To be filled by O.E.M.
  Motherboard
    Motherboard Vendor:                Unknown (0001)
    Vendor URL:                        Unknown
    Board Model:                       Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
    Motherboard ID:                    BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
    Version:                           8.0
    Serial Number:                     07A3880_KB1E018736
    Asset Tag:                         To be filled by O.E.M.
    BIOS Version:                      American Megatrends International, LLC. B.L0
    BIOS Version:                      AMI BIOS 08.00.10
    BIOS Date:                         10/26/2023
    Chipset Name:                      AMD B450 (Promontory)
    Northbridge Vendor:                Advanced Micro Devices (AMD)
    Northbridge:                       Starship/Matisse Root Complex
    Southbridge Vendor:                Advanced Micro Devices (AMD)
    Southbridge:                       B450 Fusion Controller Hub (FCH)
  Onboard Device 1
    Description:                       Broadcom 5762
    Device Type:                       Ethernet
    Status:                            Disabled
  Configuration Options
    To be filled by O.E.M.
  System Enclosure
    Manufacturer:                      Micro-Star International Co., Ltd.
    Type:                              Desktop
    Version:                           8.0
    Serial Number:                     To be filled by O.E.M.
    Asset Tag:                         To be filled by O.E.M.
    Boot-up State:                     Safe
    Power Supply State:                Safe
    Thermal State:                     Safe
    Security Status:                   None
    OEM-defined:                       00000000h
    Height:                            0.0 sm
    Power Cords:                       1
    Contained Element:                 0
                                       
                  +-----------------------------------------+
                  |                  CPU                    |
                  +-----------------------------------------+
  CPU 
    Processor:                         AMD Ryzen 5 5600 3500 MHz
    Coprocessor:                       Internal
    CPU Clock:                         3500.0 MHz
    Level 1 Cache:                     6 x 32 kB + 6 x 32 kB (data+instr.)
    Level 2 Cache:                     6 x 512 kB
    Level 3 Cache:                     1 x 32 MB
    Code Name:                         Vermeer (Zen 3)
    Manufacturing Process:             7 nm
    FSB Clock:                         100.0 MHz
    Multiplier:                        35.0
    Expected Clock:                    3500 MHz
    Overclocking Support:              Unlocked Multiplier
    AMD Core Performance Boost:        Supported (Enabled)
    Max Turbo Clock:                   4450.0 MHz
    Processor Topology:                Nodes: 1, CPU Complexes (CCX): 1, Cores: 6, Threads: 12
    Socket Type:                       Socket AM4
    Instruction Set:                   IA-32, AMD64, MMX, AMDMMX, SSE, SSE2, SSE3, SSSE3
    Instruction Set:                   SSE4.1, SSE4.2, SSE4A, AVX, AVX2, AES, FMA, SHA, AMD-V
    Maximum Temperature (Tjmax):       95 øC (203 øF)
    Core Voltage:                      1.125 V
    Infinity Fabric Clock (FCLK):      1800.0 MHz
    Vendor:                            AuthenticAMD
    Processor Name:                    AMD Ryzen 5 5600 6-Core Processor
    Processor Type:                    Original OEM Processor
    CPUID:                             Family: 15, Model: 1, Stepping: 2
    Ext. Family/Model:                 Family: 10, Model: 2
    CPU Signature:                     00A20F12h
    Number of Cores:                   6
    Logical Cores Count:               12
    Core Stepping:                     VMR-B2
    OPN Code:                          100-000000927, 100-100000927BOX
    Microcode Revision:                A20120Eh
    SMU Firmware Version:              56.76.00
    Power Table Version:               380905h
    Max TDP:                           65 Wattes
    Power Limit:                       76 Wattes
    Thermal Design Current (TDC):      60 Amps
    Electrical Design Current (EDC):   90 Amps
    Transistor Count:                  6240 million
    Die Size:                          81 mm2 + I/O 122 mm2
    Launch Date:                       April, 2022
    Recommended Price (USD):           $199
  Hardware Monitoring
    Core Voltage:                      1.138 V
    Core Voltage (SVI2 TFN):           1.131 V
    SoC Voltage (SVI2 TFN):            1.075 V
    Package Temperature:               58 øC (136 øF)
    CCD1 Temperature:                  51 øC (124 øF)
    SoC Temperature:                   46 øC (115 øF)
    L3 Cache Temperature:              46 øC (115 øF)
    Package Power:                     44.9 Wattes
    Cores Power:                       17.1 Wattes
    SoC Power:                         13.7 Wattes
    VDDIO Mem Power:                   11.2 Wattes
    VDD18 Power:                       1.0 Wattes
    FSB Clock:                         100.0 MHz
  Core 1
    Temperature Core:                  56 øC (133 øF)
    Core Power:                        5.2 Wattes
    Core Clock:                        4450.0 MHz
    Multiplier:                        44.5
  Instruction Set
    Floating-Point Unit On-Chip:                  [X]
    IA MMX Technology:                            [X]
    SSE Instruction Set:                          [X]
    SSE2 Instruction Set:                         [X]
    SSE3 Instruction Set:                         [X]
    Supplemental SSE3 Instruction Set:            [X]
    SSE4.1 Instruction Set:                       [X]
    SSE4.2 Instruction Set:                       [X]
    Advanced Vector Extensions (AVX):             [X]
    Advanced Vector Extensions 2 (AVX2):          [X]
    AVX-512 Foundation Instructions:              [ ]
    AVX-512 Prefetch Instructions:                [ ]
    AVX-512 Exponential and Reciprocal:           [ ]
    AVX-512 Conflict Detection:                   [ ]
    AVX-512 Byte and Word Instructions:           [ ]
    AVX-512 Doubleword and Quadword:              [ ]
    AVX-512 Vector Length Extensions:             [ ]
    AVX-512 Integer Fused Multiply-Add:           [ ]
    AVX-512 Vector Bit Manipulation:              [ ]
    AVX-512 QVNNI Instructions:                   [ ]
    AVX-512 QFMA Instructions:                    [ ]
    AVX-512 VBMI2 Instructions:                   [ ]
    AVX-512 VNNI Instructions:                    [ ]
    AVX-512 BITALG Instructions:                  [ ]
    Galois Field NI/Affine Transformation:        [ ]
    VEX-encoded AES-NI (VAES):                    [X]
    VEX-encoded PCLMUL (VPCL):                    [X]
    PCOMMIT Instruction:                          [ ]
    CLWB Instruction:                             [X]
    PREFETCHWT1 Instruction:                      [ ]
    Software Guard Extensions (SGX):              [ ]
    SGX Launch Configuration:                     [ ]
    FMA Instructions Set:                         [X]
    AES Instructions Set:                         [X]
    Intel Extended Memory 64 Tech.:               [ ]
    Intel Architecture - 64 (IA-64):              [ ]
    AMD MMX Instruction Extensions:               [X]
    AMD 3DNow! Instructions:                      [ ]
    AMD 3DNow! Extensions:                        [ ]
    AMD 3DNow! Prefetch:                          [X]
    AMD SSE4A Extensions:                         [X]
    AMD eXtended OPeration (XOP):                 [ ]
    AMD Misaligned SSE:                           [X]
    AMD64 Architecture:                           [X]
    Cyrix Extended MMX:                           [ ]
    CMPXCHG8 Instruction Supported:               [X]
    CMPXCHG16 Instruction Supported:              [X]
    Fast System Call:                             [X]
    Conditional Move Instruction:                 [X]
    CLFLUSH Insruction Supported:                 [X]
    Fast Save and Restore:                        [X]
    Monitor/MWAIT Instructions:                   [X]
    SYSCALL/SYSRET Instructions:                  [X]
    LAHF/SAHF Instructions:                       [X]
    POPCNT Insruction Supported:                  [X]
    XSAVE Insructions Supported:                  [X]
    OS Supports XSAVE Instructions:               [ ]
    PCLMULQDQ Instruction Supported:              [X]
    MOVBE Insruction Supported:                   [X]
    F16C Insruction Supported:                    [X]
    RDTSCP Insruction Supported:                  [X]
    RDRAND Insruction Supported:                  [X]
    (RD/WR)(FS/GS) BASE Instructions:             [X]
    Bit Manipulation 1 Instructions:              [X]
    Bit Manipulation 1 Instructions:              [X]
    Enhanced REP MOVSB/STOSB:                     [X]
    INVPCID Instruction:                          [X]
    XSAVEOPT Instruction:                         [X]
    RDSEED Instruction:                           [X]
    ADCX/ADOX Instructions:                       [X]
    CLAC/STAC Instructions:                       [X]
    SCLFLUSHOPT Instruction:                      [X]
    RDPID Instruction:                            [X]
    VPOPCNT[D/Q] Instructions:                    [ ]
    Fast Short REP MOV Instruction:               [X]
    PCONFIG Instruction:                          [ ]
    WBNOINVD Instruction:                         [X]
    WaitPKG Instructions:                         [ ]
    CLDEMOTE Instruction:                         [ ]
    MOVDIRI Instruction:                          [ ]
    MOVDIRI64B Instruction:                       [ ]
    RDPRU Instruction:                            [X]
    MCOMMIT Instruction:                          [ ]
    AMD Fast Save and Restore:                    [X]
    AMD SKINIT, STGI, DEV Supported:              [X]
    AMD Light Weight Profiling (LWP):             [ ]
    AMD FMA4 Insruction Supported:                [ ]
    AMD TBM Insruction Supported:                 [ ]
    AMD MONITORX/MWAITX Instructions:             [X]
    AMD CLZERO Instruction:                       [X]
  Processor Features
    Hypervisor Present:                           [ ]
    Virtual Mode Extension:                       [X]
    Debugging Extension:                          [X]
    Page Size Extension:                          [X]
    Time Stamp Counter:                           [X]
    Model Specific Registers:                     [X]
    Physical Address Extension:                   [X]
    Machine Check Exception:                      [X]
    On-chip APIC Hardware Supported:              [X]
    Memory Type Range Registers:                  [X]
    Page Global Enable:                           [X]
    Machine Check Architecture:                   [X]
    Page Attribute Table:                         [X]
    36-bit Page Size Extension:                   [X]
    Processor Serial Number:                      [ ]
    Debug Store:                                  [ ]
    64-bit Debug Store:                           [ ]
    Self-Snoop:                                   [ ]
    Hyper-Threading Technology:                   [X]
    Pending Break Enable:                         [ ]
    CPL-Qualified Debug Store:                    [ ]
    L1 Context ID:                                [ ]
    Send Task Priority Messages:                  [ ]
    Direct Cache Access:                          [ ]
    Performance Capabilities MSR:                 [ ]
    x2APIC Architecture:                          [X]
    Advanced Bit Manipulation:                    [X]
    OS Visible Workaround:                        [X]
    Instruction Based Sampling:                   [X]
    1-GB Large Page:                              [X]
    Process Context Identifiers:                  [ ]
    Time Stamp Counter Deadline:                  [ ]
    Time Stamp Counter Adjust:                    [ ]
    Intel Virtualization Technology:              [ ]
    Intel Trusted Execution Technology:           [ ]
    Supervisor Mode Execution Protection:         [X]
    Hardware Lock Elision:                        [ ]
    Restricted Transactional Memory:              [ ]
    Quality of Service Monitoring:                [X]
    Quality of Service Enforcement:               [X]
    Deprecated FPU CS and FPU DS:                 [ ]
    Memory Protection Extensions (MPX):           [ ]
    Processor Trace (PT):                         [ ]
    Secure Hash Algorithm Ext. (SHA):             [X]
    Debug Interface MSR:                          [ ]
    User-Mode Instruction Prevention:             [X]
    Protection Keys for User-Mode Pages:          [X] disabled
    5 Level Page Table:                           [ ]
    Total Memory Encryption (TME):                [ ]
    Speculation Control (IBRS and IBPB):          [ ]
    Single Thread Indirect Branch Predictors:     [ ]
    L1 Data Cache (L1D) Flush:                    [ ]
    ARCH_CAPABILITIES MSR:                        [ ]
    Speculative Store Bypass Disable (SSBD):      [ ]
    AMD Core Performance Boost:                   [X] enabled
    Intel Turbo Boost Max Technology 3.0:         [ ]
    AMD No-execute Page Protection:               [X]
    Hybrid Processor:                             [ ]
    AMD Secure Virtual Machine:                   [X]
    AMD Model-Specific Registers:                 [X]
    AMD Multiprocessing Capable:                  [ ]
    AMD CMP Legacy Mode:                          [X]
    AMD CR8 in Legacy Mode:                       [X]
    AMD Ext. APIC Register Space:                 [X]
    AMD Watchdog Timer:                           [X]
    AMD Translation Cache Extension:              [X]
    AMD NodeID MSR:                               [ ]
    AMD Topology Extensions:                      [X]
    AMD Core Performance Counter Ext.:            [X]
    AMD NB Performance Counter Ext.:              [X]
    AMD Streaming Performance Monitor:            [ ]
    AMD Data Breakpoint Extension:                [X]
    AMD Performance TSC:                          [ ]
    AMD L2I Performance Counter Ext.:             [X]
    AMD IRPERF Performance Counter:               [X]
    AMD Always Save/Restore FP Error Pointers:    [X]
    AMD Indirect Branch Prediction Barrier:       [X]
    AMD Indirect Branch Restricted Speculation:   [X]
    AMD IBRS Always On Mode:                      [ ]
    AMD IBRS Preferred:                           [X]
    AMD Single Thread Indirect Branch Predictor:  [X]
    AMD STIBP Always On Mode:                     [X]
    AMD Speculative Store Bypass Disable (SSBD):  [X]
    AMD SSBD Not Needed:                          [ ]
    AMD VIRT_SPEC_CTRL MSR:                       [ ]
  Power Management
    ACPI Supported:                               [ ]
    Thermal Monitor Supported:                    [ ]
    Thermal Monitor 2:                            [ ]
    Enhanced SpeedStep Technology:                [ ]
    Digital Thermal Sensor:                       [ ]
    Always Running APIC Timer:                    [X]
    Invariant TSC:                                [X]
    Power Limit Notification:                     [ ]
    Extended Clock Modulation Duty:               [ ]
    Package Thermal Management:                   [ ]
    Hardware Coordination Feedback:               [X]
    ACNT2 Capability:                             [ ]
    Performance-Energy Bias:                      [ ]
    Hardware-Managed P-State Base Support:        [ ]
    Hardware Duty Cycle Programming (HDC):        [ ]
    AMD Temperature Sensor:                       [X]
    AMD Frequency ID Control:                     [ ]
    AMD Voltage ID Control:                       [ ]
    AMD Thermal Trip:                             [X]
    AMD Thermal Monitoring:                       [X]
    AMD Software Thermal Control:                 [ ]
    AMD 100MHz Multiplier Steps:                  [ ]
    AMD Hardware P-State Control:                 [X]
    AMD Effective Frequency Interface:            [X]
    AMD Processor Feedback Interface:             [ ]
    AMD Processor Accumulator:                    [ ]
    AMD Connected Standby:                        [X]
    AMD Running Average Power Limit:              [X]
    AMD MCA Overflow Recovery:                    [X]
    AMD Software Uncorr. Error Containment/Recovery:[X]
    AMD Hardware Assert (HWA):                    [ ]
    AMD Scalable MCA:                             [X]
                                       
                  +-----------------------------------------+
                  |                CPU Cache                |
                  +-----------------------------------------+
  Level 1 Data Cache
    Size:                              6 x 32 kB
    Associativity:                     8-way
    Lines per Tag:                     1
    Line Size:                         64 byte
    TLB 4K Pages:                      
      Number of Entries:               64
      Associativity:                   full
    TLB 2/4M Pages:                    
      Number of Entries:               64
      Associativity:                   full
  Level 1 Instruction Cache
    Size:                              6 x 32 kB
    Associativity:                     8-way
    Lines per Tag:                     1
    Line Size:                         64 byte
    TLB 4K Pages:                      
      Number of Entries:               64
      Associativity:                   full
    TLB 2/4M Pages:                    
      Number of Entries:               64
      Associativity:                   full
  Level 2 Cache
    Size:                              6 x 512 kB
    Associativity:                     8-way
    Lines per Tag:                     1
    Line Size:                         64 byte
    Data TLB 4K Pages:                 
      Number of Entries:               2048
      Associativity:                   8-way
    Instr. TLB 4K Pages:               
      Number of Entries:               512
      Associativity:                   4-way
    Data TLB 2/4M Pages:               
      Number of Entries:               2048
      Associativity:                   4-way
    Instr. TLB 2/4M Pages:             
      Number of Entries:               512
      Associativity:                   2-way
  Level 3 Cache
    Size:                              1 x 32 MB
    Associativity:                     16-way
    Lines per Tag:                     1
    Line Size:                         64 byte
                                       
                  +-----------------------------------------+
                  |              CPU (SMBIOS)               |
                  +-----------------------------------------+
  Processor 
    Processor Vendor:                  Advanced Micro Devices, Inc.
    Processor Version:                 AMD Ryzen 5 5600 6-Core Processor
    Current Speed:                     3500 MHz
    External Clock:                    100 MHz
    Voltage:                           1.1 V
    Processor Upgrade:                 Socket AM4
    Processor Status:                  CPU Enabled
    Socket Designation:                AM4
    Processor Type:                    Central Processor
    Processor Family:                  AMD Zen
    Processor ID1:                     00A20F12h
    Processor ID2:                     178BFBFFh
    Max Speed:                         4450 MHz
    Socket Status:                     CPU Socket Populated
    Serial Number:                     Unknown
    Asset Tag:                         Unknown
    Part Number:                       Unknown
    CPU Core Count:                    6 (Enabled: 6)
    CPU Thread Count:                  12
    Structure Length:                  30h
                                       
                  +-----------------------------------------+
                  |            CPU (SMBIOS) Cache           |
                  +-----------------------------------------+
  Level 1 Cache
    Installed Size:                    384 kB
    Operational Mode:                  Write Back
    Current SRAM Type:                 Pipelined Burst
    Status:                            Enabled
    Socket Designation:                L1 - Cache
    Cache Socketed:                    Not Socketed
    Location:                          Internal
    Maximum Cache Size:                384 kB
    Supported SRAM Type:               Pipelined Burst
    Cache Speed:                       1 ns
    Error Correction:                  Multi-bit ECC
    System Cache Type:                 Unified
    Associativity:                     8-way Set-Associative
    Structure Length:                  13h
  Level 2 Cache
    Installed Size:                    3 MB
    Operational Mode:                  Write Back
    Current SRAM Type:                 Pipelined Burst
    Status:                            Enabled
    Socket Designation:                L2 - Cache
    Cache Socketed:                    Not Socketed
    Location:                          Internal
    Maximum Cache Size:                3 MB
    Supported SRAM Type:               Pipelined Burst
    Cache Speed:                       1 ns
    Error Correction:                  Multi-bit ECC
    System Cache Type:                 Unified
    Associativity:                     8-way Set-Associative
    Structure Length:                  13h
  Level 3 Cache
    Installed Size:                    32 MB
    Operational Mode:                  Write Back
    Current SRAM Type:                 Pipelined Burst
    Status:                            Enabled
    Socket Designation:                L3 - Cache
    Cache Socketed:                    Not Socketed
    Location:                          Internal
    Maximum Cache Size:                32 MB
    Supported SRAM Type:               Pipelined Burst
    Cache Speed:                       1 ns
    Error Correction:                  Multi-bit ECC
    System Cache Type:                 Unified
    Associativity:                     16-way Set-Associative
    Structure Length:                  13h
                                       
                  +-----------------------------------------+
                  |                 Chipset                 |
                  +-----------------------------------------+
  Chipset
    Chipset Name:                      AMD B450
    Code Name:                         Promontory
    Chipset Type:                      Single Chip: Southbridge-only
    Manufacturing Process:             55 nm
    Launch Date:                       March, 2018
  Northbridge
    Northbridge Vendor:                Advanced Micro Devices (AMD)
    Northbridge:                       Starship/Matisse Root Complex
    Code Name:                         Vermeer (Zen 3)
    Location:                          CPU Integrated
    Infinity Fabric Clock (FCLK):      1800.0 MHz
    Manufacturing Process:             7 nm
    Hardware ID:                       VEN_1022&DEV_1480
    Revision:                          00h
    Stepping:                          VMR-B2
  Memory Controller
    Current Memory Type:               DDR4-3600
    Supported Memory Types:            DDR4-2667, DDR4-2933, DDR4-3200
    Maximum Memory Amount:             128 GB
    Current Controller Mode:           Dual-channel (128-bit)
    Supported Controller Mode:         Dual-channel (128-bit)
    Channel 0 DIMM A:                  8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
    Channel 1 DIMM A:                  8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
    Current Memory Clock:              1800.0 MHz (Effective: 3600.0 MHz)
    FSB:DRAM Ratio:                    1:18
    Memory Bandwidth:                  56.3 GB/s
    Memory Controller Clock (UCLK):    1800.0 MHz
    ECC:                               [X] disabled
    ECC Scrubbing:                     [ ]
    Mirroring Mode (RAID):             [ ]
    ECC Chipkill:                      [ ]
  Timings
    CAS Latency (CL):                  16.0
    RAS to CAS Delay (tRCD):           20
    RAS Precharge Time (tRP):          20
    RAS Active Time (tRAS):            39
    Row Cycle Time (tRC):              83
    Row Refresh Cycle Time (tRFC):     631
    Command Rate (CR):                 1T
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse GPP Bridge
    Bus Type:                          PCI Express 3.0 x4 8.0 GT/s (Current: x4 8.0 GT/s)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse GPP Bridge
    Bus Type:                          PCI Express 3.0 x8 8.0 GT/s (Current: x4 8.0 GT/s)
    Bus Bandwidth:                     7.9 GB/sec (Current: 3.9 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse GPP Bridge
    Bus Type:                          PCI Express 3.0 x16 8.0 GT/s (Current: x16 8.0 GT/s)
    Bus Bandwidth:                     15.8 GB/sec (Current: 15.8 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Bus Type:                          PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
  PCI Express Controller
    PCI Express Controller:            AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Bus Type:                          PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
  Southbridge
    Southbridge Vendor:                Advanced Micro Devices (AMD)
    Southbridge:                       B450 Fusion Controller Hub (FCH)
    Bus Type:                          PCI Express
    Manufacturing Process:             55 nm
    Hardware ID:                       VEN_1022&DEV_790E
    Revision:                          51h
    Top Marking:                       218-0891011
    Package Type:                      LFBGA-583
  Integrated Sound
    Audio Controller:                  AMD Starship/Matisse HD Audio Controller
    Audio Codec Name:                  Realtek ALC892
    Controller Type:                   High Definition Audio
    Hardware ID:                       VEN_1022&DEV_1487
    Revision:                          00h
  Integrated Storage
    Storage Controller:                AMD 400 Series Chipset SATA Controller
    Controller Type:                   Serial ATA
    Hardware ID:                       VEN_1022&DEV_43C8
    Revision:                          01h
                                       
                  +-----------------------------------------+
                  |                  BIOS                   |
                  +-----------------------------------------+
  BIOS
    BIOS Version:                      AMI BIOS 08.00.10
    BIOS Type:                         UEFI
    BIOS Model/SubModel/Revision:      FCh/01h/00h
    BIOS Date:                         12/24/18
    BIOS Copyright:                    12/24/18(C)2010 American Megatrends, Inc. All Rights Reserved
    Motherboard ID:                    BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
    BIOS ID:                           63-0100-000001-00101111-122418-Chipset
    AMI BIOS Tag:                      0AAAA000
    BIOS Size:                         512 kB
    Processor:                         686
    Chipset ID:                        Chipset
    BIOS Revision:                     0100
    PnP Version:                       1.0
    ACPI Version:                      2.0+ (ALASKA)
    MCFG Address:                      F0000000h
    MP Specification Ver.:             Not Supported
    DMI/SMBIOS Version:                2.8
    DMI/SMBIOS Structures:             62
    DMI/SMBIOS Address:                000Eh:6CF0h
    APM Version:                       Not Supported
  SMBIOS
    BIOS Vendor:                       American Megatrends International, LLC.
    BIOS Version:                      B.L0
    BIOS Date:                         10/26/2023
    BIOS ROM Size:                     16 MB
    System BIOS Version:               5.17
    Starting Segment:                  F000h
    Structure Length:                  1Ah
  Bus Supported
    PCI is Supported:                             [X]
    AGP is Supported:                             [ ]
    USB is Supported:                             [X]
    ISA is Supported:                             [ ]
    VLBus is Supported:                           [ ]
    MCA is Supported:                             [ ]
    EISA is Supported:                            [ ]
    PC Card is Supported:                         [ ]
  Boot Options
    Selectable Boot:                              [X]
    Boot From CD:                                 [X]
    ATAPI ZIP Drive Boot:                         [ ]
    LS-120 Boot:                                  [ ]
    BIOS Boot Specification:                      [X]
    Boot From PC Card:                            [ ]
    Network Service Boot Supported:               [ ]
    I2O Boot:                                     [ ]
    1394 Boot:                                    [ ]
  BIOS Features
    BIOS Characteristics:                         [X]
    ACPI Supported:                               [ ]
    PnP is Supported:                             [ ]
    APM is Supported:                             [ ]
    ESCD Support:                                 [ ]
    Enhanced Disk Drive (EDD):                    [X]
    BIOS is Upgradeable (Flash):                  [X]
    BIOS ROM is Socketed:                         [X]
    BIOS Shadowing is Allowed:                    [X]
    Smart Battery Supported:                      [ ]
    Targeted Content Distribution:                [X]
    UEFI Specification is Supported:              [X]
    Virtual Machine:                              [ ]
    Int 13h - 5.25"/360kB Floppy:                 [X]
    Int 13h - 5.25"/1.2MB Floppy:                 [X]
    Int 13h - 3.5"/720kB Floppy:                  [X]
    Int 13h - 3.5"/2.88MB Floppy:                 [X]
    Int 5h, Print Screen Service:                 [X]
    Int 9h, 8042 Keyboard Services:               [X]
    Int 14h, Serial Services:                     [X]
    Int 17h, Printer Services:                    [X]
    Int 10h, CGA/Mono Video Services:             [X]
    Int 13h - Floppy for NEC 9800:                [X]
    Int 13h - Floppy for Toshiba:                 [X]
    NEC PC-98:                                    [ ]
  ROM Extension
    Adapter Vendor:                    Intel Corporation
    Adapter Name:                      Realtek PXE B25 D00
    BIOS Version:                      PXE-EC6: UNDI driver image is invalid.
    BIOS Copyright:                    Copyright (C) 1997-2000  Intel Corporation
    Device Class:                      Network
    ROM Address:                       CF80h
    BIOS ROM Size:                     4 kB
  ROM Extension
    Device Name:                       NVIDIA GeForce RTX 3060 Ti LHR [GA104]
    BIOS Version:                      Version 94.04.46.00.D2
    BIOS Copyright:                    Copyright (C) 1996-2021 NVIDIA Corp.
    Device Class:                      Display
    ROM Address:                       C000h
    BIOS ROM Size:                     61 kB
  OEM SMBIOS Strings
    To be filled by O.E.M.
  Other SMBIOS Structures
    System Boot Information (32)
    Unknown (44)
    TPM Device (43)
    32-bit Memory Error Information (18)
    Memory Array Mapped Address (19)
    Memory Array Mapped Address (19)
    32-bit Memory Error Information (18)
    32-bit Memory Error Information (18)
    Memory Device Mapped Address (20)
    32-bit Memory Error Information (18)
    32-bit Memory Error Information (18)
    Memory Device Mapped Address (20)
    Unknown (143)
                                       
                  +-----------------------------------------+
                  |             PCI/AGP Devices             |
                  +-----------------------------------------+
  PCI/AGP
    PCI Bus Version:                   3.0
    Number of PCI Buses:               128
                                       
  Bus: 00h, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1480h):                    Starship/Matisse Root Complex
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1480
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 00h, Function: 02h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1481h):                    Starship/Matisse IOMMU
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (08h):                       System Peripheral
    SubClass (06h):                    IOMMU
    Hardware ID:                       VEN_1022&DEV_1481
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 01h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 01h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1483h):                    Starship/Matisse GPP Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Base I/O Port:                     00F00000h - 000FFFFFh
    Memory Address:                    FC800000h - FC8FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  1
    Physical Slot Number:              0
    Slot Power Limit:                  75 Wattes
                                       
  Bus: 00h, Device: 01h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1483h):                    Starship/Matisse GPP Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - FFFFh
    Memory Address:                    FC500000h - FC7FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x8 (Current: x4)
    Bus Bandwidth:                     7.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
    Physical Slot Number:              0
    Slot Power Limit:                  75 Wattes
                                       
  Bus: 00h, Device: 02h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 03h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 03h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1483h):                    Starship/Matisse GPP Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1483
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     E000h - EFFFh
    Memory Address:                    FB000000h - FC0FFFFFh
    Memory Address:                    D0000000h - E1FFFFFFh
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     15.8 GB/sec (Current: 15.8 GB/sec)
    Link Port Number:                  0
    Physical Slot Number:              0
    Slot Power Limit:                  75 Wattes
                                       
  Bus: 00h, Device: 04h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 05h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 07h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 07h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1484h):                    Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Base I/O Port:                     00F00000h - 000FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 00h, Device: 08h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1482h):                    Starship/Matisse PCIe Dummy Host Bridge
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1482
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 08h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1484h):                    Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_1484
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Base I/O Port:                     00F00000h - 000FFFFFh
    Memory Address:                    FC200000h - FC4FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  Root Port of PCI-E Root Complex
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 00h, Device: 14h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (790Bh):                    Hudson SMBus Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (0Ch):                       Serial
    SubClass (05h):                    SMBus Controller
    Hardware ID:                       VEN_1022&DEV_790B
    Revision:                          61h
    Interface:                         00h
  Device Properties
    Device Timing:                     Medium
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [X]
  Device Resources
    SMBus Port:                        0B00h
                                       
  Bus: 00h, Device: 14h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (790Eh):                    B450 Fusion Controller Hub (FCH)
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (06h):                       Bridge
    SubClass (01h):                    PCI/ISA
    Hardware ID:                       VEN_1022&DEV_790E
    Revision:                          51h
    Interface:                         00h
  Device Properties
    Device Timing:                     Medium
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [X]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1440h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 0
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1440
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1441h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 1
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1441
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 02h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1442h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 2
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1442
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1443h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 3
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1443
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 04h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1444h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 4
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1444
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 05h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1445h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 5
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1445
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 06h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1446h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 6
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1446
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 00h, Device: 18h, Function: 07h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1447h):                    Matisse/Vermeer Data Fabric: Device 18h; Function 7
    Class (06h):                       Bridge
    SubClass (00h):                    PCI/CPU
    Hardware ID:                       VEN_1022&DEV_1447
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [ ]
    I/O Access:                        [ ]
    Bus Master:                        [ ]
    66 MHz Speed Support:              [ ]
  Device Resources
                                       
  Bus: 01h, Device: 00h, Function: 00h         
    Vendor (144Dh):                    Samsung Electronics Co Ltd
    Device (A808h):                    NVMe SSD Controller SM981/PM981/PM983
    Subsys Vendor (144Dh):             Samsung Electronics Co Ltd
    Subsystem ID (A801h):              SSD 970 EVO/PRO
    Class (01h):                       Storage
    SubClass (08h):                    Non-Volatile memory controller
    Hardware ID:                       VEN_144D&DEV_A808
    Revision:                          00h
    Interface:                         02h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC800000h - FC803FFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 03h, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43D5h):                    400 Series Chipset USB 3.1 xHCI Compliant Host Controller
    Subsys Vendor (1B21h):             ASMedia Technology Inc.
    Subsystem ID (1142h):              Unknown
    Class (0Ch):                       Serial
    SubClass (03h):                    USB
    Hardware ID:                       VEN_1022&DEV_43D5
    Revision:                          01h
    Interface:                         30h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC7A0000h - FC7A7FFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 03h, Device: 00h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C8h):                    400 Series Chipset SATA Controller
    Subsys Vendor (1B21h):             ASMedia Technology Inc.
    Subsystem ID (1062h):              Unknown
    Class (01h):                       Storage
    SubClass (06h):                    Serial ATA
    Hardware ID:                       VEN_1022&DEV_43C8
    Revision:                          01h
    Interface:                         01h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    ROM Address:                       FC700000h
    Memory Address:                    FC780000h - FC79FFFFh
    System IRQ:                        10
    Interrupt Pin:                     INTB#
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 03h, Device: 00h, Function: 02h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C6h):                    400 Series Chipset PCIe Bridge
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C6
    Revision:                          01h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - FFFFh
    Memory Address:                    FC500000h - FC6FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        11
    Interrupt Pin:                     INTC#
  PCI-E Capabilities
    PCI Express Version:               3.0
    Device/Port Type:                  Upstream Port of PCI-E Switch
    Link Speed:                        8.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x4 (Current: x4)
    Bus Bandwidth:                     3.9 GB/sec (Current: 3.9 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 20h, Device: 04h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - FFFFh
    Memory Address:                    FC600000h - FC6FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  4
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
                                       
  Bus: 20h, Device: 05h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Base I/O Port:                     00F00000h - 000FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        10
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  5
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
                                       
  Bus: 20h, Device: 06h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Base I/O Port:                     00F00000h - 000FFFFFh
    Memory Address:                    FC500000h - FC5FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.5 GB/sec)
    Link Port Number:                  6
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
                                       
  Bus: 20h, Device: 07h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (43C7h):                    400 Series Chipset PCIe Port
    Class (06h):                       Bridge
    SubClass (04h):                    PCI/PCI
    Hardware ID:                       VEN_1022&DEV_43C7
    Revision:                          01h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     F000h - 0FFFh
    Base I/O Port:                     00F00000h - 000FFFFFh
    Memory Address:                    FFF00000h - 000FFFFFh
    System IRQ:                        10
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Downstream Port of PCI-E Switch
    Link Speed:                        5.0 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  7
    Physical Slot Number:              1
    Slot Power Limit:                  26 Wattes
                                       
  Bus: 25h, Device: 00h, Function: 00h         
    Vendor (10ECh):                    Realtek Semiconductor
    Device (8168h):                    RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (02h):                       Network
    SubClass (00h):                    Ethernet
    Hardware ID:                       VEN_10EC&DEV_8168
    Revision:                          15h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Base I/O Port:                     0000F000h - 0000F0FFh
    Memory Address:                    FC604000h - FC604FFFh
    Memory Address:                    FC600000h - FC603FFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               1.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        2.5 GT/s (Current: 2.5 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.25 GB/sec (Current: 0.25 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 27h, Device: 00h, Function: 00h         
    Vendor (1B21h):                    ASMedia Technology Inc.
    Device (1142h):                    ASM1042A USB 3.0 Host Controller
    Subsys Vendor (1043h):             ASUSTeK Computer Inc
    Subsystem ID (86A0h):              Unknown
    Class (0Ch):                       Serial
    SubClass (03h):                    USB
    Hardware ID:                       VEN_1B21&DEV_1142
    Revision:                          00h
    Interface:                         30h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC500000h - FC507FFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               2.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        5.0 GT/s (Current: 5.0 GT/s)
    Link Width:                        x1 (Current: x1)
    Bus Bandwidth:                     0.5 GB/sec (Current: 0.5 GB/sec)
    Link Port Number:                  1
                                       
  Bus: 29h, Device: 00h, Function: 00h         
    Vendor (10DEh):                    NVIDIA Corporation
    Device (2489h):                    GeForce RTX 3060 Ti LHR [GA104]
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (3972h):              MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
    Class (03h):                       Display
    SubClass (00h):                    VGA
    Hardware ID:                       VEN_10DE&DEV_2489
    Revision:                          A1h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    ROM Address:                       FC000000h
    Memory Address:                    FB000000h - FBFFFFFFh
    Memory Address:                    D0000000h - DFFFFFFFh
    Memory Address:                    E0000000h - E1FFFFFFh
    Base I/O Port:                     0000E000h - 0000E07Fh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 15.8 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 29h, Device: 00h, Function: 01h         
    Vendor (10DEh):                    NVIDIA Corporation
    Device (228Bh):                    GA104 High Definition Audio Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (3972h):              Unknown
    Class (04h):                       Multimedia
    SubClass (03h):                    High Definition Audio
    Hardware ID:                       VEN_10DE&DEV_228B
    Revision:                          A1h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [ ]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC080000h - FC083FFFh
    System IRQ:                        10
    Interrupt Pin:                     INTB#
  Sound
    Audio Codec Name:                  NVidia GPU GA104 HDMI/DP
    Controller Type:                   High Definition Audio
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 15.8 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 2Ah, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (148Ah):                    Starship/Matisse PCIe Dummy Function
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (13h):                       Non-Essential Instrumentation
    SubClass (00h):                    Unknown
    Hardware ID:                       VEN_1022&DEV_148A
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 2Bh, Device: 00h, Function: 00h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1485h):                    Starship/Matisse Reserved SPP
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (13h):                       Non-Essential Instrumentation
    SubClass (00h):                    Unknown
    Hardware ID:                       VEN_1022&DEV_1485
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 2Bh, Device: 00h, Function: 01h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1486h):                    Starship/Matisse Cryptographic Coprocessor PSPCPP
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (10h):                       En/Decryption
    SubClass (80h):                    Other
    Hardware ID:                       VEN_1022&DEV_1486
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC300000h - FC3FFFFFh
    Memory Address:                    FC408000h - FC409FFFh
    System IRQ:                        11
    Interrupt Pin:                     INTA#
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 2Bh, Device: 00h, Function: 03h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (149Ch):                    Matisse USB 3.0 Host Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (7A38h):              Unknown
    Class (0Ch):                       Serial
    SubClass (03h):                    USB
    Hardware ID:                       VEN_1022&DEV_149C
    Revision:                          00h
    Interface:                         30h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC200000h - FC2FFFFFh
    System IRQ:                        10
    Interrupt Pin:                     INTC#
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
                                       
  Bus: 2Bh, Device: 00h, Function: 04h         
    Vendor (1022h):                    Advanced Micro Devices (AMD)
    Device (1487h):                    Starship/Matisse HD Audio Controller
    Subsys Vendor (1462h):             Micro-Star International Co Ltd (MSI)
    Subsystem ID (9A38h):              Unknown
    Class (04h):                       Multimedia
    SubClass (03h):                    High Definition Audio
    Hardware ID:                       VEN_1022&DEV_1487
    Revision:                          00h
    Interface:                         00h
  Device Properties
    Device Timing:                     Fast
    Memory Access:                     [X]
    I/O Access:                        [X]
    Bus Master:                        [X]
    66 MHz Speed Support:              [ ]
  Device Resources
    Memory Address:                    FC400000h - FC407FFFh
    System IRQ:                        10
    Interrupt Pin:                     INTD#
  Sound
    Audio Codec Name:                  Realtek ALC892
    Controller Type:                   High Definition Audio
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 16.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 31.5 GB/sec)
    Link Port Number:                  0
                                       
                  +-----------------------------------------+
                  |              Memory Modules             |
                  +-----------------------------------------+
  Memory Slot 3
    Memory Type:                       8 GB DDR4-3602 (1801 MHz) SDRAM
    Manufacturer:                      Kingston
    DRAM Manufacturer:                 SK Hynix
    Module Type:                       Unbuffered DIMM
    Number of Ranks/Banks:             1 Ranks, 16 Banks
    Module Attributes:                 Unbuffered
    Error Checking:                    None
    JEDEC Timings:                     CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
    JEDEC Profile @ 1200 MHz:          18.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1200 MHz:          17.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1163 MHz:          16.0-16-16-38-54-408-303-187
    JEDEC Profile @ 1090 MHz:          15.0-15-15-35-50-382-284-175
    JEDEC Profile @ 1018 MHz:          14.0-14-14-33-47-357-265-163
    JEDEC Profile @ 945 MHz:           13.0-13-13-31-44-331-246-152
    JEDEC Profile @ 872 MHz:           12.0-12-12-28-40-306-227-140
    JEDEC Profile @ 799 MHz:           11.0-11-11-26-37-280-208-128
    JEDEC Profile @ 727 MHz:           10.0-10-10-24-34-255-190-117
    Data Width:                        64 bits
    SDRAM Width:                       x8
    Voltage Interface:                 1.20 V
    SPD Revision:                      1.1
    Part Number:                       KF3600C16D4/8GX   
    Manufacturing Location:            7
    Manufacture Date:                  September 2023 (2338h)
    Serial Number:                     211C9E38h
    Revision Code:                     None
    EPP Support:                       [ ]
    XMP Support:                       [X]
    XMP Revision:                      2.0
  XMP Profile 1
    Profile Name:                      XMP-3602 (1801 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1801 MHz:            18.0-20-20-39-85
    XMP Profile @ 1801 MHz:            17.0-20-20-39-85
    XMP Profile @ 1801 MHz:            16.0-20-20-39-85 (Active)
    XMP Profile @ 1689 MHz:            15.0-19-19-37-80
    XMP Profile @ 1576 MHz:            14.0-18-18-35-75
    XMP Profile @ 1463 MHz:            13.0-17-17-32-69
    XMP Profile @ 1351 MHz:            12.0-15-15-30-64
    XMP Profile @ 1238 MHz:            11.0-14-14-27-59
    XMP Profile @ 1126 MHz:            10.0-13-13-25-53
  XMP Profile 2
    Profile Name:                      XMP-2998 (1499 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1499 MHz:            17.0-17-17-36-64
    XMP Profile @ 1499 MHz:            16.0-17-17-36-64
    XMP Profile @ 1499 MHz:            15.0-17-17-36-64
    XMP Profile @ 1399 MHz:            14.0-16-16-34-60
    XMP Profile @ 1299 MHz:            13.0-15-15-32-56
    XMP Profile @ 1199 MHz:            12.0-14-14-29-52
    XMP Profile @ 1099 MHz:            11.0-13-13-27-47
    XMP Profile @ 899 MHz:             9.0-11-11-22-39
                                       
  Memory Slot 4
    Memory Type:                       8 GB DDR4-3602 (1801 MHz) SDRAM
    Manufacturer:                      Kingston
    DRAM Manufacturer:                 SK Hynix
    Module Type:                       Unbuffered DIMM
    Number of Ranks/Banks:             1 Ranks, 16 Banks
    Module Attributes:                 Unbuffered
    Error Checking:                    None
    JEDEC Timings:                     CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
    JEDEC Profile @ 1200 MHz:          18.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1200 MHz:          17.0-17-17-39-55-421-313-193
    JEDEC Profile @ 1163 MHz:          16.0-16-16-38-54-408-303-187
    JEDEC Profile @ 1090 MHz:          15.0-15-15-35-50-382-284-175
    JEDEC Profile @ 1018 MHz:          14.0-14-14-33-47-357-265-163
    JEDEC Profile @ 945 MHz:           13.0-13-13-31-44-331-246-152
    JEDEC Profile @ 872 MHz:           12.0-12-12-28-40-306-227-140
    JEDEC Profile @ 799 MHz:           11.0-11-11-26-37-280-208-128
    JEDEC Profile @ 727 MHz:           10.0-10-10-24-34-255-190-117
    Data Width:                        64 bits
    SDRAM Width:                       x8
    Voltage Interface:                 1.20 V
    SPD Revision:                      1.1
    Part Number:                       KF3600C16D4/8GX   
    Manufacturing Location:            7
    Manufacture Date:                  November 2023 (2346h)
    Serial Number:                     804C34DDh
    Revision Code:                     None
    EPP Support:                       [ ]
    XMP Support:                       [X]
    XMP Revision:                      2.0
  XMP Profile 1
    Profile Name:                      XMP-3602 (1801 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1801 MHz:            18.0-20-20-39-85
    XMP Profile @ 1801 MHz:            17.0-20-20-39-85
    XMP Profile @ 1801 MHz:            16.0-20-20-39-85 (Active)
    XMP Profile @ 1689 MHz:            15.0-19-19-37-80
    XMP Profile @ 1576 MHz:            14.0-18-18-35-75
    XMP Profile @ 1463 MHz:            13.0-17-17-32-69
    XMP Profile @ 1351 MHz:            12.0-15-15-30-64
    XMP Profile @ 1238 MHz:            11.0-14-14-27-59
    XMP Profile @ 1126 MHz:            10.0-13-13-25-53
  XMP Profile 2
    Profile Name:                      XMP-2998 (1499 MHz)
    Voltage Interface:                 1.35 V
    XMP Timings:                       CL-tRCD-tRP-tRAS-tRC
    XMP Profile @ 1499 MHz:            17.0-17-17-36-64
    XMP Profile @ 1499 MHz:            16.0-17-17-36-64
    XMP Profile @ 1499 MHz:            15.0-17-17-36-64
    XMP Profile @ 1399 MHz:            14.0-16-16-34-60
    XMP Profile @ 1299 MHz:            13.0-15-15-32-56
    XMP Profile @ 1199 MHz:            12.0-14-14-29-52
    XMP Profile @ 1099 MHz:            11.0-13-13-27-47
    XMP Profile @ 899 MHz:             9.0-11-11-22-39
                                       
                  +-----------------------------------------+
                  |             Memory (SMBIOS)             |
                  +-----------------------------------------+
  Physical Memory Array 1
    Maximum Capacity:                  131072 MB
    Location:                          System Board or Motherboard
    Use:                               System Memory
    Memory Error Correct.:             None
    Memory Devices:                    4
    Structure Length:                  17h
  Memory Device 1
    Size:                              Not Installed
    Form Factor:                       Unknown
    Memory Type:                       Unknown
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                Unknown
    Maximum Voltage:                   Unknown
    Minimum Voltage:                   Unknown
    Device Locator:                    DIMM 0
    Bank Locator:                      P0 CHANNEL A
    Total Width:                       Unknown
    Data Width:                        Unknown
    Device Set:                        00h
    Type Detail:                       Unknown
    Manufacturer:                      Unknown
    Serial Number:                     Unknown
    Asset Tag:                         
    Part Number:                       Unknown
    Structure Length:                  28h
  Memory Device 2
    Size:                              8192 MB
    Form Factor:                       DIMM
    Memory Type:                       DDR4
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                1.2 V
    Maximum Voltage:                   1.2 V
    Minimum Voltage:                   1.2 V
    Device Locator:                    DIMM 1
    Bank Locator:                      P0 CHANNEL A
    Total Width:                       64 bits
    Data Width:                        64 bits
    Device Set:                        00h
    Type Detail:                       Synchronous, Unbuffered (Unregistered)
    Manufacturer:                      Kingston
    Serial Number:                     211C9E38
    Asset Tag:                         
    Part Number:                       KF3600C16D4/8GX
    Structure Length:                  28h
  Memory Device 3
    Size:                              Not Installed
    Form Factor:                       Unknown
    Memory Type:                       Unknown
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                Unknown
    Maximum Voltage:                   Unknown
    Minimum Voltage:                   Unknown
    Device Locator:                    DIMM 0
    Bank Locator:                      P0 CHANNEL B
    Total Width:                       Unknown
    Data Width:                        Unknown
    Device Set:                        00h
    Type Detail:                       Unknown
    Manufacturer:                      Unknown
    Serial Number:                     Unknown
    Asset Tag:                         
    Part Number:                       Unknown
    Structure Length:                  28h
  Memory Device 4
    Size:                              8192 MB
    Form Factor:                       DIMM
    Memory Type:                       DDR4
    Speed:                             3600 MHz
    Configured Speed:                  3600 MHz
    Configured Voltage:                1.2 V
    Maximum Voltage:                   1.2 V
    Minimum Voltage:                   1.2 V
    Device Locator:                    DIMM 1
    Bank Locator:                      P0 CHANNEL B
    Total Width:                       64 bits
    Data Width:                        64 bits
    Device Set:                        00h
    Type Detail:                       Synchronous, Unbuffered (Unregistered)
    Manufacturer:                      Kingston
    Serial Number:                     804C34DD
    Asset Tag:                         
    Part Number:                       KF3600C16D4/8GX
    Structure Length:                  28h
                                       
                  +-----------------------------------------+
                  |                  Disk                   |
                  +-----------------------------------------+
    ATA/ATAPI drives not found
                                       
                  +-----------------------------------------+
                  |              Storage (ASPI)             |
                  +-----------------------------------------+
    ASPI manager not found
                                       
                  +-----------------------------------------+
                  |                  Drives                 |
                  +-----------------------------------------+
  BIOS Drives
    INT 13h Extensions:                3.0
  C:
    Drive Letter:                      C:
    Drive Size:                        931.51 GB
    Drive Type:                        Fixed Disk
    Cylinders:                         121601
    Heads:                             255
    Sectors:                           63
  D:
    Drive Letter:                      D:
    Drive Size:                        931.51 GB
    Drive Type:                        Fixed Disk
    Cylinders:                         121601
    Heads:                             255
    Sectors:                           63
  E:
    Drive Letter:                      E:
    Drive Size:                        931.51 GB
    Drive Type:                        Fixed Disk
    Cylinders:                         121601
    Heads:                             255
    Sectors:                           63
  F:
    Drive Letter:                      F:
    Drive Size:                        232.89 GB
    Drive Type:                        Fixed Disk
    Cylinders:                         30401
    Heads:                             255
    Sectors:                           63
                                       
  Local Drives
  C:[SYSTEM]
    Drive Letter:                      C:
    Drive Type:                        Fixed Disk
    Volume Label:                      SYSTEM
    File System:                       FAT16
    Volume Serial Number:              0805-FB80
    Total Size:                        1.99 GB
    Free Space:                        747.47 MB (36.6%)
  D:[UTILITIES]
    Drive Letter:                      D:
    Drive Type:                        Fixed Disk
    Volume Label:                      UTILITIES
    File System:                       FAT32
    Volume Serial Number:              089E-9200
    Total Size:                        29.99 GB
    Free Space:                        8.74 GB (29.2%)
                                       
                  +-----------------------------------------+
                  |            Physical Printers            |
                  +-----------------------------------------+
    LPT/PnP or USB printer not found
                                       
                  +-----------------------------------------+
                  |              Slots (SMBIOS)             |
                  +-----------------------------------------+
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    16x or x16
    Slot Designation:                  J6B2
    Slot Length:                       Long Length
    Slot ID:                           0
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J6B1
    Slot Length:                       Short Length
    Slot ID:                           1
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J6D1
    Slot Length:                       Short Length
    Slot ID:                           2
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J7B1
    Slot Length:                       Short Length
    Slot ID:                           3
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J8B4
    Slot Length:                       Short Length
    Slot ID:                           4
  Slot PCI Express
    Slot Type:                         PCI Express
    Current Usage:                     In Use
    Data Bus Width:                    1x or x1
    Slot Designation:                  J8D1
    Slot Length:                       Short Length
    Slot ID:                           5
  Slot PCI
    Slot Type:                         PCI
    Current Usage:                     In Use
    Data Bus Width:                    32 bit
    Slot Designation:                  J8B3
    Slot Length:                       Short Length
    Slot ID:                           6
  Slot PCI Express x16
    Slot Type:                         PCI Express x16
    Current Usage:                     In Use
    Data Bus Width:                    16x or x16
    Slot Designation:                  J10
    Slot Length:                       Short Length
    Slot ID:                           12
  Slot PCI Express x8
    Slot Type:                         PCI Express x8
    Current Usage:                     Available
    Data Bus Width:                    8x or x8
    Slot Designation:                  J3600 Pcie x8 slot
    Slot Length:                       Short Length
    Slot ID:                           13
  Slot PCI Express x4
    Slot Type:                         PCI Express x4
    Current Usage:                     Other
    Data Bus Width:                    4x or x4
    Slot Designation:                  J3707 Pcie x4 slot
    Slot Length:                       Short Length
    Slot ID:                           32
  Slot PCI Express x4
    Slot Type:                         PCI Express x4
    Current Usage:                     In Use
    Data Bus Width:                    4x or x4
    Slot Designation:                  J3700 PCIE x4 slot from Promontory
    Slot Length:                       Short Length
    Slot ID:                           2
  Slot PCI Express x1
    Slot Type:                         PCI Express x1
    Current Usage:                     Available
    Data Bus Width:                    1x or x1
    Slot Designation:                  J3702 PCIE x1 slot from Promontory
    Slot Length:                       Short Length
    Slot ID:                           3
  Slot PCI Express x1
    Slot Type:                         PCI Express x1
    Current Usage:                     Available
    Data Bus Width:                    1x or x1
    Slot Designation:                  J3703 PCIE x1 slot from Promontory
    Slot Length:                       Short Length
    Slot ID:                           4
  Slot PCI Express x1
    Slot Type:                         PCI Express x1
    Current Usage:                     Available
    Data Bus Width:                    1x or x1
    Slot Designation:                  J3701 M.2 WLAN/BT slot
    Slot Length:                       Short Length
    Slot ID:                           5
                                       
                  +-----------------------------------------+
                  |              Ports (SMBIOS)             |
                  +-----------------------------------------+
  Port 1 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1500
    Ext. Designator:                   USB 3.0
  Port 2 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1501
    Ext. Designator:                   USB 3.0
  Port 3 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1502
    Ext. Designator:                   USB-C
  Port 4 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1503
    Ext. Designator:                   USB 3.0
  Port 5 USB
    Int. Connector Type:               None
    Ext. Connector Type:               USB
    Port Type:                         USB
    Int. Designator:                   J1504
    Ext. Designator:                   USB 3.1
  Port 6 Network Port
    Int. Connector Type:               None
    Ext. Connector Type:               RJ-45
    Port Type:                         Network Port
    Int. Designator:                   J1503
    Ext. Designator:                   Network
  Port 7 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1704
    Ext. Designator:                   Sata Express
  Port 8 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1705
    Ext. Designator:                   Sata Express
  Port 9 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1701
    Ext. Designator:                   iSATA
  Port 10 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1702
    Ext. Designator:                   iSATA
  Port 11 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1703
    Ext. Designator:                   iSATA
  Port 12 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1706
    Ext. Designator:                   iSATA
  Port 13 Video Port
    Int. Connector Type:               None
    Ext. Connector Type:               None
    Port Type:                         Video Port
    Int. Designator:                   J1100
    Ext. Designator:                   HDMI
  Port 14 Video Port
    Int. Connector Type:               None
    Ext. Connector Type:               None
    Port Type:                         Video Port
    Int. Designator:                   J1101
    Ext. Designator:                   HDMI
  Port 15 Video Port
    Int. Connector Type:               None
    Ext. Connector Type:               None
    Port Type:                         Video Port
    Int. Designator:                   J1102
    Ext. Designator:                   DP
  Port 16 Audio Port
    Int. Connector Type:               None
    Ext. Connector Type:               Mini-jack (headphones)
    Port Type:                         Audio Port
    Int. Designator:                   J2100
    Ext. Designator:                   Front Audio
  Port 17 Audio Port
    Int. Connector Type:               None
    Ext. Connector Type:               Mini-jack (headphones)
    Port Type:                         Audio Port
    Int. Designator:                   J2101
    Ext. Designator:                   Audio Jack
  Port 18 SATA
    Int. Connector Type:               SAS/SATA Plug Receptacle
    Ext. Connector Type:               None
    Port Type:                         SATA
    Int. Designator:                   J1700
    Ext. Designator:                   Sata Express
                                       
                  +-----------------------------------------+
                  |                  Sound                  |
                  +-----------------------------------------+
  Sound
    Sound Chip Vendor:                 NVIDIA Corporation
    Sound Chip:                        GA104 High Definition Audio Controller
    Audio Codec Name:                  NVidia GPU GA104 HDMI/DP
    Hardware ID:                       VEN_10DE&DEV_228B
    Revision:                          A1h
    Bus Type:                          PCI
  Sound 2
    Sound Chip Vendor:                 Advanced Micro Devices (AMD)
    Sound Chip:                        Starship/Matisse HD Audio Controller
    Audio Codec Name:                  Realtek ALC892
    Hardware ID:                       VEN_1022&DEV_1487
    Revision:                          00h
    Bus Type:                          PCI
                                       
                  +-----------------------------------------+
                  |                 Monitor                 |
                  +-----------------------------------------+
  Monitor
    Monitor Vendor:                    AOC International (TPV Technology)
    Monitor Model:                     Q27G2G3 / Q27G2E / 27G2G4 / 27G2G8 / Q27G2G4 / Q27G2WG4 / 27G2G5 / U27P2G6B / 27V2G5 / 27B2 / 27B2G5
    Viewable Size:                     27.0" (68.5 sm)
    Serial Number:                     7393
    Manufacture Date:                  October 2023
    EDID Version:                      1.4
    Monitor ID:                        AOC2702
    Aspect Ratio:                      16:9
    Horizontal Size:                   597 mm
    Vertical Size:                     336 mm
    Gamma Factor:                      2.200
    Display Type:                      RGB Color
    Input Signal:                      Digital
    Internal Model:                    Q27G2SG4
    Internal Number:                   XFXPAHA007393
    Vertical Frequency:                48-155 Hz
    Horizontal Frequency:              230-230 kHz
  DPMS Features
    Active Off:                        [X]
    Suspend:                           [ ]
    Standby:                           [ ]
  Supported Modes
    Mode 1:                            640x480   @ 60 Hz (VGA)
    Mode 2:                            640x480   @ 67 Hz (Mac II)
    Mode 3:                            640x480   @ 72 Hz (VESA)
    Mode 4:                            640x480   @ 75 Hz (VESA)
    Mode 5:                            640x480   @ 100 Hz
    Mode 6:                            640x480   @ 120 Hz
    Mode 7:                            720x400   @ 70 Hz (VGA)
    Mode 8:                            800x600   @ 56 Hz (VESA)
    Mode 9:                            800x600   @ 60 Hz (VESA)
    Mode 10:                           800x600   @ 72 Hz (VESA)
    Mode 11:                           800x600   @ 75 Hz (VESA)
    Mode 12:                           800x600   @ 100 Hz
    Mode 13:                           800x600   @ 120 Hz
    Mode 14:                           832x624   @ 75 Hz (Mac II)
    Mode 15:                           1024x768  @ 60 Hz (VESA)
    Mode 16:                           1024x768  @ 70 Hz (VESA)
    Mode 17:                           1024x768  @ 75 Hz (VESA)
    Mode 18:                           1024x768  @ 100 Hz
    Mode 19:                           1024x768  @ 120 Hz
    Mode 20:                           1280x1024 @ 60 Hz
    Mode 21:                           1280x1024 @ 75 Hz (VESA)
    Mode 22:                           1920x1080 @ 60 Hz
    Mode 23:                           2560x1440 @ 60 Hz (Recommended)
                                       
                  +-----------------------------------------+
                  |                Video Card               |
                  +-----------------------------------------+
  Video
    Video Chip Vendor:                 NVIDIA Corporation
    Video Chip:                        GeForce RTX 3060 Ti LHR [GA104]
    Subsystem Vendor:                  Micro-Star International Co Ltd (MSI)
    Subsystem ID:                      MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
    Hardware ID:                       VEN_10DE&DEV_2489
    Revision:                          A1h
  Memory
    Video Memory Size:                 8 GB
    Memory Type:                       GDDR6
    Bus Width:                         256-bit
  Architecture
    Architecture:                      Ampere
    Code Name:                         GA104 A1h
    GPU Variant:                       GA104-202
    Unified Shaders:                   4864
    Texture Mapping Units (TPU):       152
    Render Output Units (ROPS):        80
    Streaming Multiprocessors:         38
    Tensor Cores:                      152
    RT Cores:                          38
    Level 1 Cache:                     4.75 MB
    Level 2 Cache:                     4 MB
    GPU Manufacturer:                  Samsung
    Manufacturing Process:             8 nm
    Transistor Count:                  17400 million
    Die Size:                          392 mm2
    Package Type:                      BGA-2713
    Max TDP:                           200.0 Wattes
    Launch Date:                       May, 2021
  Theoretical Performance
    Estimated Speed:                   35% of GeForce GTX 4090
  BIOS
    Bootup Message:                    PG190 SKU 12 VGA BIOS  MSINV397MH.520
    Video BIOS Version:                Version 94.04.46.00.D2
    Video BIOS Date:                   05/19/21
    BIOS Copyright:                    Copyright (C) 1996-2021 NVIDIA Corp.
    Board Model:                       GPU Board
  API Supported
    DirectX Version:                   12 (12_2)
    OpenGL Version:                    4.6
    Shader Model:                      6.7
    Vulkan Version:                    1.3
    CUDA Version:                      8.6
    OpenCL Version:                    3.0
  Other
    Bus Type:                          PCI Express 4.0 x16 16.0 GT/s (Current: x16 8.0 GT/s)
    Bus Bandwidth:                     31.5 GB/sec (Current: 15.8 GB/sec)
    RAMDAC Type:                       32-bit True Color
    Maximum Resolution:                1920x1080 16M Colors
    Maximum Colors:                    1920x1080 16M Colors
    VESA OEM String:                   NVIDIA
    VESA Version:                      3.0
    Vendor Name:                       NVIDIA Corporation
    Product Name:                      GPU Board Chip Rev   
    OEM Software Version:              148.4
  VESA Power Management
    VESA PM Version:                   1.0
    Standby:                           [X]
    Suspend:                           [X]
    Off:                               [X]
    Reduced On:                        [ ]
  PCI-E Capabilities
    PCI Express Version:               4.0
    Device/Port Type:                  Legacy PCI-E Endpoint
    Link Speed:                        16.0 GT/s (Current: 8.0 GT/s)
    Link Width:                        x16 (Current: x16)
    Bus Bandwidth:                     31.5 GB/sec (Current: 15.8 GB/sec)
    Link Port Number:                  0
    Physical Slot Number:              0
  VESA Modes
     Number | Mode  |Resolution|Colors| bpp| Features
     -------+-------+----------+------+----+----------
       101h | Graph |   640x480|   256|   8| Bank + LFB
       103h | Graph |   800x600|   256|   8| Bank + LFB
       105h | Graph |  1024x768|   256|   8| Bank + LFB
       107h | Graph | 1280x1024|   256|   8| Bank + LFB
       111h | Graph |   640x480|   64k|  16| Bank + LFB
       112h | Graph |   640x480|   16M|  32| Bank + LFB
       114h | Graph |   800x600|   64k|  16| Bank + LFB
       115h | Graph |   800x600|   16M|  32| Bank + LFB
       117h | Graph |  1024x768|   64k|  16| Bank + LFB
       118h | Graph |  1024x768|   16M|  32| Bank + LFB
       11Ah | Graph | 1280x1024|   64k|  16| Bank + LFB
       11Bh | Graph | 1280x1024|   16M|  32| Bank + LFB
       145h | Graph | 1600x1200|   256|   8| Bank + LFB
       146h | Graph | 1600x1200|   64k|  16| Bank + LFB
       14Ah | Graph | 1600x1200|   16M|  32| Bank + LFB
       171h | Graph |  1360x768|   16M|  32| Bank + LFB
       177h | Graph | 1920x1080|   16M|  32| Bank + LFB
                                       
                                [End of Report]                               
