Quick Navigation
| Background
| System Summary
| Motherboard
| Processor
| Chipset
| BIOS
| PCI/AGP Devices
| Memory Modules
| Memory (SMBIOS)
| Disk
| ATAPI
| Storage (ASPI)
| Drives
| Printers
| Slots (SMBIOS)
| Ports (SMBIOS)
| Monitor
| Video
Background
| Background
| Version | ASTRA - Advanced Sysinfo Tool 7.20
| Home Page | www.sysinfolab.com
| Report Date | Feb-03-2025
| Report Time | 8:48:05 AM
| OS Version | FreeDOS 7.10 rev.0 in HMA
| Registered To | Sysinfo Lab
| License Type | Professional for 1 computer
| Command Line | /RTJXHCE examples\astra.txt
System Summary
| Processor
| Processor | AMD Ryzen 5 5600 3500 MHz
| CPU Clock | 3500.0 MHz (35.0 x 100.0 MHz)
| Level 1 Cache | 6 x 32 kB + 6 x 32 kB (data+instr.)
| Level 2 Cache | 6 x 512 kB
| Level 3 Cache | 1 x 32 MB
| Motherboard
| System Name | Micro-Star International Co., Ltd. MS-7A38
| Board Model | Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
| BIOS Version | American Megatrends International, LLC. B.L0
| BIOS Version | AMI BIOS 08.00.10
| Chipset Name | AMD B450 (Promontory)
| Northbridge Vendor | Advanced Micro Devices (AMD)
| Northbridge | Starship/Matisse Root Complex
| Southbridge Vendor | Advanced Micro Devices (AMD)
| Southbridge | B450 Fusion Controller Hub (FCH)
| PCI Bus Version | 3.0
| PnP Version | Not Present
| DMI/SMBIOS Version | 2.8
| Memory
| Base Memory | 629 kB (582 kB free)
| Extended Memory | 16700340 kB (16308.93 MB)
| System Memory | 16310 MB
| Memory Module | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Memory Module | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Storage
| Disk Size | 953869 MB (931.51 GB)
| Disk Size | 953869 MB (931.51 GB)
| Disk Size | 953869 MB (931.51 GB)
| Disk Size | 238475 MB (232.89 GB)
| Monitor
| Monitor Vendor | AOC International (TPV Technology)
| Monitor Model | Q27G2G3 / Q27G2E / 27G2G4 / 27G2G8 / Q27G2G4 / Q27G2WG4 / 27G2G5 / U27P2G6B / 27V2G5 / 27B2 / 27B2G5 (27.0")
| Video Card
| Video Chip Vendor | NVIDIA Corporation
| Video Chip | GeForce RTX 3060 Ti LHR [GA104]
| VESA OEM String | NVIDIA
| Bus Type | PCI Express 4.0 x16
| Video Memory Size | 8 GB GDDR6
| Sound
| Sound Chip Vendor | NVIDIA Corporation
| Sound Chip | GA104 High Definition Audio Controller
| Audio Codec Name | NVidia GPU GA104 HDMI/DP
| Sound 2
| Sound Chip Vendor | Advanced Micro Devices (AMD)
| Sound Chip | Starship/Matisse HD Audio Controller
| Audio Codec Name | Realtek ALC892
| Operating System
| DOS Version | FreeDOS 7.10 rev.0 in HMA
| Network
| Network Chip Vendor | Realtek Semiconductor
| Network Chip | RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
| Ports
| Mouse Type | PS/2 (version 7.05)
| LPT Ports | LPT1 (0378h)
| COM Ports | COM1 (03F8h)
| Joystick | Not Present
Motherboard
| System
| System Vendor | Micro-Star International Co., Ltd.
| Product Name | MS-7A38
| Version | 8.0
| Serial Number | To be filled by O.E.M.
| UUID | 12983CA982A41496AAC82CF05DD2A722
| Wake-up Type | Power Switch
| SKU Number | To be filled by O.E.M.
| Family | To be filled by O.E.M.
| Motherboard
| Motherboard Vendor | Unknown (0001)
| Vendor URL | Unknown
| Board Model | Micro-Star International Co., Ltd. B450M PRO-VDH MAX (MS-7A38)
| Motherboard ID | BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
| Version | 8.0
| Serial Number | 07A3880_KB1E018736
| Asset Tag | To be filled by O.E.M.
| BIOS Version | American Megatrends International, LLC. B.L0
| BIOS Version | AMI BIOS 08.00.10
| BIOS Date | 10/26/2023
| Chipset Name | AMD B450 (Promontory)
| Northbridge Vendor | Advanced Micro Devices (AMD)
| Northbridge | Starship/Matisse Root Complex
| Southbridge Vendor | Advanced Micro Devices (AMD)
| Southbridge | B450 Fusion Controller Hub (FCH)
| Onboard Device 1
| Description | Broadcom 5762
| Device Type | Ethernet
| Status | Disabled
| Configuration Options
| To be filled by O.E.M.
| System Enclosure
| Manufacturer | Micro-Star International Co., Ltd.
| Type | Desktop
| Version | 8.0
| Serial Number | To be filled by O.E.M.
| Asset Tag | To be filled by O.E.M.
| Boot-up State | Safe
| Power Supply State | Safe
| Thermal State | Safe
| Security Status | None
| OEM-defined | 00000000h
| Height | 0.0 sm
| Power Cords | 1
| Contained Element | 0
CPU
| CPU
| Processor | AMD Ryzen 5 5600 3500 MHz
| Coprocessor | Internal
| CPU Clock | 3500.0 MHz
| Level 1 Cache | 6 x 32 kB + 6 x 32 kB (data+instr.)
| Level 2 Cache | 6 x 512 kB
| Level 3 Cache | 1 x 32 MB
| Code Name | Vermeer (Zen 3)
| Manufacturing Process | 7 nm
| FSB Clock | 100.0 MHz
| Multiplier | 35.0
| Expected Clock | 3500 MHz
| Overclocking Support | Unlocked Multiplier
| AMD Core Performance Boost | Supported (Enabled)
| Max Turbo Clock | 4450.0 MHz
| Processor Topology | Nodes: 1, CPU Complexes (CCX): 1, Cores: 6, Threads: 12
| Socket Type | Socket AM4
| Instruction Set | IA-32, AMD64, MMX, AMDMMX, SSE, SSE2, SSE3, SSSE3
| Instruction Set | SSE4.1, SSE4.2, SSE4A, AVX, AVX2, AES, FMA, SHA, AMD-V
| Maximum Temperature (Tjmax) | 95 øC (203 øF)
| Core Voltage | 1.125 V
| Infinity Fabric Clock (FCLK) | 1800.0 MHz
| Vendor | AuthenticAMD
| Processor Name | AMD Ryzen 5 5600 6-Core Processor
| Processor Type | Original OEM Processor
| CPUID | Family: 15, Model: 1, Stepping: 2
| Ext. Family/Model | Family: 10, Model: 2
| CPU Signature | 00A20F12h
| Number of Cores | 6
| Logical Cores Count | 12
| Core Stepping | VMR-B2
| OPN Code | 100-000000927, 100-100000927BOX
| Microcode Revision | A20120Eh
| SMU Firmware Version | 56.76.00
| Power Table Version | 380905h
| Max TDP | 65 Wattes
| Power Limit | 76 Wattes
| Thermal Design Current (TDC) | 60 Amps
| Electrical Design Current (EDC) | 90 Amps
| Transistor Count | 6240 million
| Die Size | 81 mm2 + I/O 122 mm2
| Launch Date | April, 2022
| Recommended Price (USD) | $199
| Hardware Monitoring
| Core Voltage | 1.138 V
| Core Voltage (SVI2 TFN) | 1.131 V
| SoC Voltage (SVI2 TFN) | 1.075 V
| Package Temperature | 58 øC (136 øF)
| CCD1 Temperature | 51 øC (124 øF)
| SoC Temperature | 46 øC (115 øF)
| L3 Cache Temperature | 46 øC (115 øF)
| Package Power | 44.9 Wattes
| Cores Power | 17.1 Wattes
| SoC Power | 13.7 Wattes
| VDDIO Mem Power | 11.2 Wattes
| VDD18 Power | 1.0 Wattes
| FSB Clock | 100.0 MHz
| Core 1
| Temperature Core | 56 øC (133 øF)
| Core Power | 5.2 Wattes
| Core Clock | 4450.0 MHz
| Multiplier | 44.5
| Instruction Set
| Floating-Point Unit On-Chip | Supported
| IA MMX Technology | Supported
| SSE Instruction Set | Supported
| SSE2 Instruction Set | Supported
| SSE3 Instruction Set | Supported
| Supplemental SSE3 Instruction Set | Supported
| SSE4.1 Instruction Set | Supported
| SSE4.2 Instruction Set | Supported
| Advanced Vector Extensions (AVX) | Supported
| Advanced Vector Extensions 2 (AVX2) | Supported
| AVX-512 Foundation Instructions | Not Supported
| AVX-512 Prefetch Instructions | Not Supported
| AVX-512 Exponential and Reciprocal | Not Supported
| AVX-512 Conflict Detection | Not Supported
| AVX-512 Byte and Word Instructions | Not Supported
| AVX-512 Doubleword and Quadword | Not Supported
| AVX-512 Vector Length Extensions | Not Supported
| AVX-512 Integer Fused Multiply-Add | Not Supported
| AVX-512 Vector Bit Manipulation | Not Supported
| AVX-512 QVNNI Instructions | Not Supported
| AVX-512 QFMA Instructions | Not Supported
| AVX-512 VBMI2 Instructions | Not Supported
| AVX-512 VNNI Instructions | Not Supported
| AVX-512 BITALG Instructions | Not Supported
| Galois Field NI/Affine Transformation | Not Supported
| VEX-encoded AES-NI (VAES) | Supported
| VEX-encoded PCLMUL (VPCL) | Supported
| PCOMMIT Instruction | Not Supported
| CLWB Instruction | Supported
| PREFETCHWT1 Instruction | Not Supported
| Software Guard Extensions (SGX) | Not Supported
| SGX Launch Configuration | Not Supported
| FMA Instructions Set | Supported
| AES Instructions Set | Supported
| Intel Extended Memory 64 Tech. | Not Supported
| Intel Architecture - 64 (IA-64) | Not Supported
| AMD MMX Instruction Extensions | Supported
| AMD 3DNow! Instructions | Not Supported
| AMD 3DNow! Extensions | Not Supported
| AMD 3DNow! Prefetch | Supported
| AMD SSE4A Extensions | Supported
| AMD eXtended OPeration (XOP) | Not Supported
| AMD Misaligned SSE | Supported
| AMD64 Architecture | Supported
| Cyrix Extended MMX | Not Supported
| CMPXCHG8 Instruction Supported | Supported
| CMPXCHG16 Instruction Supported | Supported
| Fast System Call | Supported
| Conditional Move Instruction | Supported
| CLFLUSH Insruction Supported | Supported
| Fast Save and Restore | Supported
| Monitor/MWAIT Instructions | Supported
| SYSCALL/SYSRET Instructions | Supported
| LAHF/SAHF Instructions | Supported
| POPCNT Insruction Supported | Supported
| XSAVE Insructions Supported | Supported
| OS Supports XSAVE Instructions | Not Supported
| PCLMULQDQ Instruction Supported | Supported
| MOVBE Insruction Supported | Supported
| F16C Insruction Supported | Supported
| RDTSCP Insruction Supported | Supported
| RDRAND Insruction Supported | Supported
| (RD/WR)(FS/GS) BASE Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Enhanced REP MOVSB/STOSB | Supported
| INVPCID Instruction | Supported
| XSAVEOPT Instruction | Supported
| RDSEED Instruction | Supported
| ADCX/ADOX Instructions | Supported
| CLAC/STAC Instructions | Supported
| SCLFLUSHOPT Instruction | Supported
| RDPID Instruction | Supported
| VPOPCNT[D/Q] Instructions | Not Supported
| Fast Short REP MOV Instruction | Supported
| PCONFIG Instruction | Not Supported
| WBNOINVD Instruction | Supported
| WaitPKG Instructions | Not Supported
| CLDEMOTE Instruction | Not Supported
| MOVDIRI Instruction | Not Supported
| MOVDIRI64B Instruction | Not Supported
| RDPRU Instruction | Supported
| MCOMMIT Instruction | Not Supported
| AMD Fast Save and Restore | Supported
| AMD SKINIT, STGI, DEV Supported | Supported
| AMD Light Weight Profiling (LWP) | Not Supported
| AMD FMA4 Insruction Supported | Not Supported
| AMD TBM Insruction Supported | Not Supported
| AMD MONITORX/MWAITX Instructions | Supported
| AMD CLZERO Instruction | Supported
| Processor Features
| Hypervisor Present | Not Supported
| Virtual Mode Extension | Supported
| Debugging Extension | Supported
| Page Size Extension | Supported
| Time Stamp Counter | Supported
| Model Specific Registers | Supported
| Physical Address Extension | Supported
| Machine Check Exception | Supported
| On-chip APIC Hardware Supported | Supported
| Memory Type Range Registers | Supported
| Page Global Enable | Supported
| Machine Check Architecture | Supported
| Page Attribute Table | Supported
| 36-bit Page Size Extension | Supported
| Processor Serial Number | Not Supported
| Debug Store | Not Supported
| 64-bit Debug Store | Not Supported
| Self-Snoop | Not Supported
| Hyper-Threading Technology | Supported
| Pending Break Enable | Not Supported
| CPL-Qualified Debug Store | Not Supported
| L1 Context ID | Not Supported
| Send Task Priority Messages | Not Supported
| Direct Cache Access | Not Supported
| Performance Capabilities MSR | Not Supported
| x2APIC Architecture | Supported
| Advanced Bit Manipulation | Supported
| OS Visible Workaround | Supported
| Instruction Based Sampling | Supported
| 1-GB Large Page | Supported
| Process Context Identifiers | Not Supported
| Time Stamp Counter Deadline | Not Supported
| Time Stamp Counter Adjust | Not Supported
| Intel Virtualization Technology | Not Supported
| Intel Trusted Execution Technology | Not Supported
| Supervisor Mode Execution Protection | Supported
| Hardware Lock Elision | Not Supported
| Restricted Transactional Memory | Not Supported
| Quality of Service Monitoring | Supported
| Quality of Service Enforcement | Supported
| Deprecated FPU CS and FPU DS | Not Supported
| Memory Protection Extensions (MPX) | Not Supported
| Processor Trace (PT) | Not Supported
| Secure Hash Algorithm Ext. (SHA) | Supported
| Debug Interface MSR | Not Supported
| User-Mode Instruction Prevention | Supported
| Protection Keys for User-Mode Pages | Supported, Disabled
| 5 Level Page Table | Not Supported
| Total Memory Encryption (TME) | Not Supported
| Speculation Control (IBRS and IBPB) | Not Supported
| Single Thread Indirect Branch Predictors | Not Supported
| L1 Data Cache (L1D) Flush | Not Supported
| ARCH_CAPABILITIES MSR | Not Supported
| Speculative Store Bypass Disable (SSBD) | Not Supported
| AMD Core Performance Boost | Supported, Enabled
| Intel Turbo Boost Max Technology 3.0 | Not Supported
| AMD No-execute Page Protection | Supported
| Hybrid Processor | Not Supported
| AMD Secure Virtual Machine | Supported
| AMD Model-Specific Registers | Supported
| AMD Multiprocessing Capable | Not Supported
| AMD CMP Legacy Mode | Supported
| AMD CR8 in Legacy Mode | Supported
| AMD Ext. APIC Register Space | Supported
| AMD Watchdog Timer | Supported
| AMD Translation Cache Extension | Supported
| AMD NodeID MSR | Not Supported
| AMD Topology Extensions | Supported
| AMD Core Performance Counter Ext. | Supported
| AMD NB Performance Counter Ext. | Supported
| AMD Streaming Performance Monitor | Not Supported
| AMD Data Breakpoint Extension | Supported
| AMD Performance TSC | Not Supported
| AMD L2I Performance Counter Ext. | Supported
| AMD IRPERF Performance Counter | Supported
| AMD Always Save/Restore FP Error Pointers | Supported
| AMD Indirect Branch Prediction Barrier | Supported
| AMD Indirect Branch Restricted Speculation | Supported
| AMD IBRS Always On Mode | Not Supported
| AMD IBRS Preferred | Supported
| AMD Single Thread Indirect Branch Predictor | Supported
| AMD STIBP Always On Mode | Supported
| AMD Speculative Store Bypass Disable (SSBD) | Supported
| AMD SSBD Not Needed | Not Supported
| AMD VIRT_SPEC_CTRL MSR | Not Supported
| Power Management
| ACPI Supported | Not Supported
| Thermal Monitor Supported | Not Supported
| Thermal Monitor 2 | Not Supported
| Enhanced SpeedStep Technology | Not Supported
| Digital Thermal Sensor | Not Supported
| Always Running APIC Timer | Supported
| Invariant TSC | Supported
| Power Limit Notification | Not Supported
| Extended Clock Modulation Duty | Not Supported
| Package Thermal Management | Not Supported
| Hardware Coordination Feedback | Supported
| ACNT2 Capability | Not Supported
| Performance-Energy Bias | Not Supported
| Hardware-Managed P-State Base Support | Not Supported
| Hardware Duty Cycle Programming (HDC) | Not Supported
| AMD Temperature Sensor | Supported
| AMD Frequency ID Control | Not Supported
| AMD Voltage ID Control | Not Supported
| AMD Thermal Trip | Supported
| AMD Thermal Monitoring | Supported
| AMD Software Thermal Control | Not Supported
| AMD 100MHz Multiplier Steps | Not Supported
| AMD Hardware P-State Control | Supported
| AMD Effective Frequency Interface | Supported
| AMD Processor Feedback Interface | Not Supported
| AMD Processor Accumulator | Not Supported
| AMD Connected Standby | Supported
| AMD Running Average Power Limit | Supported
| AMD MCA Overflow Recovery | Supported
| AMD Software Uncorr. Error Containment/Recovery | Supported
| AMD Hardware Assert (HWA) | Not Supported
| AMD Scalable MCA | Supported
CPU Cache
| Level 1 Data Cache
| Size | 6 x 32 kB
| Associativity | 8-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 64
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 64
| Associativity | full
| Level 1 Instruction Cache
| Size | 6 x 32 kB
| Associativity | 8-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 64
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 64
| Associativity | full
| Level 2 Cache
| Size | 6 x 512 kB
| Associativity | 8-way
| Lines per Tag | 1
| Line Size | 64 byte
| Data TLB 4K Pages |
| Number of Entries | 2048
| Associativity | 8-way
| Instr. TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Data TLB 2/4M Pages |
| Number of Entries | 2048
| Associativity | 4-way
| Instr. TLB 2/4M Pages |
| Number of Entries | 512
| Associativity | 2-way
| Level 3 Cache
| Size | 1 x 32 MB
| Associativity | 16-way
| Lines per Tag | 1
| Line Size | 64 byte
CPU (SMBIOS)
| Processor
| Processor Vendor | Advanced Micro Devices, Inc.
| Processor Version | AMD Ryzen 5 5600 6-Core Processor
| Current Speed | 3500 MHz
| External Clock | 100 MHz
| Voltage | 1.1 V
| Processor Upgrade | Socket AM4
| Processor Status | CPU Enabled
| Socket Designation | AM4
| Processor Type | Central Processor
| Processor Family | AMD Zen
| Processor ID1 | 00A20F12h
| Processor ID2 | 178BFBFFh
| Max Speed | 4450 MHz
| Socket Status | CPU Socket Populated
| Serial Number | Unknown
| Asset Tag | Unknown
| Part Number | Unknown
| CPU Core Count | 6 (Enabled: 6)
| CPU Thread Count | 12
| Structure Length | 30h
CPU (SMBIOS) Cache
| Level 1 Cache
| Installed Size | 384 kB
| Operational Mode | Write Back
| Current SRAM Type | Pipelined Burst
| Status | Enabled
| Socket Designation | L1 - Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 384 kB
| Supported SRAM Type | Pipelined Burst
| Cache Speed | 1 ns
| Error Correction | Multi-bit ECC
| System Cache Type | Unified
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 2 Cache
| Installed Size | 3 MB
| Operational Mode | Write Back
| Current SRAM Type | Pipelined Burst
| Status | Enabled
| Socket Designation | L2 - Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 3 MB
| Supported SRAM Type | Pipelined Burst
| Cache Speed | 1 ns
| Error Correction | Multi-bit ECC
| System Cache Type | Unified
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 3 Cache
| Installed Size | 32 MB
| Operational Mode | Write Back
| Current SRAM Type | Pipelined Burst
| Status | Enabled
| Socket Designation | L3 - Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 32 MB
| Supported SRAM Type | Pipelined Burst
| Cache Speed | 1 ns
| Error Correction | Multi-bit ECC
| System Cache Type | Unified
| Associativity | 16-way Set-Associative
| Structure Length | 13h
Chipset
| Chipset
| Chipset Name | AMD B450
| Code Name | Promontory
| Chipset Type | Single Chip: Southbridge-only
| Manufacturing Process | 55 nm
| Launch Date | March, 2018
| Northbridge
| Northbridge Vendor | Advanced Micro Devices (AMD)
| Northbridge | Starship/Matisse Root Complex
| Code Name | Vermeer (Zen 3)
| Location | CPU Integrated
| Infinity Fabric Clock (FCLK) | 1800.0 MHz
| Manufacturing Process | 7 nm
| Hardware ID | VEN_1022&DEV_1480
| Revision | 00h
| Stepping | VMR-B2
| Memory Controller
| Current Memory Type | DDR4-3600
| Supported Memory Types | DDR4-2667, DDR4-2933, DDR4-3200
| Maximum Memory Amount | 128 GB
| Current Controller Mode | Dual-channel (128-bit)
| Supported Controller Mode | Dual-channel (128-bit)
| Channel 0 DIMM A | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Channel 1 DIMM A | 8 GB DDR4-3602 (1801 MHz) SDRAM (Kingston)
| Current Memory Clock | 1800.0 MHz (Effective: 3600.0 MHz)
| FSB:DRAM Ratio | 1:18
| Memory Bandwidth | 56.3 GB/s
| Memory Controller Clock (UCLK) | 1800.0 MHz
| ECC | Supported, Disabled
| ECC Scrubbing | Not Supported
| Mirroring Mode (RAID) | Not Supported
| ECC Chipkill | Not Supported
| Timings
| CAS Latency (CL) | 16.0
| RAS to CAS Delay (tRCD) | 20
| RAS Precharge Time (tRP) | 20
| RAS Active Time (tRAS) | 39
| Row Cycle Time (tRC) | 83
| Row Refresh Cycle Time (tRFC) | 631
| Command Rate (CR) | 1T
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse GPP Bridge
| Bus Type | PCI Express 3.0 x4 8.0 GT/s (Current: x4 8.0 GT/s)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse GPP Bridge
| Bus Type | PCI Express 3.0 x8 8.0 GT/s (Current: x4 8.0 GT/s)
| Bus Bandwidth | 7.9 GB/sec (Current: 3.9 GB/sec)
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse GPP Bridge
| Bus Type | PCI Express 3.0 x16 8.0 GT/s (Current: x16 8.0 GT/s)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Bus Type | PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| PCI Express Controller
| PCI Express Controller | AMD Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Bus Type | PCI Express 4.0 x16 16.0 GT/s (Current: x16 16.0 GT/s)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| Southbridge
| Southbridge Vendor | Advanced Micro Devices (AMD)
| Southbridge | B450 Fusion Controller Hub (FCH)
| Bus Type | PCI Express
| Manufacturing Process | 55 nm
| Hardware ID | VEN_1022&DEV_790E
| Revision | 51h
| Top Marking | 218-0891011
| Package Type | LFBGA-583
| Integrated Sound
| Audio Controller | AMD Starship/Matisse HD Audio Controller
| Audio Codec Name | Realtek ALC892
| Controller Type | High Definition Audio
| Hardware ID | VEN_1022&DEV_1487
| Revision | 00h
| Integrated Storage
| Storage Controller | AMD 400 Series Chipset SATA Controller
| Controller Type | Serial ATA
| Hardware ID | VEN_1022&DEV_43C8
| Revision | 01h
BIOS
| BIOS
| BIOS Version | AMI BIOS 08.00.10
| BIOS Type | UEFI
| BIOS Model/SubModel/Revision | FCh/01h/00h
| BIOS Date | 12/24/18
| BIOS Copyright | 12/24/18(C)2010 American Megatrends, Inc. All Rights Reserved
| Motherboard ID | BIOS Date: 10/26/23 08:57:43 Ver: VB.L0
| BIOS ID | 63-0100-000001-00101111-122418-Chipset
| AMI BIOS Tag | 0AAAA000
| BIOS Size | 512 kB
| Processor | 686
| Chipset ID | Chipset
| BIOS Revision | 0100
| PnP Version | 1.0
| ACPI Version | 2.0+ (ALASKA)
| MCFG Address | F0000000h
| MP Specification Ver. | Not Supported
| DMI/SMBIOS Version | 2.8
| DMI/SMBIOS Structures | 62
| DMI/SMBIOS Address | 000Eh:6CF0h
| APM Version | Not Supported
| SMBIOS
| BIOS Vendor | American Megatrends International, LLC.
| BIOS Version | B.L0
| BIOS Date | 10/26/2023
| BIOS ROM Size | 16 MB
| System BIOS Version | 5.17
| Starting Segment | F000h
| Structure Length | 1Ah
| Bus Supported
| PCI is Supported | Supported
| AGP is Supported | Not Supported
| USB is Supported | Supported
| ISA is Supported | Not Supported
| VLBus is Supported | Not Supported
| MCA is Supported | Not Supported
| EISA is Supported | Not Supported
| PC Card is Supported | Not Supported
| Boot Options
| Selectable Boot | Supported
| Boot From CD | Supported
| ATAPI ZIP Drive Boot | Not Supported
| LS-120 Boot | Not Supported
| BIOS Boot Specification | Supported
| Boot From PC Card | Not Supported
| Network Service Boot Supported | Not Supported
| I2O Boot | Not Supported
| 1394 Boot | Not Supported
| BIOS Features
| BIOS Characteristics | Supported
| ACPI Supported | Not Supported
| PnP is Supported | Not Supported
| APM is Supported | Not Supported
| ESCD Support | Not Supported
| Enhanced Disk Drive (EDD) | Supported
| BIOS is Upgradeable (Flash) | Supported
| BIOS ROM is Socketed | Supported
| BIOS Shadowing is Allowed | Supported
| Smart Battery Supported | Not Supported
| Targeted Content Distribution | Supported
| UEFI Specification is Supported | Supported
| Virtual Machine | Not Supported
| Int 13h - 5.25"/360kB Floppy | Supported
| Int 13h - 5.25"/1.2MB Floppy | Supported
| Int 13h - 3.5"/720kB Floppy | Supported
| Int 13h - 3.5"/2.88MB Floppy | Supported
| Int 5h, Print Screen Service | Supported
| Int 9h, 8042 Keyboard Services | Supported
| Int 14h, Serial Services | Supported
| Int 17h, Printer Services | Supported
| Int 10h, CGA/Mono Video Services | Supported
| Int 13h - Floppy for NEC 9800 | Supported
| Int 13h - Floppy for Toshiba | Supported
| NEC PC-98 | Not Supported
| ROM Extension
| Adapter Vendor | Intel Corporation
| Adapter Name | Realtek PXE B25 D00
| BIOS Version | PXE-EC6: UNDI driver image is invalid.
| BIOS Copyright | Copyright (C) 1997-2000 Intel Corporation
| Device Class | Network
| ROM Address | CF80h
| BIOS ROM Size | 4 kB
| ROM Extension
| Device Name | NVIDIA GeForce RTX 3060 Ti LHR [GA104]
| BIOS Version | Version 94.04.46.00.D2
| BIOS Copyright | Copyright (C) 1996-2021 NVIDIA Corp.
| Device Class | Display
| ROM Address | C000h
| BIOS ROM Size | 61 kB
| OEM SMBIOS Strings
| To be filled by O.E.M.
| Other SMBIOS Structures
| System Boot Information (32)
| Unknown (44)
| TPM Device (43)
| 32-bit Memory Error Information (18)
| Memory Array Mapped Address (19)
| Memory Array Mapped Address (19)
| 32-bit Memory Error Information (18)
| 32-bit Memory Error Information (18)
| Memory Device Mapped Address (20)
| 32-bit Memory Error Information (18)
| 32-bit Memory Error Information (18)
| Memory Device Mapped Address (20)
| Unknown (143)
PCI/AGP Devices
| PCI/AGP
| PCI Bus Version | 3.0
| Number of PCI Buses | 128
| Bus: 00h, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1480h) | Starship/Matisse Root Complex
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1480
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 00h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1481h) | Starship/Matisse IOMMU
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (08h) | System Peripheral
| SubClass (06h) | IOMMU
| Hardware ID | VEN_1022&DEV_1481
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 01h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 01h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1483h) | Starship/Matisse GPP Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Base I/O Port | 00F00000h - 000FFFFFh
| Memory Address | FC800000h - FC8FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 1
| Physical Slot Number | 0
| Slot Power Limit | 75 Wattes
| Bus: 00h, Device: 01h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1483h) | Starship/Matisse GPP Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - FFFFh
| Memory Address | FC500000h - FC7FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x8 (Current: x4)
| Bus Bandwidth | 7.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Physical Slot Number | 0
| Slot Power Limit | 75 Wattes
| Bus: 00h, Device: 02h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 03h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 03h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1483h) | Starship/Matisse GPP Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1483
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | E000h - EFFFh
| Memory Address | FB000000h - FC0FFFFFh
| Memory Address | D0000000h - E1FFFFFFh
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 15.8 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Physical Slot Number | 0
| Slot Power Limit | 75 Wattes
| Bus: 00h, Device: 04h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 05h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 07h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 07h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1484h) | Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Base I/O Port | 00F00000h - 000FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Bus: 00h, Device: 08h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1482h) | Starship/Matisse PCIe Dummy Host Bridge
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1482
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 08h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1484h) | Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_1484
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Base I/O Port | 00F00000h - 000FFFFFh
| Memory Address | FC200000h - FC4FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Bus: 00h, Device: 14h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (790Bh) | Hudson SMBus Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (0Ch) | Serial
| SubClass (05h) | SMBus Controller
| Hardware ID | VEN_1022&DEV_790B
| Revision | 61h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Supported
| Device Resources
| SMBus Port | 0B00h
| Bus: 00h, Device: 14h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (790Eh) | B450 Fusion Controller Hub (FCH)
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (06h) | Bridge
| SubClass (01h) | PCI/ISA
| Hardware ID | VEN_1022&DEV_790E
| Revision | 51h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1440h) | Matisse/Vermeer Data Fabric: Device 18h; Function 0
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1440
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1441h) | Matisse/Vermeer Data Fabric: Device 18h; Function 1
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1441
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1442h) | Matisse/Vermeer Data Fabric: Device 18h; Function 2
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1442
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1443h) | Matisse/Vermeer Data Fabric: Device 18h; Function 3
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1443
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 04h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1444h) | Matisse/Vermeer Data Fabric: Device 18h; Function 4
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1444
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 05h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1445h) | Matisse/Vermeer Data Fabric: Device 18h; Function 5
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1445
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 06h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1446h) | Matisse/Vermeer Data Fabric: Device 18h; Function 6
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1446
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 07h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1447h) | Matisse/Vermeer Data Fabric: Device 18h; Function 7
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Hardware ID | VEN_1022&DEV_1447
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 01h, Device: 00h, Function: 00h
| Vendor (144Dh) | Samsung Electronics Co Ltd
| Device (A808h) | NVMe SSD Controller SM981/PM981/PM983
| Subsys Vendor (144Dh) | Samsung Electronics Co Ltd
| Subsystem ID (A801h) | SSD 970 EVO/PRO
| Class (01h) | Storage
| SubClass (08h) | Non-Volatile memory controller
| Hardware ID | VEN_144D&DEV_A808
| Revision | 00h
| Interface | 02h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC800000h - FC803FFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Bus: 03h, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43D5h) | 400 Series Chipset USB 3.1 xHCI Compliant Host Controller
| Subsys Vendor (1B21h) | ASMedia Technology Inc.
| Subsystem ID (1142h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Hardware ID | VEN_1022&DEV_43D5
| Revision | 01h
| Interface | 30h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC7A0000h - FC7A7FFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Bus: 03h, Device: 00h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C8h) | 400 Series Chipset SATA Controller
| Subsys Vendor (1B21h) | ASMedia Technology Inc.
| Subsystem ID (1062h) | Unknown
| Class (01h) | Storage
| SubClass (06h) | Serial ATA
| Hardware ID | VEN_1022&DEV_43C8
| Revision | 01h
| Interface | 01h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| ROM Address | FC700000h
| Memory Address | FC780000h - FC79FFFFh
| System IRQ | 10
| Interrupt Pin | INTB#
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Bus: 03h, Device: 00h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C6h) | 400 Series Chipset PCIe Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C6
| Revision | 01h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - FFFFh
| Memory Address | FC500000h - FC6FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 11
| Interrupt Pin | INTC#
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Upstream Port of PCI-E Switch
| Link Speed | 8.0 GT/s (Current: 8.0 GT/s)
| Link Width | x4 (Current: x4)
| Bus Bandwidth | 3.9 GB/sec (Current: 3.9 GB/sec)
| Link Port Number | 0
| Bus: 20h, Device: 04h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - FFFFh
| Memory Address | FC600000h - FC6FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 4
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Bus: 20h, Device: 05h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Base I/O Port | 00F00000h - 000FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 5
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Bus: 20h, Device: 06h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Base I/O Port | 00F00000h - 000FFFFFh
| Memory Address | FC500000h - FC5FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 5.0 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.5 GB/sec)
| Link Port Number | 6
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Bus: 20h, Device: 07h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (43C7h) | 400 Series Chipset PCIe Port
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Hardware ID | VEN_1022&DEV_43C7
| Revision | 01h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | F000h - 0FFFh
| Base I/O Port | 00F00000h - 000FFFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Downstream Port of PCI-E Switch
| Link Speed | 5.0 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 7
| Physical Slot Number | 1
| Slot Power Limit | 26 Wattes
| Bus: 25h, Device: 00h, Function: 00h
| Vendor (10ECh) | Realtek Semiconductor
| Device (8168h) | RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (02h) | Network
| SubClass (00h) | Ethernet
| Hardware ID | VEN_10EC&DEV_8168
| Revision | 15h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000F000h - 0000F0FFh
| Memory Address | FC604000h - FC604FFFh
| Memory Address | FC600000h - FC603FFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 1.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 2.5 GT/s (Current: 2.5 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.25 GB/sec (Current: 0.25 GB/sec)
| Link Port Number | 0
| Bus: 27h, Device: 00h, Function: 00h
| Vendor (1B21h) | ASMedia Technology Inc.
| Device (1142h) | ASM1042A USB 3.0 Host Controller
| Subsys Vendor (1043h) | ASUSTeK Computer Inc
| Subsystem ID (86A0h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Hardware ID | VEN_1B21&DEV_1142
| Revision | 00h
| Interface | 30h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC500000h - FC507FFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 5.0 GT/s (Current: 5.0 GT/s)
| Link Width | x1 (Current: x1)
| Bus Bandwidth | 0.5 GB/sec (Current: 0.5 GB/sec)
| Link Port Number | 1
| Bus: 29h, Device: 00h, Function: 00h
| Vendor (10DEh) | NVIDIA Corporation
| Device (2489h) | GeForce RTX 3060 Ti LHR [GA104]
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (3972h) | MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
| Class (03h) | Display
| SubClass (00h) | VGA
| Hardware ID | VEN_10DE&DEV_2489
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| ROM Address | FC000000h
| Memory Address | FB000000h - FBFFFFFFh
| Memory Address | D0000000h - DFFFFFFFh
| Memory Address | E0000000h - E1FFFFFFh
| Base I/O Port | 0000E000h - 0000E07Fh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Bus: 29h, Device: 00h, Function: 01h
| Vendor (10DEh) | NVIDIA Corporation
| Device (228Bh) | GA104 High Definition Audio Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (3972h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | High Definition Audio
| Hardware ID | VEN_10DE&DEV_228B
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC080000h - FC083FFFh
| System IRQ | 10
| Interrupt Pin | INTB#
| Sound
| Audio Codec Name | NVidia GPU GA104 HDMI/DP
| Controller Type | High Definition Audio
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Bus: 2Ah, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (148Ah) | Starship/Matisse PCIe Dummy Function
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (13h) | Non-Essential Instrumentation
| SubClass (00h) | Unknown
| Hardware ID | VEN_1022&DEV_148A
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Bus: 2Bh, Device: 00h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1485h) | Starship/Matisse Reserved SPP
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (13h) | Non-Essential Instrumentation
| SubClass (00h) | Unknown
| Hardware ID | VEN_1022&DEV_1485
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Bus: 2Bh, Device: 00h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1486h) | Starship/Matisse Cryptographic Coprocessor PSPCPP
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (10h) | En/Decryption
| SubClass (80h) | Other
| Hardware ID | VEN_1022&DEV_1486
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC300000h - FC3FFFFFh
| Memory Address | FC408000h - FC409FFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Bus: 2Bh, Device: 00h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (149Ch) | Matisse USB 3.0 Host Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (7A38h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Hardware ID | VEN_1022&DEV_149C
| Revision | 00h
| Interface | 30h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC200000h - FC2FFFFFh
| System IRQ | 10
| Interrupt Pin | INTC#
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
| Bus: 2Bh, Device: 00h, Function: 04h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1487h) | Starship/Matisse HD Audio Controller
| Subsys Vendor (1462h) | Micro-Star International Co Ltd (MSI)
| Subsystem ID (9A38h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | High Definition Audio
| Hardware ID | VEN_1022&DEV_1487
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FC400000h - FC407FFFh
| System IRQ | 10
| Interrupt Pin | INTD#
| Sound
| Audio Codec Name | Realtek ALC892
| Controller Type | High Definition Audio
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 16.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 31.5 GB/sec)
| Link Port Number | 0
Memory Modules
| Memory Slot 3
| Memory Type | 8 GB DDR4-3602 (1801 MHz) SDRAM
| Manufacturer | Kingston
| DRAM Manufacturer | SK Hynix
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 16 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| JEDEC Timings | CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
| JEDEC Profile @ 1200 MHz | 18.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1200 MHz | 17.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1163 MHz | 16.0-16-16-38-54-408-303-187
| JEDEC Profile @ 1090 MHz | 15.0-15-15-35-50-382-284-175
| JEDEC Profile @ 1018 MHz | 14.0-14-14-33-47-357-265-163
| JEDEC Profile @ 945 MHz | 13.0-13-13-31-44-331-246-152
| JEDEC Profile @ 872 MHz | 12.0-12-12-28-40-306-227-140
| JEDEC Profile @ 799 MHz | 11.0-11-11-26-37-280-208-128
| JEDEC Profile @ 727 MHz | 10.0-10-10-24-34-255-190-117
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.20 V
| SPD Revision | 1.1
| Part Number | KF3600C16D4/8GX
| Manufacturing Location | 7
| Manufacture Date | September 2023 (2338h)
| Serial Number | 211C9E38h
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Supported
| XMP Revision | 2.0
| XMP Profile 1
| Profile Name | XMP-3602 (1801 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1801 MHz | 18.0-20-20-39-85
| XMP Profile @ 1801 MHz | 17.0-20-20-39-85
| XMP Profile @ 1801 MHz | 16.0-20-20-39-85 (Active)
| XMP Profile @ 1689 MHz | 15.0-19-19-37-80
| XMP Profile @ 1576 MHz | 14.0-18-18-35-75
| XMP Profile @ 1463 MHz | 13.0-17-17-32-69
| XMP Profile @ 1351 MHz | 12.0-15-15-30-64
| XMP Profile @ 1238 MHz | 11.0-14-14-27-59
| XMP Profile @ 1126 MHz | 10.0-13-13-25-53
| XMP Profile 2
| Profile Name | XMP-2998 (1499 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1499 MHz | 17.0-17-17-36-64
| XMP Profile @ 1499 MHz | 16.0-17-17-36-64
| XMP Profile @ 1499 MHz | 15.0-17-17-36-64
| XMP Profile @ 1399 MHz | 14.0-16-16-34-60
| XMP Profile @ 1299 MHz | 13.0-15-15-32-56
| XMP Profile @ 1199 MHz | 12.0-14-14-29-52
| XMP Profile @ 1099 MHz | 11.0-13-13-27-47
| XMP Profile @ 899 MHz | 9.0-11-11-22-39
| Memory Slot 4
| Memory Type | 8 GB DDR4-3602 (1801 MHz) SDRAM
| Manufacturer | Kingston
| DRAM Manufacturer | SK Hynix
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 16 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| JEDEC Timings | CL-tRCD-tRP-tRAS-tRC-tRFC1-tRFC2-tRFC4
| JEDEC Profile @ 1200 MHz | 18.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1200 MHz | 17.0-17-17-39-55-421-313-193
| JEDEC Profile @ 1163 MHz | 16.0-16-16-38-54-408-303-187
| JEDEC Profile @ 1090 MHz | 15.0-15-15-35-50-382-284-175
| JEDEC Profile @ 1018 MHz | 14.0-14-14-33-47-357-265-163
| JEDEC Profile @ 945 MHz | 13.0-13-13-31-44-331-246-152
| JEDEC Profile @ 872 MHz | 12.0-12-12-28-40-306-227-140
| JEDEC Profile @ 799 MHz | 11.0-11-11-26-37-280-208-128
| JEDEC Profile @ 727 MHz | 10.0-10-10-24-34-255-190-117
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.20 V
| SPD Revision | 1.1
| Part Number | KF3600C16D4/8GX
| Manufacturing Location | 7
| Manufacture Date | November 2023 (2346h)
| Serial Number | 804C34DDh
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Supported
| XMP Revision | 2.0
| XMP Profile 1
| Profile Name | XMP-3602 (1801 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1801 MHz | 18.0-20-20-39-85
| XMP Profile @ 1801 MHz | 17.0-20-20-39-85
| XMP Profile @ 1801 MHz | 16.0-20-20-39-85 (Active)
| XMP Profile @ 1689 MHz | 15.0-19-19-37-80
| XMP Profile @ 1576 MHz | 14.0-18-18-35-75
| XMP Profile @ 1463 MHz | 13.0-17-17-32-69
| XMP Profile @ 1351 MHz | 12.0-15-15-30-64
| XMP Profile @ 1238 MHz | 11.0-14-14-27-59
| XMP Profile @ 1126 MHz | 10.0-13-13-25-53
| XMP Profile 2
| Profile Name | XMP-2998 (1499 MHz)
| Voltage Interface | 1.35 V
| XMP Timings | CL-tRCD-tRP-tRAS-tRC
| XMP Profile @ 1499 MHz | 17.0-17-17-36-64
| XMP Profile @ 1499 MHz | 16.0-17-17-36-64
| XMP Profile @ 1499 MHz | 15.0-17-17-36-64
| XMP Profile @ 1399 MHz | 14.0-16-16-34-60
| XMP Profile @ 1299 MHz | 13.0-15-15-32-56
| XMP Profile @ 1199 MHz | 12.0-14-14-29-52
| XMP Profile @ 1099 MHz | 11.0-13-13-27-47
| XMP Profile @ 899 MHz | 9.0-11-11-22-39
Memory (SMBIOS)
| Physical Memory Array 1
| Maximum Capacity | 131072 MB
| Location | System Board or Motherboard
| Use | System Memory
| Memory Error Correct. | None
| Memory Devices | 4
| Structure Length | 17h
| Memory Device 1
| Size | Not Installed
| Form Factor | Unknown
| Memory Type | Unknown
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | Unknown
| Maximum Voltage | Unknown
| Minimum Voltage | Unknown
| Device Locator | DIMM 0
| Bank Locator | P0 CHANNEL A
| Total Width | Unknown
| Data Width | Unknown
| Device Set | 00h
| Type Detail | Unknown
| Manufacturer | Unknown
| Serial Number | Unknown
| Asset Tag |
| Part Number | Unknown
| Structure Length | 28h
| Memory Device 2
| Size | 8192 MB
| Form Factor | DIMM
| Memory Type | DDR4
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | 1.2 V
| Maximum Voltage | 1.2 V
| Minimum Voltage | 1.2 V
| Device Locator | DIMM 1
| Bank Locator | P0 CHANNEL A
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous, Unbuffered (Unregistered)
| Manufacturer | Kingston
| Serial Number | 211C9E38
| Asset Tag |
| Part Number | KF3600C16D4/8GX
| Structure Length | 28h
| Memory Device 3
| Size | Not Installed
| Form Factor | Unknown
| Memory Type | Unknown
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | Unknown
| Maximum Voltage | Unknown
| Minimum Voltage | Unknown
| Device Locator | DIMM 0
| Bank Locator | P0 CHANNEL B
| Total Width | Unknown
| Data Width | Unknown
| Device Set | 00h
| Type Detail | Unknown
| Manufacturer | Unknown
| Serial Number | Unknown
| Asset Tag |
| Part Number | Unknown
| Structure Length | 28h
| Memory Device 4
| Size | 8192 MB
| Form Factor | DIMM
| Memory Type | DDR4
| Speed | 3600 MHz
| Configured Speed | 3600 MHz
| Configured Voltage | 1.2 V
| Maximum Voltage | 1.2 V
| Minimum Voltage | 1.2 V
| Device Locator | DIMM 1
| Bank Locator | P0 CHANNEL B
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous, Unbuffered (Unregistered)
| Manufacturer | Kingston
| Serial Number | 804C34DD
| Asset Tag |
| Part Number | KF3600C16D4/8GX
| Structure Length | 28h
Disk
| ATA/ATAPI drives not found
Storage (ASPI)
| ASPI manager not found
Drives
| BIOS Drives
| INT 13h Extensions | 3.0
| C:
| Drive Letter | C:
| Drive Size | 931.51 GB
| Drive Type | Fixed Disk
| Cylinders | 121601
| Heads | 255
| Sectors | 63
| D:
| Drive Letter | D:
| Drive Size | 931.51 GB
| Drive Type | Fixed Disk
| Cylinders | 121601
| Heads | 255
| Sectors | 63
| E:
| Drive Letter | E:
| Drive Size | 931.51 GB
| Drive Type | Fixed Disk
| Cylinders | 121601
| Heads | 255
| Sectors | 63
| F:
| Drive Letter | F:
| Drive Size | 232.89 GB
| Drive Type | Fixed Disk
| Cylinders | 30401
| Heads | 255
| Sectors | 63
| Local Drives
| C:[SYSTEM]
| Drive Letter | C:
| Drive Type | Fixed Disk
| Volume Label | SYSTEM
| File System | FAT16
| Volume Serial Number | 0805-FB80
| Total Size | 1.99 GB
| Free Space | 747.47 MB (36.6%)
| D:[UTILITIES]
| Drive Letter | D:
| Drive Type | Fixed Disk
| Volume Label | UTILITIES
| File System | FAT32
| Volume Serial Number | 089E-9200
| Total Size | 29.99 GB
| Free Space | 8.74 GB (29.2%)
Physical Printers
| LPT/PnP or USB printer not found
Slots (SMBIOS)
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J6B2
| Slot Length | Long Length
| Slot ID | 0
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J6B1
| Slot Length | Short Length
| Slot ID | 1
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J6D1
| Slot Length | Short Length
| Slot ID | 2
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J7B1
| Slot Length | Short Length
| Slot ID | 3
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J8B4
| Slot Length | Short Length
| Slot ID | 4
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J8D1
| Slot Length | Short Length
| Slot ID | 5
| Slot PCI
| Slot Type | PCI
| Current Usage | In Use
| Data Bus Width | 32 bit
| Slot Designation | J8B3
| Slot Length | Short Length
| Slot ID | 6
| Slot PCI Express x16
| Slot Type | PCI Express x16
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J10
| Slot Length | Short Length
| Slot ID | 12
| Slot PCI Express x8
| Slot Type | PCI Express x8
| Current Usage | Available
| Data Bus Width | 8x or x8
| Slot Designation | J3600 Pcie x8 slot
| Slot Length | Short Length
| Slot ID | 13
| Slot PCI Express x4
| Slot Type | PCI Express x4
| Current Usage | Other
| Data Bus Width | 4x or x4
| Slot Designation | J3707 Pcie x4 slot
| Slot Length | Short Length
| Slot ID | 32
| Slot PCI Express x4
| Slot Type | PCI Express x4
| Current Usage | In Use
| Data Bus Width | 4x or x4
| Slot Designation | J3700 PCIE x4 slot from Promontory
| Slot Length | Short Length
| Slot ID | 2
| Slot PCI Express x1
| Slot Type | PCI Express x1
| Current Usage | Available
| Data Bus Width | 1x or x1
| Slot Designation | J3702 PCIE x1 slot from Promontory
| Slot Length | Short Length
| Slot ID | 3
| Slot PCI Express x1
| Slot Type | PCI Express x1
| Current Usage | Available
| Data Bus Width | 1x or x1
| Slot Designation | J3703 PCIE x1 slot from Promontory
| Slot Length | Short Length
| Slot ID | 4
| Slot PCI Express x1
| Slot Type | PCI Express x1
| Current Usage | Available
| Data Bus Width | 1x or x1
| Slot Designation | J3701 M.2 WLAN/BT slot
| Slot Length | Short Length
| Slot ID | 5
Ports (SMBIOS)
| Port 1 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1500
| Ext. Designator | USB 3.0
| Port 2 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1501
| Ext. Designator | USB 3.0
| Port 3 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1502
| Ext. Designator | USB-C
| Port 4 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1503
| Ext. Designator | USB 3.0
| Port 5 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J1504
| Ext. Designator | USB 3.1
| Port 6 Network Port
| Int. Connector Type | None
| Ext. Connector Type | RJ-45
| Port Type | Network Port
| Int. Designator | J1503
| Ext. Designator | Network
| Port 7 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1704
| Ext. Designator | Sata Express
| Port 8 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1705
| Ext. Designator | Sata Express
| Port 9 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1701
| Ext. Designator | iSATA
| Port 10 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1702
| Ext. Designator | iSATA
| Port 11 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1703
| Ext. Designator | iSATA
| Port 12 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1706
| Ext. Designator | iSATA
| Port 13 Video Port
| Int. Connector Type | None
| Ext. Connector Type | None
| Port Type | Video Port
| Int. Designator | J1100
| Ext. Designator | HDMI
| Port 14 Video Port
| Int. Connector Type | None
| Ext. Connector Type | None
| Port Type | Video Port
| Int. Designator | J1101
| Ext. Designator | HDMI
| Port 15 Video Port
| Int. Connector Type | None
| Ext. Connector Type | None
| Port Type | Video Port
| Int. Designator | J1102
| Ext. Designator | DP
| Port 16 Audio Port
| Int. Connector Type | None
| Ext. Connector Type | Mini-jack (headphones)
| Port Type | Audio Port
| Int. Designator | J2100
| Ext. Designator | Front Audio
| Port 17 Audio Port
| Int. Connector Type | None
| Ext. Connector Type | Mini-jack (headphones)
| Port Type | Audio Port
| Int. Designator | J2101
| Ext. Designator | Audio Jack
| Port 18 SATA
| Int. Connector Type | SAS/SATA Plug Receptacle
| Ext. Connector Type | None
| Port Type | SATA
| Int. Designator | J1700
| Ext. Designator | Sata Express
Sound
| Sound
| Sound Chip Vendor | NVIDIA Corporation
| Sound Chip | GA104 High Definition Audio Controller
| Audio Codec Name | NVidia GPU GA104 HDMI/DP
| Hardware ID | VEN_10DE&DEV_228B
| Revision | A1h
| Bus Type | PCI
| Sound 2
| Sound Chip Vendor | Advanced Micro Devices (AMD)
| Sound Chip | Starship/Matisse HD Audio Controller
| Audio Codec Name | Realtek ALC892
| Hardware ID | VEN_1022&DEV_1487
| Revision | 00h
| Bus Type | PCI
Monitor
| Monitor
| Monitor Vendor | AOC International (TPV Technology)
| Monitor Model | Q27G2G3 / Q27G2E / 27G2G4 / 27G2G8 / Q27G2G4 / Q27G2WG4 / 27G2G5 / U27P2G6B / 27V2G5 / 27B2 / 27B2G5
| Viewable Size | 27.0" (68.5 sm)
| Serial Number | 7393
| Manufacture Date | October 2023
| EDID Version | 1.4
| Monitor ID | AOC2702
| Aspect Ratio | 16:9
| Horizontal Size | 597 mm
| Vertical Size | 336 mm
| Gamma Factor | 2.200
| Display Type | RGB Color
| Input Signal | Digital
| Internal Model | Q27G2SG4
| Internal Number | XFXPAHA007393
| Vertical Frequency | 48-155 Hz
| Horizontal Frequency | 230-230 kHz
| DPMS Features
| Active Off | Supported
| Suspend | Not Supported
| Standby | Not Supported
| Supported Modes
| Mode 1 | 640x480 @ 60 Hz (VGA)
| Mode 2 | 640x480 @ 67 Hz (Mac II)
| Mode 3 | 640x480 @ 72 Hz (VESA)
| Mode 4 | 640x480 @ 75 Hz (VESA)
| Mode 5 | 640x480 @ 100 Hz
| Mode 6 | 640x480 @ 120 Hz
| Mode 7 | 720x400 @ 70 Hz (VGA)
| Mode 8 | 800x600 @ 56 Hz (VESA)
| Mode 9 | 800x600 @ 60 Hz (VESA)
| Mode 10 | 800x600 @ 72 Hz (VESA)
| Mode 11 | 800x600 @ 75 Hz (VESA)
| Mode 12 | 800x600 @ 100 Hz
| Mode 13 | 800x600 @ 120 Hz
| Mode 14 | 832x624 @ 75 Hz (Mac II)
| Mode 15 | 1024x768 @ 60 Hz (VESA)
| Mode 16 | 1024x768 @ 70 Hz (VESA)
| Mode 17 | 1024x768 @ 75 Hz (VESA)
| Mode 18 | 1024x768 @ 100 Hz
| Mode 19 | 1024x768 @ 120 Hz
| Mode 20 | 1280x1024 @ 60 Hz
| Mode 21 | 1280x1024 @ 75 Hz (VESA)
| Mode 22 | 1920x1080 @ 60 Hz
| Mode 23 | 2560x1440 @ 60 Hz (Recommended)
Video Card
| Video
| Video Chip Vendor | NVIDIA Corporation
| Video Chip | GeForce RTX 3060 Ti LHR [GA104]
| Subsystem Vendor | Micro-Star International Co Ltd (MSI)
| Subsystem ID | MSI GeForce RTX 3060 Ti VENTUS 3X 8G OC LHR
| Hardware ID | VEN_10DE&DEV_2489
| Revision | A1h
| Memory
| Video Memory Size | 8 GB
| Memory Type | GDDR6
| Bus Width | 256-bit
| Architecture
| Architecture | Ampere
| Code Name | GA104 A1h
| GPU Variant | GA104-202
| Unified Shaders | 4864
| Texture Mapping Units (TPU) | 152
| Render Output Units (ROPS) | 80
| Streaming Multiprocessors | 38
| Tensor Cores | 152
| RT Cores | 38
| Level 1 Cache | 4.75 MB
| Level 2 Cache | 4 MB
| GPU Manufacturer | Samsung
| Manufacturing Process | 8 nm
| Transistor Count | 17400 million
| Die Size | 392 mm2
| Package Type | BGA-2713
| Max TDP | 200.0 Wattes
| Launch Date | May, 2021
| Theoretical Performance
| Estimated Speed | 35% of GeForce GTX 4090
| BIOS
| Bootup Message | PG190 SKU 12 VGA BIOS MSINV397MH.520
| Video BIOS Version | Version 94.04.46.00.D2
| Video BIOS Date | 05/19/21
| BIOS Copyright | Copyright (C) 1996-2021 NVIDIA Corp.
| Board Model | GPU Board
| API Supported
| DirectX Version | 12 (12_2)
| OpenGL Version | 4.6
| Shader Model | 6.7
| Vulkan Version | 1.3
| CUDA Version | 8.6
| OpenCL Version | 3.0
| Other
| Bus Type | PCI Express 4.0 x16 16.0 GT/s (Current: x16 8.0 GT/s)
| Bus Bandwidth | 31.5 GB/sec (Current: 15.8 GB/sec)
| RAMDAC Type | 32-bit True Color
| Maximum Resolution | 1920x1080 16M Colors
| Maximum Colors | 1920x1080 16M Colors
| VESA OEM String | NVIDIA
| VESA Version | 3.0
| Vendor Name | NVIDIA Corporation
| Product Name | GPU Board Chip Rev
| OEM Software Version | 148.4
| VESA Power Management
| VESA PM Version | 1.0
| Standby | Supported
| Suspend | Supported
| Off | Supported
| Reduced On | Not Supported
| PCI-E Capabilities
| PCI Express Version | 4.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 16.0 GT/s (Current: 8.0 GT/s)
| Link Width | x16 (Current: x16)
| Bus Bandwidth | 31.5 GB/sec (Current: 15.8 GB/sec)
| Link Port Number | 0
| Physical Slot Number | 0
| VESA Modes
| Number | Mode | Resolution | Colors | bpp | Features
| 101h | Graph | 640x480 | 256 | 8 | Bank + LFB
| 103h | Graph | 800x600 | 256 | 8 | Bank + LFB
| 105h | Graph | 1024x768 | 256 | 8 | Bank + LFB
| 107h | Graph | 1280x1024 | 256 | 8 | Bank + LFB
| 111h | Graph | 640x480 | 64k | 16 | Bank + LFB
| 112h | Graph | 640x480 | 16M | 32 | Bank + LFB
| 114h | Graph | 800x600 | 64k | 16 | Bank + LFB
| 115h | Graph | 800x600 | 16M | 32 | Bank + LFB
| 117h | Graph | 1024x768 | 64k | 16 | Bank + LFB
| 118h | Graph | 1024x768 | 16M | 32 | Bank + LFB
| 11Ah | Graph | 1280x1024 | 64k | 16 | Bank + LFB
| 11Bh | Graph | 1280x1024 | 16M | 32 | Bank + LFB
| 145h | Graph | 1600x1200 | 256 | 8 | Bank + LFB
| 146h | Graph | 1600x1200 | 64k | 16 | Bank + LFB
| 14Ah | Graph | 1600x1200 | 16M | 32 | Bank + LFB
| 171h | Graph | 1360x768 | 16M | 32 | Bank + LFB
| 177h | Graph | 1920x1080 | 16M | 32 | Bank + LFB