Last update 08-Aug-2000

# MBSE BBS Setup - TTY Lines.

### Introduction.

For each line your bbs has you must setup a tty line. This also includes console lines (for local login), network lines for internet, lan connections and X-terminal connections, ISDN lines, and Analogue modem lines. If a call comes in over a tty you didn't define, that call is refused. So if you are directly connected to the internet, and have only 5 network tty's defined, then maximum 5 users are allowed to telnet your bbs via the internet.

One thing about the portspeed, this is only needed for devices connected to serial ports such as modems and external ISDN adapters. For network tty's and internal ISDN cards this should be set to zero. If you set it to some value, things still wordk but you will get error messages in the logs.

### Setup a line.

    Comment      A description for this line.
    TTY device   The tty device name without /dev/
    Phone nr.    The phone number on this line.
    Line Speed   The maximum line speed for this line.
    Fido Flags   The EMSI flags for this line, include your modem flags here!
    Line Type    Can be POTS, ISDN, Network and Local.
    Available    Is this line available for use.
    Auth. log    Not in use yet.
    Honor ZMH    Deny users during ZMH on this line.
    Deleted      If this line must be deleted.
    Callout      Allow calling other systems from this line.
    Portspeed    The "locked" modemspeed, 0 to 4000000 baud, only for serial ports.
    Modemtype    The modem connected to this line.
    EMSI name    The EMSI name presented for this (modem) line.

### Some examples.

Back to index
Back to main index