    Document: FTS-0008
    Version:  003
    Date:     15-Oct-1990
    Updates:  FTS-0001

                      An Enhanced FidoNet(r) Technical Standard
                     Extending FTS-0001 to include Bark requests

                                October 15, 1990

    Status of this document:

        This document specifies an optional standard for the FidoNet community.
        Implementation of the protocols defined in this document is not mandatory,
        but all implementations of these protocols are expected to adhere to this
        standard.  Distribution of this document is subject to the limitations of
        the copyright notice displayed below.

        Copyright 1989-90 by Philip L. Becker.  Portions of this document are
        copyright 1986-90 by Randy Bush and are incorporated with his consent.
        All rights reserved.  A right to distribute only without modification and
        only at no charge is granted.  Under no circumstances is this document to
        be reproduced or distributed as part of or packaged with any product or
        other sales transaction for which any fee is charged.  Any and all other
        reproduction or excerpting requires the explicit written consent of the
        copyright holders.

     A. Introduction

     1. This Document

        This document describes the standard for "Bark" type FidoNet file
        request operation.  Bark file requests are an extension to the basic
        FTS-0001 mail session, and this document presents these requests as a
        modification to that document.

     2. What are File Requests?

        File Requests are a way of requesting that a specific file be sent during
        a FidoNet mail session.  This has many advantages over simply logging on to
        a BBS and downloading a file:

           o  You need not be a validated user

           o  You don't have to spend time searching for the file on the BBS

           o  You can schedule the file request to take place at any time without
              your being near your computer.

        There are two commonly used types of file requests on FidoNet today, WaZOO
        and Bark requests.  WaZOO requests are used by Opus and BinkleyTerm, and
        are not documented here.  See the document FTS-0006 by V. Perriello for a
        description of these.   Bark requests were the first file request extension
        to the FTS-0001 protocol, and are supported (at least partially) by many
        mailers, including SEAdog, Dutchie, BinkleyTerm, and to a certain extent
        Opus.  This document describes how to implement Bark-type file requests.

     B. Terms Used in this Document

     1. The diagrams and notations used in this document are the same as those used
        in the FTS-0001 document.  Please see FTS-0001 for a description of these.
        This document should be considered as an extension to the FTS-0001 session
        layer protocol, and you will require FTS-0001 in addition to this document
        to fully understand what is presented here.

        In addition to the data description language described in FTS-0001 section
        A.4, one extra terminal used in this notation:

        (* terminals *)
        someName - String of up to max chars, NOT null terminated
     C. Performing File Requests

     1. Introduction

        A Bark request consists of transmitting a special Bark Request packet which
        contains a filename, a date (used for update requests), and optionally a
        password.  The system receiving the request then decides if it can send the
        requested file or not, and if it can does so using the same protocol used
        to send attached files.  Bark request handling is always controlled by the
        answering system, and consists of two phases.  In phase one, the receiving
        system asks the calling system to honor requests it may have to ask for
        files from the caller.  In phase two, the receiving system allows the
        calling system to request files from it.

        Update file requests are the same as normal file requests, with one
        exception.  If the date in the Bark Request packet (described below) is
        greater than or equal to the date of the actual file requested, the file
        will not be sent.  The requestor should set the date to the date of the
        the actual file on its own end if an update request is desired.

     D. The Bark Request Packet

     1. Data Link Layer Data Definition.

        The Bark Request packet is a variable-sized packet containing a header, a
        filename, a date (which is used only for update requests - in a normal file
        request it's 0) and an optional password. When receiving a Bark Request
        packet, the ETX may be used to determine the end of the data portion. Note
        that the CRC is sent in the reverse byte order of a normal CRC XMODEM data
        block (see FTS-0001 section G.1).

        Note: some systems will send a password in the data block even if none is
        needed.  Incoming passwords should be ignored unless the other system is
        trying to request a passworded file.

                              Bark File Request Packet
          Offset
          dec hex
                  .-----------------------------------------------.
            0   0 |       ACK - Start of Bark Request - 06H       |
                  +-----------------------------------------------+
            1   1 |     Filename - Packed DOS file format         |
                  +-----------------------------------------------+
            n   n |              SPACE - 20H                      |
                  +-----------------------------------------------+
            n   n |              Date (0 if not Update Request)   |
                  +-----------------------------------------------+
            n   n |      SPACE - 20H  (only if pswd follows)      |
                  +-----------------------------------------------+
            n   n |         Password (optional)                   |
                  +-----------------------------------------------+
            n   n |       ETX -  End of RESYNC packet  - 03H      |
                  +-----------------------------------------------+
            n   n |     (*1)     CRC  low order byte              |
                  +-----------------------------------------------+
            n   n |     (*1)     CRC high order byte              |
                  `-----------------------------------------------'

                  *1 - CRC does not include the ACK or ETX and is
                       in the reverse byte order from the CRC in a
                       normal XMODEM data packet.
     2. Data Description Notation of Bark Request Packet

        DataBlock (no password) = ACK
                                  Filename<12>
                                  Space
                                  Date<11>
                                  ETX
                                  CRC

        DataBlock (with password) = ACK
                                    Filename<12>
                                    Space
                                    Date<11>
                                    Space
                                    Password<6|8>
                                    ETX
                                    CRC

        ACK   = 06H       (* Header for file request block *)
        Space = 20H       (* Space character *)
        ETX   = 03H       (* End of block *)

        Filename          (* Name of file requested *)
        Date              (* ASCII string; the number of seconds
                             since midnight, January 1, 1970 *)
        Password          (* The password needed to request this
                             file, if any.  Maximum length is 6 for
                             BinkleyTerm and Opus, 8 for SEAdog
                             and Dutchie. *)

        CRC = crc[2]      (* CCITT Cyclic Redundancy Check.  The
                             same algorithm as used for XModem
                             CRCs.  The CRC is calculated on
                             all data in the block between but
                             not including the ACK and the ETX *)
     E. Session Layer Protocol:

        This section describes the modified FTS-0001 session layer protocol.  This
        is the only area of FTS-0001 which is modified to implement Bark style file
        requests.  File Requests are performed at the end of the normal FidoNet
        mail session, after any mail pickup is performed.

        The diagrams below desribe the session level protocol with Bark file
        requests implemented.  The state tables have been broken into subroutines
        but the FTS-0001 portion is not functionally changed.  FTS-0001 sender
        states S4 through S7 are now table "Send Mail SM0".  FTS-0001 receiver
        states R3 through R6 are now table "Receive Mail RM0".  They are not
        functionally changed in any way from FTS-0001, they are just broken out
        to allow them to be used as subroutines.  Finally Sender states S0 through
        S3 are unchanged, as are Receiver states R0 through R2.

        The remaining FTS-0001 states are enhanced to implement the Bark file
        request protocol. In addition, the subroutine state tables "Send Bark SB0"
        and "Receive Bark RB0" have been added to handle the actual file requests.

        The following diagrams fully replace the Session Layer protocol state
        tables in FTS-0001.  No other changes to FTS-0001 are required to implement
        the Bark File request feature.
        Sender  (Top level)

        .-----+----------+-------------------------+-------------------------+-----.
        |State| State    | Predicate(s)            | Action(s)               | Next|
        |  #  | Name     |                         |                         | St  |
        +-----+----------+-------------------------+-------------------------+-----+
        | S0  | SendInit |                         | dial modem              | S1  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | S1  | WaitCxD  |1| carrier detected      | delay 1-5 seconds       | S2  |
        |     |  (*1)    | |                       | Set SLO if > 2400bps,   |     |
        |     |          | |                       | Reset SLO if <= 2400bps |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| busy, etc.            | report no connection    | exit|
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| voice                 | report no carrier       | exit|
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |4| carrier not detected  | report no connection    | exit|
        |     |          | | within 60 seconds     |                         |     |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | S2  | WhackCRs |1| over 30 seconds       | report no response  | exit|
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| ?? s received     | delay 1 sec             | S3  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| s not received    | send    | S2  |
        |     |          | |                       |   delay ??? secs        |     |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | S3  | WaitClear|1| no input for 0.5 secs | send TSYNCH = AEH       | S4  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| over 60 seconds       | hang up, report garbage | exit|
        |     |          | | and line not clear    |                         |     |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | S4  | SendMail |                         | (Send Mail SM0)         | S5  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | S5  | TryPickup|1| Rcv TSYNC             | (Receive Mail RM0)      | S5  |
        |     |   (*2)   +-+-----------------------+-------------------------+-----+
        |     |          |2| Rcv SYN               | (Receive Bark Req RB0)  | S5  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| Rcv ENQ               | (Do Bark Requests SB0)  | S5  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |4| Rcv 'C' or NAK        | Send EOT                | S5  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |5| Rcv Other Char        | Send SUB                | S5  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |6| No Data for 45 secs   | Hang Up                 | exit|
        `-----+----------+-+-----------------------+-------------------------+-----'

        *1 - This state is shown for the extended SEAlink protocol.  Omit the
             set/reset SLO actions if adding Bark to a strict FTS-0001 protocol
             implementation, or if not implementing overdrive in SEAdog.

        *2 - To refuse to pickup mail (S5.1) may send a CAN and stay in (S5).

        Note: Although the above shows the sender emitting only one TSYNCH, it is
        recommended that a timeout of 5-20 seconds should initiate another TSYNCH.
        The receiver should tolerate multiple TSYNCHs.
        Receiver (Top Level)

        The  receiving FSM is given  an external timer, the expiration of  which
        will cause termination with a result of 'no calls' (R0.2).
        .-----+----------+-------------------------+-------------------------+-----.
        |State| State    | Predicate(s)            | Action(s)               | Next|
        |  #  | Name     |                         |                         | St  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R0  | WaitCxD  |1| carrier detected      |                         | R1  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| external timer expires| report no calls         | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R1  | WaitBaud |1| baud rate detected    | send signon with s  | R2  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| no detect in ?? secs  | hang up, report no baud | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R2  | WaitTsync|1| TSYNCH received       | ignore input not TSYNCH | R3  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| 60 seconds timeout    | hang up, report not Fido| exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R3  | RecMail  |                         | (Receive Mail RM0)      | R4  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R4  | AllowPkup|1| Have pickup for sender| Send Tsync,             | R5  |
        |     |          | |                       |   Set T1=1 sec          |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| No pickup for sender  |                         | R6  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R5  | WtPickup |1| Rcv NAK or 'C'        | (Send Mail SM0)         | R6  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Rcv SUB               | Send Tsync,             | R5  |
        |     |          | |                       |   Set T1=1 sec          |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| Rcv CAN               | Report Mail Refused     | R6  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |4| T1 expired            | Send Tsync,             | R5  |
        |     |          | |                       |   Set T1=1 sec          |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |5| 45 secs in R5         | Hang Up, report error   | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R6  | AskBark  |1| Wish to make requests | Send SYN                | R7  |
        |     |   (*1)   +-+-----------------------+-------------------------+-----+
        |     |          |2| No requests to make   |                         | R8  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R7  | DoRequest|1| Rcv CAN               | Report Requests Refused | R8  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Rcv ENQ               | (Send Bark SB0)         | R8  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| Rcv SUB               | Send SYN                | R7  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |4| Rcv NAK or 'C'        | Send EOT                | R6  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |5| Rcv Other             | eat character           | R7  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |6| 5 sec, no input       | Send SYN                | R7  |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |7| 45 secs in R7         |                         | R8  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | R8  | WtPickup |1| Allow File Request    | (Receive Bark RB0),     | exit|
        |     |          | |                       |   Hang Up               |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Disallow Requests     | Hang Up                 | exit|
        `-----+----------+-+-----------------------+-------------------------+-----'
        *1 - Some implementations always do (R6.1) even if they have no requests.
        Sender - Send Mail

        .-----+----------+-------------------------+-------------------------+-----.
        |State| State    | Predicate(s)            | Action(s)               | Next|
        |  #  | Name     |                         |                         | St  |
        +-----+----------+-------------------------+-------------------------+-----+
        | SM0 | SendMail |                         | (XMODEM send packet XS0)| SM1 |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | SM1 | CheckMail|1| XMODEM successful     | (Fido registers success)| SM2 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| XMODEM fail or timeout| hang up, report mail bad| exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | SM2 | SendFiles|                         | (BATCH send files BS0)  | SM3 |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | SM3 | CheckFile|1| BATCH send successful | report success          | exit|
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| BATCH send failed     | hang up, rept files fail| exit|
        `-----+----------+-+-----------------------+-------------------------+-----'

        Sender - Send Bark

        .-----+----------+-------------------------+-------------------------+-----.
        |State| State    | Predicate(s)            | Action(s)               | Next|
        |  #  | Name     |                         |                         | St  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | SB0 | SendBark |1| File to request       | Build Bark Request Pkt, | SB1 |
        |     |          | |                       |   Set tries = 0         |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| No more files to req  | Send ETB                | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | SB1 | AskFile  |                         | Send Bark Packet        | SB2 |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | SB2 | RcvFile  |1| Rcv ACK               | (Batch Receive BR0)     | SB3 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Tries > 5             | Send ETB, report failed | exit|
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| Rcv Other             | Purge input, Incr tries | SB1 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |4| 10 sec w/o ACK        | Incr tries              | SB1 |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | SB3 | NxtFile  |1| Rcv ENQ               |                         | SB0 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Rcv Other             | Purge Input             | SB3 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| 5 sec, no input       | Send SUB                | SB3 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |4| 45 sec in SB3         | Hang up, report error   | exit|
        `-----+----------+-+-----------------------+-------------------------+-----'
        Sender & Receiver - Receive Mail

        .-----+----------+-------------------------+-------------------------+-----.
        |State| State    | Predicate(s)            | Action(s)               | Next|
        |  #  | Name     |                         |                         | St  |
        +-----+----------+-------------------------+-------------------------+-----+
        | RM0 | RecMail  |                         | (XMODEM rec packet XR0) | RM1 |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RM1 | XRecEnd  |1| XMODEM successful     | delay 1 second          | RM2 |
        |     |          | |                       |   flush input           |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| XMODEM failed         | hang up, rept mail fail | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RM2 | RecFiles |                         | (BATCH rec files BR0)   | RM3 |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RM3 | ChkFiles |1| BATCH recv successful | delay 2 secs, rprt good | exit|
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| BATCH recv failed     | hang up, report bad file| exit|
        `-----+----------+-+-----------------------+-------------------------+-----'

        Sender & Receiver - Receive Bark

        .-----+----------+-------------------------+-------------------------+-----.
        |State| State    | Predicate(s)            | Action(s)               | Next|
        |  #  | Name     |                         |                         | St  |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RB0 | HonorReq |1| Ok to honor request   | Purge Input, Send ENQ,  | RB1 |
        |     |          | |                       |   Set T1 = 2 seconds    |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Don't wish to honor   | Send CAN                | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RB1 | WaitBark |1| Got ACK               | Rcv Bark Packet (*1)    | RB2 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Got ETB               | Report done             | exit|
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| Got ENQ               | Send ETB                | RB0 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |4| T1 expired            | Purge Input, Send ENQ,  | RB1 |
        |     |          | |                       |   Set T1 = 2 seconds    |     |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |5| 20 seconds in RB1     | Hang Up, Report error   | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RB2 | AckBark  |1| Bark Pkt Rcvd Good    | Send ACK                | RB3 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| Bark Pkt Rcv Error    | Send NAK                | RB1 |
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RB3 | WaitStrt |1| Got 'C' or NAK        |                         | RB4 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |2| No data for 3 seconds | Send ACK                | RB3 |
        |     |          +-+-----------------------+-------------------------+-----+
        |     |          |3| 15 seconds in RB3     | Hang Up, Report Error   | exit|
        +-----+----------+-+-----------------------+-------------------------+-----+
        | RB4 | SendFile |1| Can snd requested file| (Batch Send File BS0)   | RB0 |
        |     |   (*2)   +-+-----------------------+-------------------------+-----+
        |     |          |2| Can't send file       | Send EOT                | RB0 |
        `-----+----------+-+-----------------------+-------------------------+-----'
        *1 - If SUB (16H) received before ETX go to RB0 to resync bark receive

        *2 - While deciding if file exists, and if the password allows it to be
             sent etc., a NUL may be sent to buy 20 seconds more on the timeout
             on the other end if it is using the SEAlink extended FTS-0001
             specification protocol.  Sending a NUL is harmless for a strict
             FTS-0001 session, but will not buy more time.

Go Back