Chapter 1 (b) - Disks created by MS-DOS 6.0 Upgrade using SETUP /F
  
You can create a single startup floppy disk for drive A by specifying the setup command with the
 /f switch. The contents of the startup floppy disk will vary based on the disk’s capacity.
  
Note   You cannot use MS-DOS 6 Upgrade to install the complete operating system (with all programs) 
to floppy disks.
  
The following files will be copied to a floppy disk if you specify the setup /f command:
  
Filename	FileAttributes	Disk Size

                                                360K (5.25)	 720K (3.5)	1.2MB (5.25)	1.44MB (3.5)

IO.SYS	                   SHR	            X 	            X	            X	            X
MSDOS.SYS	       SHR	            X	            X	            X	            X
COMMAND.COM	R		X		X		X	            X
DBLSPACE.BIN			X		X		X		X
ATTRIB.EXE		A		X		X		X		X
DEBUG.EXE		A		X		X		X		X
EXPAND.EXE		A		X		X		X		X
FDISK.EXE		A		X		X		X		X
FORMAT.COM		A		X		X		X		X
RESTORE.EXE		A		X		X		X		X

  
Filename	FileAttributes	Disk Size

                                                360K (5.25)	720K (3.5)	1.2MB (5.25)	1.44MB (3.5)

SYS.COM		A		X		X		X		X
CHKDSK.EXE		A		X		X		X		X
EDIT.COM		A				X		X		X
QBASIC.EXE		A				X		X		X
XCOPY.EXE		A						X		X
MSD.EXE		A						X		X
MSAV.EXE		A				X		X		X
DBLSPACE.EXE	A						X		X

 