\magnification=\magstep1
\vsize=227 true mm \hsize=170 true mm
   \voffset=-0.4 true mm \hoffset=-5.4 true mm

\def\folio{\ifnum\pageno>0 \number\pageno \else\fi}

\font\Largebf=cmbx10  scaled \magstep2
\font\largerm=cmr12
\font\largeit=cmti12
\font\largesc=cmcsc10  scaled \magstep1

\font\tensc=cmcsc10
\font\sevensc=cmcsc10 scaled 700
\newfam\scfam \def\sc{\fam\scfam\tensc}
\textfont\scfam=\tensc \scriptfont\scfam=\sevensc

\pageno=0

\null\vskip72pt

\centerline{\Largebf ON A GENERAL CENTRE OF APPLIED FORCES}

\vskip24pt

\centerline{\Largebf By}

\vskip24pt

\centerline{\Largebf William Rowan Hamilton}

\vskip24pt

\centerline{\largerm (Proceedings of the Royal Irish Academy, 8 (1864),
p.~394.)}

\vskip36pt

\vfill

\centerline{\largerm Edited by David R. Wilkins}

\vskip 12pt

\centerline{\largerm 2000}

\vskip36pt\eject

\null\vskip36pt


\centerline{{\sc On a general Centre of applied Forces}}

\vskip12pt

\centerline{\largerm Sir William Rowan Hamilton}
\vskip12pt
\centerline{[Read June 22nd, 1863.]}
\vskip12pt
\centerline{[{\it Proceedings of the Royal Irish Academy},
   vol.~viii (1864), p.~394.]}

\bigbreak

Sir W.~R. Hamilton wishes a note to be preserved in the
Proceedings of the Royal Irish Academy, that on recently
reconsidering an application of Quaternions to the Statics of a
Solid Body, some account of which was laid before the Academy
many years ago (see the Proceedings for December 1845), he has
been led to perceive the {\it theoretical\/} (and to suspect the
{\it practical\/}) existence of a certain {\it Central Point\/}
for {\it every system of applied forces}, not reducible to a
{\it couple}, nor to {\it zero\/}: which {\it generally new
point}, for the case of {\it parallel forces}, coincides with
their well-known {\it centre}.

An {\it applied force\/} $A B$, acting at a
point~$A$, being said to have a {\it quaternion moment},
equal to the quaternion {\it product\/}
$O A \mathbin{.} A B$,
with respect to any assumed point~$O$, the {\it sum\/} of
all {\it such\/} moments, or the quaternion,
${\rm Q}
   =  \Sigma ( O A \mathbin{.} A B )
   =     O A \mathbin{.} A B
       + O A' \mathbin{.} A' B'
       + \hbox{\&c.}$,
is called the {\it total quaternion moment\/} of the applied
system with respect to the same point~$O$.

This {\it total moment~${\rm Q}$ varies\/} generally with the
{\it point\/} to which it is referred; and there is {\it one\/}
point~$C$, or {\it one position\/} of $O$, for which
the condition
$${\rm T} {\rm Q} = \hbox{\it a minimum},$$
is satisfied, with the exceptions (of {\it couple\/} and
{\it equilibrium}) above alluded to.

It is {\it this point\/}~$C$, which Sir W.~R.~H. proposes
to call {\it generally\/} the {\it Centre of a System of Applied
Forces}.

In the most general case of such a system, he finds it to be
situated {\it on the Central Axis}, the {\it minimum\/}
${\rm T} {\rm Q}$ representing then what was called by Poinsot
the {\it Energy of the Central Couple}.

For the less general case of an {\it unique resultant force}, the
quaternion~${\rm Q}$ reduces itself to {\it zero\/} at the new
Central Point~$C$, which is now situated {\it on the
resultant}, and determines its {\it line of application}.

\bye

.
