# Command: keycode

      KEYCODE helps you scan the output of the keyboard driver.

## Syntax:

      - none -

#### [Main menu] [top] (Syntax) [Options] [Comments] [Examples] [See also] [File]

## Options:

      - none -

#### [Main menu] [top] [Syntax] (Options) [Comments] [Examples] [See also] [File]

## Comments:

      The compiler KC comes with a small program called KEYCODE, which can be
      used to determine the scancode/character pair that is produced by a
      keyboard enhancer (such as FD-KEYB) into the BIOS keyboard buffer.
      To execute it, just enter KEYCODE in the commandline.
      Press the keys or key combinations that you want to guess.
      To exit, press Esc or F1.
      KEYCODE comes with the packet KC200.

#### [Main menu] [top] [Syntax] [Options] (Comments) [Examples] [See also] [File]

## Examples:

      keycocde

#### [Main menu] [top] [Syntax] [Options] [Comments] (Examples) [See also] [File]

## See also:

      cpidos
      display
      kc
      keyb
      keyman
      klib
      kpdos
      mkeyb
      mode
      xkeyb

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] (See also) [File]

## File:

      Please read this command's lsm file also.
      You will find the updated version (internet) here and
      the version described in this manual page here.
      The lsm file contains information about the name of the programmer,
      the download site, and some other command related information.

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] [See also] (File)

      Copyright © 2003 Aitor SANTAMARIA MERINO, updated 2008 by W. Spiegl.

      This file is derived from the FreeDOS Spec Command HOWTO.
      See the file H2Cpying for copying conditions.