# The Netwide Assembler: NASM

Next Chapter | Previous Chapter | Contents | Index

## Appendix B: Instruction List

### B.1 Introduction

The following sections show the instructions which NASM currently supports. For each instruction, there is a separate entry for each supported addressing mode. The third column shows the processor type in which the instruction was introduced and, when appropriate, one or more usage flags.

#### B.1.1 Special instructions...

    DB
    DW
    DD
    DQ
    DT
    DO
    DY
    RESB             imm                      8086
    RESW
    RESD
    RESQ
    REST
    RESO
    RESY

#### B.1.2 Conventional instructions

    AAA                                       8086,NOLONG
    AAD                                       8086,NOLONG
    AAD              imm                      8086,NOLONG
    AAM                                       8086,NOLONG
    AAM              imm                      8086,NOLONG
    AAS                                       8086,NOLONG
    ADC              mem,reg8                 8086
    ADC              reg8,reg8                8086
    ADC              mem,reg16                8086
    ADC              reg16,reg16              8086
    ADC              mem,reg32                386
    ADC              reg32,reg32              386
    ADC              mem,reg64                X64
    ADC              reg64,reg64              X64
    ADC              reg8,mem                 8086
    ADC              reg8,reg8                8086
    ADC              reg16,mem                8086
    ADC              reg16,reg16              8086
    ADC              reg32,mem                386
    ADC              reg32,reg32              386
    ADC              reg64,mem                X64
    ADC              reg64,reg64              X64
    ADC              rm16,imm8                8086
    ADC              rm32,imm8                386
    ADC              rm64,imm8                X64
    ADC              reg_al,imm               8086
    ADC              reg_ax,imm               8086
    ADC              reg_eax,imm              386
    ADC              reg_rax,imm              X64
    ADC              rm8,imm                  8086
    ADC              rm16,imm                 8086
    ADC              rm32,imm                 386
    ADC              rm64,imm                 X64
    ADC              mem,imm8                 8086
    ADC              mem,imm16                8086
    ADC              mem,imm32                386
    ADD              mem,reg8                 8086
    ADD              reg8,reg8                8086
    ADD              mem,reg16                8086
    ADD              reg16,reg16              8086
    ADD              mem,reg32                386
    ADD              reg32,reg32              386
    ADD              mem,reg64                X64
    ADD              reg64,reg64              X64
    ADD              reg8,mem                 8086
    ADD              reg8,reg8                8086
    ADD              reg16,mem                8086
    ADD              reg16,reg16              8086
    ADD              reg32,mem                386
    ADD              reg32,reg32              386
    ADD              reg64,mem                X64
    ADD              reg64,reg64              X64
    ADD              rm16,imm8                8086
    ADD              rm32,imm8                386
    ADD              rm64,imm8                X64
    ADD              reg_al,imm               8086
    ADD              reg_ax,imm               8086
    ADD              reg_eax,imm              386
    ADD              reg_rax,imm              X64
    ADD              rm8,imm                  8086
    ADD              rm16,imm                 8086
    ADD              rm32,imm                 386
    ADD              rm64,imm                 X64
    ADD              mem,imm8                 8086
    ADD              mem,imm16                8086
    ADD              mem,imm32                386
    AND              mem,reg8                 8086
    AND              reg8,reg8                8086
    AND              mem,reg16                8086
    AND              reg16,reg16              8086
    AND              mem,reg32                386
    AND              reg32,reg32              386
    AND              mem,reg64                X64
    AND              reg64,reg64              X64
    AND              reg8,mem                 8086
    AND              reg8,reg8                8086
    AND              reg16,mem                8086
    AND              reg16,reg16              8086
    AND              reg32,mem                386
    AND              reg32,reg32              386
    AND              reg64,mem                X64
    AND              reg64,reg64              X64
    AND              rm16,imm8                8086
    AND              rm32,imm8                386
    AND              rm64,imm8                X64
    AND              reg_al,imm               8086
    AND              reg_ax,imm               8086
    AND              reg_eax,imm              386
    AND              reg_rax,imm              X64
    AND              rm8,imm                  8086
    AND              rm16,imm                 8086
    AND              rm32,imm                 386
    AND              rm64,imm                 X64
    AND              mem,imm8                 8086
    AND              mem,imm16                8086
    AND              mem,imm32                386
    ARPL             mem,reg16                286,PROT,NOLONG
    ARPL             reg16,reg16              286,PROT,NOLONG
    BB0_RESET                                 PENT,CYRIX,ND
    BB1_RESET                                 PENT,CYRIX,ND
    BOUND            reg16,mem                186,NOLONG
    BOUND            reg32,mem                386,NOLONG
    BSF              reg16,mem                386
    BSF              reg16,reg16              386
    BSF              reg32,mem                386
    BSF              reg32,reg32              386
    BSF              reg64,mem                X64
    BSF              reg64,reg64              X64
    BSR              reg16,mem                386
    BSR              reg16,reg16              386
    BSR              reg32,mem                386
    BSR              reg32,reg32              386
    BSR              reg64,mem                X64
    BSR              reg64,reg64              X64
    BSWAP            reg32                    486
    BSWAP            reg64                    X64
    BT               mem,reg16                386
    BT               reg16,reg16              386
    BT               mem,reg32                386
    BT               reg32,reg32              386
    BT               mem,reg64                X64
    BT               reg64,reg64              X64
    BT               rm16,imm                 386
    BT               rm32,imm                 386
    BT               rm64,imm                 X64
    BTC              mem,reg16                386
    BTC              reg16,reg16              386
    BTC              mem,reg32                386
    BTC              reg32,reg32              386
    BTC              mem,reg64                X64
    BTC              reg64,reg64              X64
    BTC              rm16,imm                 386
    BTC              rm32,imm                 386
    BTC              rm64,imm                 X64
    BTR              mem,reg16                386
    BTR              reg16,reg16              386
    BTR              mem,reg32                386
    BTR              reg32,reg32              386
    BTR              mem,reg64                X64
    BTR              reg64,reg64              X64
    BTR              rm16,imm                 386
    BTR              rm32,imm                 386
    BTR              rm64,imm                 X64
    BTS              mem,reg16                386
    BTS              reg16,reg16              386
    BTS              mem,reg32                386
    BTS              reg32,reg32              386
    BTS              mem,reg64                X64
    BTS              reg64,reg64              X64
    BTS              rm16,imm                 386
    BTS              rm32,imm                 386
    BTS              rm64,imm                 X64
    CALL             imm                      8086
    CALL             imm|near                 8086
    CALL             imm|far                  8086,ND,NOLONG
    CALL             imm16                    8086
    CALL             imm16|near               8086
    CALL             imm16|far                8086,ND,NOLONG
    CALL             imm32                    386
    CALL             imm32|near               386
    CALL             imm32|far                386,ND,NOLONG
    CALL             imm:imm                  8086,NOLONG
    CALL             imm16:imm                8086,NOLONG
    CALL             imm:imm16                8086,NOLONG
    CALL             imm32:imm                386,NOLONG
    CALL             imm:imm32                386,NOLONG
    CALL             mem|far                  8086,NOLONG
    CALL             mem|far                  X64
    CALL             mem16|far                8086
    CALL             mem32|far                386
    CALL             mem64|far                X64
    CALL             mem|near                 8086
    CALL             mem16|near               8086
    CALL             mem32|near               386,NOLONG
    CALL             mem64|near               X64
    CALL             reg16                    8086
    CALL             reg32                    386,NOLONG
    CALL             reg64                    X64
    CALL             mem                      8086
    CALL             mem16                    8086
    CALL             mem32                    386,NOLONG
    CALL             mem64                    X64
    CBW                                       8086
    CDQ                                       386
    CDQE                                      X64
    CLC                                       8086
    CLD                                       8086
    CLGI                                      X64,AMD
    CLI                                       8086
    CLTS                                      286,PRIV
    CMC                                       8086
    CMP              mem,reg8                 8086
    CMP              reg8,reg8                8086
    CMP              mem,reg16                8086
    CMP              reg16,reg16              8086
    CMP              mem,reg32                386
    CMP              reg32,reg32              386
    CMP              mem,reg64                X64
    CMP              reg64,reg64              X64
    CMP              reg8,mem                 8086
    CMP              reg8,reg8                8086
    CMP              reg16,mem                8086
    CMP              reg16,reg16              8086
    CMP              reg32,mem                386
    CMP              reg32,reg32              386
    CMP              reg64,mem                X64
    CMP              reg64,reg64              X64
    CMP              rm16,imm8                8086
    CMP              rm32,imm8                386
    CMP              rm64,imm8                X64
    CMP              reg_al,imm               8086
    CMP              reg_ax,imm               8086
    CMP              reg_eax,imm              386
    CMP              reg_rax,imm              X64
    CMP              rm8,imm                  8086
    CMP              rm16,imm                 8086
    CMP              rm32,imm                 386
    CMP              rm64,imm                 X64
    CMP              mem,imm8                 8086
    CMP              mem,imm16                8086
    CMP              mem,imm32                386
    CMPSB                                     8086
    CMPSD                                     386
    CMPSQ                                     X64
    CMPSW                                     8086
    CMPXCHG          mem,reg8                 PENT
    CMPXCHG          reg8,reg8                PENT
    CMPXCHG          mem,reg16                PENT
    CMPXCHG          reg16,reg16              PENT
    CMPXCHG          mem,reg32                PENT
    CMPXCHG          reg32,reg32              PENT
    CMPXCHG          mem,reg64                X64
    CMPXCHG          reg64,reg64              X64
    CMPXCHG486       mem,reg8                 486,UNDOC,ND
    CMPXCHG486       reg8,reg8                486,UNDOC,ND
    CMPXCHG486       mem,reg16                486,UNDOC,ND
    CMPXCHG486       reg16,reg16              486,UNDOC,ND
    CMPXCHG486       mem,reg32                486,UNDOC,ND
    CMPXCHG486       reg32,reg32              486,UNDOC,ND
    CMPXCHG8B        mem                      PENT
    CMPXCHG16B       mem                      X64
    CPUID                                     PENT
    CPU_READ                                  PENT,CYRIX
    CPU_WRITE                                 PENT,CYRIX
    CQO                                       X64
    CWD                                       8086
    CWDE                                      386
    DAA                                       8086,NOLONG
    DAS                                       8086,NOLONG
    DEC              reg16                    8086,NOLONG
    DEC              reg32                    386,NOLONG
    DEC              rm8                      8086
    DEC              rm16                     8086
    DEC              rm32                     386
    DEC              rm64                     X64
    DIV              rm8                      8086
    DIV              rm16                     8086
    DIV              rm32                     386
    DIV              rm64                     X64
    DMINT                                     P6,CYRIX
    EMMS                                      PENT,MMX
    ENTER            imm,imm                  186
    EQU              imm                      8086
    EQU              imm:imm                  8086
    F2XM1                                     8086,FPU
    FABS                                      8086,FPU
    FADD             mem32                    8086,FPU
    FADD             mem64                    8086,FPU
    FADD             fpureg|to                8086,FPU
    FADD             fpureg                   8086,FPU
    FADD             fpureg,fpu0              8086,FPU
    FADD             fpu0,fpureg              8086,FPU
    FADD                                      8086,FPU,ND
    FADDP            fpureg                   8086,FPU
    FADDP            fpureg,fpu0              8086,FPU
    FADDP                                     8086,FPU,ND
    FBLD             mem80                    8086,FPU
    FBLD             mem                      8086,FPU
    FBSTP            mem80                    8086,FPU
    FBSTP            mem                      8086,FPU
    FCHS                                      8086,FPU
    FCLEX                                     8086,FPU
    FCMOVB           fpureg                   P6,FPU
    FCMOVB           fpu0,fpureg              P6,FPU
    FCMOVB                                    P6,FPU,ND
    FCMOVBE          fpureg                   P6,FPU
    FCMOVBE          fpu0,fpureg              P6,FPU
    FCMOVBE                                   P6,FPU,ND
    FCMOVE           fpureg                   P6,FPU
    FCMOVE           fpu0,fpureg              P6,FPU
    FCMOVE                                    P6,FPU,ND
    FCMOVNB          fpureg                   P6,FPU
    FCMOVNB          fpu0,fpureg              P6,FPU
    FCMOVNB                                   P6,FPU,ND
    FCMOVNBE         fpureg                   P6,FPU
    FCMOVNBE         fpu0,fpureg              P6,FPU
    FCMOVNBE                                  P6,FPU,ND
    FCMOVNE          fpureg                   P6,FPU
    FCMOVNE          fpu0,fpureg              P6,FPU
    FCMOVNE                                   P6,FPU,ND
    FCMOVNU          fpureg                   P6,FPU
    FCMOVNU          fpu0,fpureg              P6,FPU
    FCMOVNU                                   P6,FPU,ND
    FCMOVU           fpureg                   P6,FPU
    FCMOVU           fpu0,fpureg              P6,FPU
    FCMOVU                                    P6,FPU,ND
    FCOM             mem32                    8086,FPU
    FCOM             mem64                    8086,FPU
    FCOM             fpureg                   8086,FPU
    FCOM             fpu0,fpureg              8086,FPU
    FCOM                                      8086,FPU,ND
    FCOMI            fpureg                   P6,FPU
    FCOMI            fpu0,fpureg              P6,FPU
    FCOMI                                     P6,FPU,ND
    FCOMIP           fpureg                   P6,FPU
    FCOMIP           fpu0,fpureg              P6,FPU
    FCOMIP                                    P6,FPU,ND
    FCOMP            mem32                    8086,FPU
    FCOMP            mem64                    8086,FPU
    FCOMP            fpureg                   8086,FPU
    FCOMP            fpu0,fpureg              8086,FPU
    FCOMP                                     8086,FPU,ND
    FCOMPP                                    8086,FPU
    FCOS                                      386,FPU
    FDECSTP                                   8086,FPU
    FDISI                                     8086,FPU
    FDIV             mem32                    8086,FPU
    FDIV             mem64                    8086,FPU
    FDIV             fpureg|to                8086,FPU
    FDIV             fpureg                   8086,FPU
    FDIV             fpureg,fpu0              8086,FPU
    FDIV             fpu0,fpureg              8086,FPU
    FDIV                                      8086,FPU,ND
    FDIVP            fpureg                   8086,FPU
    FDIVP            fpureg,fpu0              8086,FPU
    FDIVP                                     8086,FPU,ND
    FDIVR            mem32                    8086,FPU
    FDIVR            mem64                    8086,FPU
    FDIVR            fpureg|to                8086,FPU
    FDIVR            fpureg,fpu0              8086,FPU
    FDIVR            fpureg                   8086,FPU
    FDIVR            fpu0,fpureg              8086,FPU
    FDIVR                                     8086,FPU,ND
    FDIVRP           fpureg                   8086,FPU
    FDIVRP           fpureg,fpu0              8086,FPU
    FDIVRP                                    8086,FPU,ND
    FEMMS                                     PENT,3DNOW
    FENI                                      8086,FPU
    FFREE            fpureg                   8086,FPU
    FFREE                                     8086,FPU
    FFREEP           fpureg                   286,FPU,UNDOC
    FFREEP                                    286,FPU,UNDOC
    FIADD            mem32                    8086,FPU
    FIADD            mem16                    8086,FPU
    FICOM            mem32                    8086,FPU
    FICOM            mem16                    8086,FPU
    FICOMP           mem32                    8086,FPU
    FICOMP           mem16                    8086,FPU
    FIDIV            mem32                    8086,FPU
    FIDIV            mem16                    8086,FPU
    FIDIVR           mem32                    8086,FPU
    FIDIVR           mem16                    8086,FPU
    FILD             mem32                    8086,FPU
    FILD             mem16                    8086,FPU
    FILD             mem64                    8086,FPU
    FIMUL            mem32                    8086,FPU
    FIMUL            mem16                    8086,FPU
    FINCSTP                                   8086,FPU
    FINIT                                     8086,FPU
    FIST             mem32                    8086,FPU
    FIST             mem16                    8086,FPU
    FISTP            mem32                    8086,FPU
    FISTP            mem16                    8086,FPU
    FISTP            mem64                    8086,FPU
    FISTTP           mem16                    PRESCOTT,FPU
    FISTTP           mem32                    PRESCOTT,FPU
    FISTTP           mem64                    PRESCOTT,FPU
    FISUB            mem32                    8086,FPU
    FISUB            mem16                    8086,FPU
    FISUBR           mem32                    8086,FPU
    FISUBR           mem16                    8086,FPU
    FLD              mem32                    8086,FPU
    FLD              mem64                    8086,FPU
    FLD              mem80                    8086,FPU
    FLD              fpureg                   8086,FPU
    FLD                                       8086,FPU,ND
    FLD1                                      8086,FPU
    FLDCW            mem                      8086,FPU,SW
    FLDENV           mem                      8086,FPU
    FLDL2E                                    8086,FPU
    FLDL2T                                    8086,FPU
    FLDLG2                                    8086,FPU
    FLDLN2                                    8086,FPU
    FLDPI                                     8086,FPU
    FLDZ                                      8086,FPU
    FMUL             mem32                    8086,FPU
    FMUL             mem64                    8086,FPU
    FMUL             fpureg|to                8086,FPU
    FMUL             fpureg,fpu0              8086,FPU
    FMUL             fpureg                   8086,FPU
    FMUL             fpu0,fpureg              8086,FPU
    FMUL                                      8086,FPU,ND
    FMULP            fpureg                   8086,FPU
    FMULP            fpureg,fpu0              8086,FPU
    FMULP                                     8086,FPU,ND
    FNCLEX                                    8086,FPU
    FNDISI                                    8086,FPU
    FNENI                                     8086,FPU
    FNINIT                                    8086,FPU
    FNOP                                      8086,FPU
    FNSAVE           mem                      8086,FPU
    FNSTCW           mem                      8086,FPU,SW
    FNSTENV          mem                      8086,FPU
    FNSTSW           mem                      8086,FPU,SW
    FNSTSW           reg_ax                   286,FPU
    FPATAN                                    8086,FPU
    FPREM                                     8086,FPU
    FPREM1                                    386,FPU
    FPTAN                                     8086,FPU
    FRNDINT                                   8086,FPU
    FRSTOR           mem                      8086,FPU
    FSAVE            mem                      8086,FPU
    FSCALE                                    8086,FPU
    FSETPM                                    286,FPU
    FSIN                                      386,FPU
    FSINCOS                                   386,FPU
    FSQRT                                     8086,FPU
    FST              mem32                    8086,FPU
    FST              mem64                    8086,FPU
    FST              fpureg                   8086,FPU
    FST                                       8086,FPU,ND
    FSTCW            mem                      8086,FPU,SW
    FSTENV           mem                      8086,FPU
    FSTP             mem32                    8086,FPU
    FSTP             mem64                    8086,FPU
    FSTP             mem80                    8086,FPU
    FSTP             fpureg                   8086,FPU
    FSTP                                      8086,FPU,ND
    FSTSW            mem                      8086,FPU,SW
    FSTSW            reg_ax                   286,FPU
    FSUB             mem32                    8086,FPU
    FSUB             mem64                    8086,FPU
    FSUB             fpureg|to                8086,FPU
    FSUB             fpureg,fpu0              8086,FPU
    FSUB             fpureg                   8086,FPU
    FSUB             fpu0,fpureg              8086,FPU
    FSUB                                      8086,FPU,ND
    FSUBP            fpureg                   8086,FPU
    FSUBP            fpureg,fpu0              8086,FPU
    FSUBP                                     8086,FPU,ND
    FSUBR            mem32                    8086,FPU
    FSUBR            mem64                    8086,FPU
    FSUBR            fpureg|to                8086,FPU
    FSUBR            fpureg,fpu0              8086,FPU
    FSUBR            fpureg                   8086,FPU
    FSUBR            fpu0,fpureg              8086,FPU
    FSUBR                                     8086,FPU,ND
    FSUBRP           fpureg                   8086,FPU
    FSUBRP           fpureg,fpu0              8086,FPU
    FSUBRP                                    8086,FPU,ND
    FTST                                      8086,FPU
    FUCOM            fpureg                   386,FPU
    FUCOM            fpu0,fpureg              386,FPU
    FUCOM                                     386,FPU,ND
    FUCOMI           fpureg                   P6,FPU
    FUCOMI           fpu0,fpureg              P6,FPU
    FUCOMI                                    P6,FPU,ND
    FUCOMIP          fpureg                   P6,FPU
    FUCOMIP          fpu0,fpureg              P6,FPU
    FUCOMIP                                   P6,FPU,ND
    FUCOMP           fpureg                   386,FPU
    FUCOMP           fpu0,fpureg              386,FPU
    FUCOMP                                    386,FPU,ND
    FUCOMPP                                   386,FPU
    FXAM                                      8086,FPU
    FXCH             fpureg                   8086,FPU
    FXCH             fpureg,fpu0              8086,FPU
    FXCH             fpu0,fpureg              8086,FPU
    FXCH                                      8086,FPU,ND
    FXTRACT                                   8086,FPU
    FYL2X                                     8086,FPU
    FYL2XP1                                   8086,FPU
    HLT                                       8086,PRIV
    IBTS             mem,reg16                386,SW,UNDOC,ND
    IBTS             reg16,reg16              386,UNDOC,ND
    IBTS             mem,reg32                386,SD,UNDOC,ND
    IBTS             reg32,reg32              386,UNDOC,ND
    ICEBP                                     386,ND
    IDIV             rm8                      8086
    IDIV             rm16                     8086
    IDIV             rm32                     386
    IDIV             rm64                     X64
    IMUL             rm8                      8086
    IMUL             rm16                     8086
    IMUL             rm32                     386
    IMUL             rm64                     X64
    IMUL             reg16,mem                386
    IMUL             reg16,reg16              386
    IMUL             reg32,mem                386
    IMUL             reg32,reg32              386
    IMUL             reg64,mem                X64
    IMUL             reg64,reg64              X64
    IMUL             reg16,mem,imm8           186
    IMUL             reg16,mem,sbyte16        186,ND
    IMUL             reg16,mem,imm16          186
    IMUL             reg16,mem,imm            186,ND
    IMUL             reg16,reg16,imm8         186
    IMUL             reg16,reg16,sbyte32      186,ND
    IMUL             reg16,reg16,imm16        186
    IMUL             reg16,reg16,imm          186,ND
    IMUL             reg32,mem,imm8           386
    IMUL             reg32,mem,sbyte64        386,ND
    IMUL             reg32,mem,imm32          386
    IMUL             reg32,mem,imm            386,ND
    IMUL             reg32,reg32,imm8         386
    IMUL             reg32,reg32,sbyte16      386,ND
    IMUL             reg32,reg32,imm32        386
    IMUL             reg32,reg32,imm          386,ND
    IMUL             reg64,mem,imm8           X64
    IMUL             reg64,mem,sbyte32        X64,ND
    IMUL             reg64,mem,imm32          X64
    IMUL             reg64,mem,imm            X64,ND
    IMUL             reg64,reg64,imm8         X64
    IMUL             reg64,reg64,sbyte64      X64,ND
    IMUL             reg64,reg64,imm32        X64
    IMUL             reg64,reg64,imm          X64,ND
    IMUL             reg16,imm8               186
    IMUL             reg16,sbyte16            186,ND
    IMUL             reg16,imm16              186
    IMUL             reg16,imm                186,ND
    IMUL             reg32,imm8               386
    IMUL             reg32,sbyte32            386,ND
    IMUL             reg32,imm32              386
    IMUL             reg32,imm                386,ND
    IMUL             reg64,imm8               X64
    IMUL             reg64,sbyte64            X64,ND
    IMUL             reg64,imm32              X64
    IMUL             reg64,imm                X64,ND
    IN               reg_al,imm               8086
    IN               reg_ax,imm               8086
    IN               reg_eax,imm              386
    IN               reg_al,reg_dx            8086
    IN               reg_ax,reg_dx            8086
    IN               reg_eax,reg_dx           386
    INC              reg16                    8086,NOLONG
    INC              reg32                    386,NOLONG
    INC              rm8                      8086
    INC              rm16                     8086
    INC              rm32                     386
    INC              rm64                     X64
    INCBIN
    INSB                                      186
    INSD                                      386
    INSW                                      186
    INT              imm                      8086
    INT01                                     386,ND
    INT1                                      386
    INT03                                     8086,ND
    INT3                                      8086
    INTO                                      8086,NOLONG
    INVD                                      486,PRIV
    INVLPG           mem                      486,PRIV
    INVLPGA          reg_ax,reg_ecx           X86_64,AMD,NOLONG
    INVLPGA          reg_eax,reg_ecx          X86_64,AMD
    INVLPGA          reg_rax,reg_ecx          X64,AMD
    INVLPGA                                   X86_64,AMD
    IRET                                      8086
    IRETD                                     386
    IRETQ                                     X64
    IRETW                                     8086
    JCXZ             imm                      8086,NOLONG
    JECXZ            imm                      386
    JMP              imm|short                8086
    JMP              imm                      8086,ND
    JMP              imm                      8086
    JMP              imm|near                 8086,ND
    JMP              imm|far                  8086,ND,NOLONG
    JMP              imm16                    8086
    JMP              imm16|near               8086,ND
    JMP              imm16|far                8086,ND,NOLONG
    JMP              imm32                    386
    JMP              imm32|near               386,ND
    JMP              imm32|far                386,ND,NOLONG
    JMP              imm:imm                  8086,NOLONG
    JMP              imm16:imm                8086,NOLONG
    JMP              imm:imm16                8086,NOLONG
    JMP              imm32:imm                386,NOLONG
    JMP              imm:imm32                386,NOLONG
    JMP              mem|far                  8086,NOLONG
    JMP              mem|far                  X64
    JMP              mem16|far                8086
    JMP              mem32|far                386
    JMP              mem64|far                X64
    JMP              mem|near                 8086
    JMP              mem16|near               8086
    JMP              mem32|near               386,NOLONG
    JMP              mem64|near               X64
    JMP              reg16                    8086
    JMP              reg32                    386,NOLONG
    JMP              reg64                    X64
    JMP              mem                      8086
    JMP              mem16                    8086
    JMP              mem32                    386,NOLONG
    JMP              mem64                    X64
    JMPE             imm                      IA64
    JMPE             imm16                    IA64
    JMPE             imm32                    IA64
    JMPE             rm16                     IA64
    JMPE             rm32                     IA64
    JRCXZ            imm                      X64
    LAHF                                      8086
    LAR              reg16,mem                286,PROT,SW
    LAR              reg16,reg16              286,PROT
    LAR              reg16,reg32              386,PROT
    LAR              reg16,reg64              X64,PROT,ND
    LAR              reg32,mem                386,PROT,SW
    LAR              reg32,reg16              386,PROT
    LAR              reg32,reg32              386,PROT
    LAR              reg32,reg64              X64,PROT,ND
    LAR              reg64,mem                X64,PROT,SW
    LAR              reg64,reg16              X64,PROT
    LAR              reg64,reg32              X64,PROT
    LAR              reg64,reg64              X64,PROT
    LDS              reg16,mem                8086,NOLONG
    LDS              reg32,mem                386,NOLONG
    LEA              reg16,mem                8086
    LEA              reg32,mem                386
    LEA              reg64,mem                X64
    LEAVE                                     186
    LES              reg16,mem                8086,NOLONG
    LES              reg32,mem                386,NOLONG
    LFENCE                                    X64,AMD
    LFS              reg16,mem                386
    LFS              reg32,mem                386
    LGDT             mem                      286,PRIV
    LGS              reg16,mem                386
    LGS              reg32,mem                386
    LIDT             mem                      286,PRIV
    LLDT             mem                      286,PROT,PRIV
    LLDT             mem16                    286,PROT,PRIV
    LLDT             reg16                    286,PROT,PRIV
    LMSW             mem                      286,PRIV
    LMSW             mem16                    286,PRIV
    LMSW             reg16                    286,PRIV
    LOADALL                                   386,UNDOC
    LOADALL286                                286,UNDOC
    LODSB                                     8086
    LODSD                                     386
    LODSQ                                     X64
    LODSW                                     8086
    LOOP             imm                      8086
    LOOP             imm,reg_cx               8086,NOLONG
    LOOP             imm,reg_ecx              386
    LOOP             imm,reg_rcx              X64
    LOOPE            imm                      8086
    LOOPE            imm,reg_cx               8086,NOLONG
    LOOPE            imm,reg_ecx              386
    LOOPE            imm,reg_rcx              X64
    LOOPNE           imm                      8086
    LOOPNE           imm,reg_cx               8086,NOLONG
    LOOPNE           imm,reg_ecx              386
    LOOPNE           imm,reg_rcx              X64
    LOOPNZ           imm                      8086
    LOOPNZ           imm,reg_cx               8086,NOLONG
    LOOPNZ           imm,reg_ecx              386
    LOOPNZ           imm,reg_rcx              X64
    LOOPZ            imm                      8086
    LOOPZ            imm,reg_cx               8086,NOLONG
    LOOPZ            imm,reg_ecx              386
    LOOPZ            imm,reg_rcx              X64
    LSL              reg16,mem                286,PROT,SW
    LSL              reg16,reg16              286,PROT
    LSL              reg16,reg32              386,PROT
    LSL              reg16,reg64              X64,PROT,ND
    LSL              reg32,mem                386,PROT,SW
    LSL              reg32,reg16              386,PROT
    LSL              reg32,reg32              386,PROT
    LSL              reg32,reg64              X64,PROT,ND
    LSL              reg64,mem                X64,PROT,SW
    LSL              reg64,reg16              X64,PROT
    LSL              reg64,reg32              X64,PROT
    LSL              reg64,reg64              X64,PROT
    LSS              reg16,mem                386
    LSS              reg32,mem                386
    LTR              mem                      286,PROT,PRIV
    LTR              mem16                    286,PROT,PRIV
    LTR              reg16                    286,PROT,PRIV
    MFENCE                                    X64,AMD
    MONITOR                                   PRESCOTT
    MONITOR          reg_eax,reg_ecx,reg_edx  PRESCOTT,ND
    MOV              mem,reg_sreg             8086
    MOV              reg16,reg_sreg           8086
    MOV              reg32,reg_sreg           386
    MOV              reg_sreg,mem             8086
    MOV              reg_sreg,reg16           8086
    MOV              reg_sreg,reg32           386
    MOV              reg_al,mem_offs          8086
    MOV              reg_ax,mem_offs          8086
    MOV              reg_eax,mem_offs         386
    MOV              reg_rax,mem_offs         X64
    MOV              mem_offs,reg_al          8086
    MOV              mem_offs,reg_ax          8086
    MOV              mem_offs,reg_eax         386
    MOV              mem_offs,reg_rax         X64
    MOV              reg32,reg_creg           386,PRIV,NOLONG
    MOV              reg64,reg_creg           X64,PRIV
    MOV              reg_creg,reg32           386,PRIV,NOLONG
    MOV              reg_creg,reg64           X64,PRIV
    MOV              reg32,reg_dreg           386,PRIV,NOLONG
    MOV              reg64,reg_dreg           X64,PRIV
    MOV              reg_dreg,reg32           386,PRIV,NOLONG
    MOV              reg_dreg,reg64           X64,PRIV
    MOV              reg32,reg_treg           386,NOLONG,ND
    MOV              reg_treg,reg32           386,NOLONG,ND
    MOV              mem,reg8                 8086
    MOV              reg8,reg8                8086
    MOV              mem,reg16                8086
    MOV              reg16,reg16              8086
    MOV              mem,reg32                386
    MOV              reg32,reg32              386
    MOV              mem,reg64                X64
    MOV              reg64,reg64              X64
    MOV              reg8,mem                 8086
    MOV              reg8,reg8                8086
    MOV              reg16,mem                8086
    MOV              reg16,reg16              8086
    MOV              reg32,mem                386
    MOV              reg32,reg32              386
    MOV              reg64,mem                X64
    MOV              reg64,reg64              X64
    MOV              reg8,imm                 8086
    MOV              reg16,imm                8086
    MOV              reg32,imm                386
    MOV              reg64,imm                X64
    MOV              reg64,imm32              X64
    MOV              rm8,imm                  8086
    MOV              rm16,imm                 8086
    MOV              rm32,imm                 386
    MOV              rm64,imm                 X64
    MOV              mem,imm8                 8086
    MOV              mem,imm16                8086
    MOV              mem,imm32                386
    MOVD             mmxreg,mem               PENT,MMX,SD
    MOVD             mmxreg,reg32             PENT,MMX
    MOVD             mem,mmxreg               PENT,MMX,SD
    MOVD             reg32,mmxreg             PENT,MMX
    MOVD             xmmreg,mem               X64,SD
    MOVD             xmmreg,reg32             X64
    MOVD             mem,xmmreg               X64,SD
    MOVD             reg32,xmmreg             X64,SSE
    MOVQ             mmxreg,mmxrm             PENT,MMX
    MOVQ             mmxrm,mmxreg             PENT,MMX
    MOVQ             mmxreg,rm64              X64,MMX
    MOVQ             rm64,mmxreg              X64,MMX
    MOVSB                                     8086
    MOVSD                                     386
    MOVSQ                                     X64
    MOVSW                                     8086
    MOVSX            reg16,mem                386
    MOVSX            reg16,reg8               386
    MOVSX            reg32,rm8                386
    MOVSX            reg32,rm16               386
    MOVSX            reg64,rm8                X64
    MOVSX            reg64,rm16               X64
    MOVSXD           reg64,rm32               X64
    MOVSX            reg64,rm32               X64,ND
    MOVZX            reg16,mem                386
    MOVZX            reg16,reg8               386
    MOVZX            reg32,rm8                386
    MOVZX            reg32,rm16               386
    MOVZX            reg64,rm8                X64
    MOVZX            reg64,rm16               X64
    MUL              rm8                      8086
    MUL              rm16                     8086
    MUL              rm32                     386
    MUL              rm64                     X64
    MWAIT                                     PRESCOTT
    MWAIT            reg_eax,reg_ecx          PRESCOTT,ND
    NEG              rm8                      8086
    NEG              rm16                     8086
    NEG              rm32                     386
    NEG              rm64                     X64
    NOP                                       8086
    NOP              rm16                     P6
    NOP              rm32                     P6
    NOP              rm64                     X64
    NOT              rm8                      8086
    NOT              rm16                     8086
    NOT              rm32                     386
    NOT              rm64                     X64
    OR               mem,reg8                 8086
    OR               reg8,reg8                8086
    OR               mem,reg16                8086
    OR               reg16,reg16              8086
    OR               mem,reg32                386
    OR               reg32,reg32              386
    OR               mem,reg64                X64
    OR               reg64,reg64              X64
    OR               reg8,mem                 8086
    OR               reg8,reg8                8086
    OR               reg16,mem                8086
    OR               reg16,reg16              8086
    OR               reg32,mem                386
    OR               reg32,reg32              386
    OR               reg64,mem                X64
    OR               reg64,reg64              X64
    OR               rm16,imm8                8086
    OR               rm32,imm8                386
    OR               rm64,imm8                X64
    OR               reg_al,imm               8086
    OR               reg_ax,imm               8086
    OR               reg_eax,imm              386
    OR               reg_rax,imm              X64
    OR               rm8,imm                  8086
    OR               rm16,imm                 8086
    OR               rm32,imm                 386
    OR               rm64,imm                 X64
    OR               mem,imm8                 8086
    OR               mem,imm16                8086
    OR               mem,imm32                386
    OUT              imm,reg_al               8086
    OUT              imm,reg_ax               8086
    OUT              imm,reg_eax              386
    OUT              reg_dx,reg_al            8086
    OUT              reg_dx,reg_ax            8086
    OUT              reg_dx,reg_eax           386
    OUTSB                                     186
    OUTSD                                     386
    OUTSW                                     186
    PACKSSDW         mmxreg,mmxrm             PENT,MMX
    PACKSSWB         mmxreg,mmxrm             PENT,MMX
    PACKUSWB         mmxreg,mmxrm             PENT,MMX
    PADDB            mmxreg,mmxrm             PENT,MMX
    PADDD            mmxreg,mmxrm             PENT,MMX
    PADDSB           mmxreg,mmxrm             PENT,MMX
    PADDSIW          mmxreg,mmxrm             PENT,MMX,CYRIX
    PADDSW           mmxreg,mmxrm             PENT,MMX
    PADDUSB          mmxreg,mmxrm             PENT,MMX
    PADDUSW          mmxreg,mmxrm             PENT,MMX
    PADDW            mmxreg,mmxrm             PENT,MMX
    PAND             mmxreg,mmxrm             PENT,MMX
    PANDN            mmxreg,mmxrm             PENT,MMX
    PAUSE                                     8086
    PAVEB            mmxreg,mmxrm             PENT,MMX,CYRIX
    PAVGUSB          mmxreg,mmxrm             PENT,3DNOW
    PCMPEQB          mmxreg,mmxrm             PENT,MMX
    PCMPEQD          mmxreg,mmxrm             PENT,MMX
    PCMPEQW          mmxreg,mmxrm             PENT,MMX
    PCMPGTB          mmxreg,mmxrm             PENT,MMX
    PCMPGTD          mmxreg,mmxrm             PENT,MMX
    PCMPGTW          mmxreg,mmxrm             PENT,MMX
    PDISTIB          mmxreg,mem               PENT,MMX,CYRIX
    PF2ID            mmxreg,mmxrm             PENT,3DNOW
    PFACC            mmxreg,mmxrm             PENT,3DNOW
    PFADD            mmxreg,mmxrm             PENT,3DNOW
    PFCMPEQ          mmxreg,mmxrm             PENT,3DNOW
    PFCMPGE          mmxreg,mmxrm             PENT,3DNOW
    PFCMPGT          mmxreg,mmxrm             PENT,3DNOW
    PFMAX            mmxreg,mmxrm             PENT,3DNOW
    PFMIN            mmxreg,mmxrm             PENT,3DNOW
    PFMUL            mmxreg,mmxrm             PENT,3DNOW
    PFRCP            mmxreg,mmxrm             PENT,3DNOW
    PFRCPIT1         mmxreg,mmxrm             PENT,3DNOW
    PFRCPIT2         mmxreg,mmxrm             PENT,3DNOW
    PFRSQIT1         mmxreg,mmxrm             PENT,3DNOW
    PFRSQRT          mmxreg,mmxrm             PENT,3DNOW
    PFSUB            mmxreg,mmxrm             PENT,3DNOW
    PFSUBR           mmxreg,mmxrm             PENT,3DNOW
    PI2FD            mmxreg,mmxrm             PENT,3DNOW
    PMACHRIW         mmxreg,mem               PENT,MMX,CYRIX
    PMADDWD          mmxreg,mmxrm             PENT,MMX
    PMAGW            mmxreg,mmxrm             PENT,MMX,CYRIX
    PMULHRIW         mmxreg,mmxrm             PENT,MMX,CYRIX
    PMULHRWA         mmxreg,mmxrm             PENT,3DNOW
    PMULHRWC         mmxreg,mmxrm             PENT,MMX,CYRIX
    PMULHW           mmxreg,mmxrm             PENT,MMX
    PMULLW           mmxreg,mmxrm             PENT,MMX
    PMVGEZB          mmxreg,mem               PENT,MMX,CYRIX
    PMVLZB           mmxreg,mem               PENT,MMX,CYRIX
    PMVNZB           mmxreg,mem               PENT,MMX,CYRIX
    PMVZB            mmxreg,mem               PENT,MMX,CYRIX
    POP              reg16                    8086
    POP              reg32                    386,NOLONG
    POP              reg64                    X64
    POP              rm16                     8086
    POP              rm32                     386,NOLONG
    POP              rm64                     X64
    POP              reg_cs                   8086,UNDOC,ND
    POP              reg_dess                 8086,NOLONG
    POP              reg_fsgs                 386
    POPA                                      186,NOLONG
    POPAD                                     386,NOLONG
    POPAW                                     186,NOLONG
    POPF                                      8086
    POPFD                                     386,NOLONG
    POPFQ                                     X64
    POPFW                                     8086
    POR              mmxreg,mmxrm             PENT,MMX
    PREFETCH         mem                      PENT,3DNOW
    PREFETCHW        mem                      PENT,3DNOW
    PSLLD            mmxreg,mmxrm             PENT,MMX
    PSLLD            mmxreg,imm               PENT,MMX
    PSLLQ            mmxreg,mmxrm             PENT,MMX
    PSLLQ            mmxreg,imm               PENT,MMX
    PSLLW            mmxreg,mmxrm             PENT,MMX
    PSLLW            mmxreg,imm               PENT,MMX
    PSRAD            mmxreg,mmxrm             PENT,MMX
    PSRAD            mmxreg,imm               PENT,MMX
    PSRAW            mmxreg,mmxrm             PENT,MMX
    PSRAW            mmxreg,imm               PENT,MMX
    PSRLD            mmxreg,mmxrm             PENT,MMX
    PSRLD            mmxreg,imm               PENT,MMX
    PSRLQ            mmxreg,mmxrm             PENT,MMX
    PSRLQ            mmxreg,imm               PENT,MMX
    PSRLW            mmxreg,mmxrm             PENT,MMX
    PSRLW            mmxreg,imm               PENT,MMX
    PSUBB            mmxreg,mmxrm             PENT,MMX
    PSUBD            mmxreg,mmxrm             PENT,MMX
    PSUBSB           mmxreg,mmxrm             PENT,MMX
    PSUBSIW          mmxreg,mmxrm             PENT,MMX,CYRIX
    PSUBSW           mmxreg,mmxrm             PENT,MMX
    PSUBUSB          mmxreg,mmxrm             PENT,MMX
    PSUBUSW          mmxreg,mmxrm             PENT,MMX
    PSUBW            mmxreg,mmxrm             PENT,MMX
    PUNPCKHBW        mmxreg,mmxrm             PENT,MMX
    PUNPCKHDQ        mmxreg,mmxrm             PENT,MMX
    PUNPCKHWD        mmxreg,mmxrm             PENT,MMX
    PUNPCKLBW        mmxreg,mmxrm             PENT,MMX
    PUNPCKLDQ        mmxreg,mmxrm             PENT,MMX
    PUNPCKLWD        mmxreg,mmxrm             PENT,MMX
    PUSH             reg16                    8086
    PUSH             reg32                    386,NOLONG
    PUSH             reg64                    X64
    PUSH             rm16                     8086
    PUSH             rm32                     386,NOLONG
    PUSH             rm64                     X64
    PUSH             reg_cs                   8086,NOLONG
    PUSH             reg_dess                 8086,NOLONG
    PUSH             reg_fsgs                 386
    PUSH             imm8                     186
    PUSH             imm16                    186,AR0,SZ
    PUSH             imm32                    386,NOLONG,AR0,SZ
    PUSH             imm32                    386,NOLONG,SD
    PUSH             imm64                    X64,AR0,SZ
    PUSHA                                     186,NOLONG
    PUSHAD                                    386,NOLONG
    PUSHAW                                    186,NOLONG
    PUSHF                                     8086
    PUSHFD                                    386,NOLONG
    PUSHFQ                                    X64
    PUSHFW                                    8086
    PXOR             mmxreg,mmxrm             PENT,MMX
    RCL              rm8,unity                8086
    RCL              rm8,reg_cl               8086
    RCL              rm8,imm                  186
    RCL              rm16,unity               8086
    RCL              rm16,reg_cl              8086
    RCL              rm16,imm                 186
    RCL              rm32,unity               386
    RCL              rm32,reg_cl              386
    RCL              rm32,imm                 386
    RCL              rm64,unity               X64
    RCL              rm64,reg_cl              X64
    RCL              rm64,imm                 X64
    RCR              rm8,unity                8086
    RCR              rm8,reg_cl               8086
    RCR              rm8,imm                  186
    RCR              rm16,unity               8086
    RCR              rm16,reg_cl              8086
    RCR              rm16,imm                 186
    RCR              rm32,unity               386
    RCR              rm32,reg_cl              386
    RCR              rm32,imm                 386
    RCR              rm64,unity               X64
    RCR              rm64,reg_cl              X64
    RCR              rm64,imm                 X64
    RDSHR            rm32                     P6,CYRIXM
    RDMSR                                     PENT,PRIV
    RDPMC                                     P6
    RDTSC                                     PENT
    RDTSCP                                    X86_64
    RET                                       8086
    RET              imm                      8086,SW
    RETF                                      8086
    RETF             imm                      8086,SW
    RETN                                      8086
    RETN             imm                      8086,SW
    ROL              rm8,unity                8086
    ROL              rm8,reg_cl               8086
    ROL              rm8,imm                  186
    ROL              rm16,unity               8086
    ROL              rm16,reg_cl              8086
    ROL              rm16,imm                 186
    ROL              rm32,unity               386
    ROL              rm32,reg_cl              386
    ROL              rm32,imm                 386
    ROL              rm64,unity               X64
    ROL              rm64,reg_cl              X64
    ROL              rm64,imm                 X64
    ROR              rm8,unity                8086
    ROR              rm8,reg_cl               8086
    ROR              rm8,imm                  186
    ROR              rm16,unity               8086
    ROR              rm16,reg_cl              8086
    ROR              rm16,imm                 186
    ROR              rm32,unity               386
    ROR              rm32,reg_cl              386
    ROR              rm32,imm                 386
    ROR              rm64,unity               X64
    ROR              rm64,reg_cl              X64
    ROR              rm64,imm                 X64
    RDM                                       P6,CYRIX,ND
    RSDC             reg_sreg,mem80           486,CYRIXM
    RSLDT            mem80                    486,CYRIXM
    RSM                                       PENTM
    RSTS             mem80                    486,CYRIXM
    SAHF                                      8086
    SAL              rm8,unity                8086,ND
    SAL              rm8,reg_cl               8086,ND
    SAL              rm8,imm                  186,ND
    SAL              rm16,unity               8086,ND
    SAL              rm16,reg_cl              8086,ND
    SAL              rm16,imm                 186,ND
    SAL              rm32,unity               386,ND
    SAL              rm32,reg_cl              386,ND
    SAL              rm32,imm                 386,ND
    SAL              rm64,unity               X64,ND
    SAL              rm64,reg_cl              X64,ND
    SAL              rm64,imm                 X64,ND
    SALC                                      8086,UNDOC
    SAR              rm8,unity                8086
    SAR              rm8,reg_cl               8086
    SAR              rm8,imm                  186
    SAR              rm16,unity               8086
    SAR              rm16,reg_cl              8086
    SAR              rm16,imm                 186
    SAR              rm32,unity               386
    SAR              rm32,reg_cl              386
    SAR              rm32,imm                 386
    SAR              rm64,unity               X64
    SAR              rm64,reg_cl              X64
    SAR              rm64,imm                 X64
    SBB              mem,reg8                 8086
    SBB              reg8,reg8                8086
    SBB              mem,reg16                8086
    SBB              reg16,reg16              8086
    SBB              mem,reg32                386
    SBB              reg32,reg32              386
    SBB              mem,reg64                X64
    SBB              reg64,reg64              X64
    SBB              reg8,mem                 8086
    SBB              reg8,reg8                8086
    SBB              reg16,mem                8086
    SBB              reg16,reg16              8086
    SBB              reg32,mem                386
    SBB              reg32,reg32              386
    SBB              reg64,mem                X64
    SBB              reg64,reg64              X64
    SBB              rm16,imm8                8086
    SBB              rm32,imm8                386
    SBB              rm64,imm8                X64
    SBB              reg_al,imm               8086
    SBB              reg_ax,imm               8086
    SBB              reg_eax,imm              386
    SBB              reg_rax,imm              X64
    SBB              rm8,imm                  8086
    SBB              rm16,imm                 8086
    SBB              rm32,imm                 386
    SBB              rm64,imm                 X64
    SBB              mem,imm8                 8086
    SBB              mem,imm16                8086
    SBB              mem,imm32                386
    SCASB                                     8086
    SCASD                                     386
    SCASQ                                     X64
    SCASW                                     8086
    SFENCE                                    X64,AMD
    SGDT             mem                      286
    SHL              rm8,unity                8086
    SHL              rm8,reg_cl               8086
    SHL              rm8,imm                  186
    SHL              rm16,unity               8086
    SHL              rm16,reg_cl              8086
    SHL              rm16,imm                 186
    SHL              rm32,unity               386
    SHL              rm32,reg_cl              386
    SHL              rm32,imm                 386
    SHL              rm64,unity               X64
    SHL              rm64,reg_cl              X64
    SHL              rm64,imm                 X64
    SHLD             mem,reg16,imm            3862
    SHLD             reg16,reg16,imm          3862
    SHLD             mem,reg32,imm            3862
    SHLD             reg32,reg32,imm          3862
    SHLD             mem,reg64,imm            X642
    SHLD             reg64,reg64,imm          X642
    SHLD             mem,reg16,reg_cl         386
    SHLD             reg16,reg16,reg_cl       386
    SHLD             mem,reg32,reg_cl         386
    SHLD             reg32,reg32,reg_cl       386
    SHLD             mem,reg64,reg_cl         X64
    SHLD             reg64,reg64,reg_cl       X64
    SHR              rm8,unity                8086
    SHR              rm8,reg_cl               8086
    SHR              rm8,imm                  186
    SHR              rm16,unity               8086
    SHR              rm16,reg_cl              8086
    SHR              rm16,imm                 186
    SHR              rm32,unity               386
    SHR              rm32,reg_cl              386
    SHR              rm32,imm                 386
    SHR              rm64,unity               X64
    SHR              rm64,reg_cl              X64
    SHR              rm64,imm                 X64
    SHRD             mem,reg16,imm            3862
    SHRD             reg16,reg16,imm          3862
    SHRD             mem,reg32,imm            3862
    SHRD             reg32,reg32,imm          3862
    SHRD             mem,reg64,imm            X642
    SHRD             reg64,reg64,imm          X642
    SHRD             mem,reg16,reg_cl         386
    SHRD             reg16,reg16,reg_cl       386
    SHRD             mem,reg32,reg_cl         386
    SHRD             reg32,reg32,reg_cl       386
    SHRD             mem,reg64,reg_cl         X64
    SHRD             reg64,reg64,reg_cl       X64
    SIDT             mem                      286
    SLDT             mem                      286
    SLDT             mem16                    286
    SLDT             reg16                    286
    SLDT             reg32                    386
    SLDT             reg64                    X64,ND
    SLDT             reg64                    X64
    SKINIT                                    X64
    SMI                                       386,UNDOC
    SMINT                                     P6,CYRIX,ND
    SMINTOLD                                  486,CYRIX,ND
    SMSW             mem                      286
    SMSW             mem16                    286
    SMSW             reg16                    286
    SMSW             reg32                    386
    STC                                       8086
    STD                                       8086
    STGI                                      X64
    STI                                       8086
    STOSB                                     8086
    STOSD                                     386
    STOSQ                                     X64
    STOSW                                     8086
    STR              mem                      286,PROT
    STR              mem16                    286,PROT
    STR              reg16                    286,PROT
    STR              reg32                    386,PROT
    STR              reg64                    X64
    SUB              mem,reg8                 8086
    SUB              reg8,reg8                8086
    SUB              mem,reg16                8086
    SUB              reg16,reg16              8086
    SUB              mem,reg32                386
    SUB              reg32,reg32              386
    SUB              mem,reg64                X64
    SUB              reg64,reg64              X64
    SUB              reg8,mem                 8086
    SUB              reg8,reg8                8086
    SUB              reg16,mem                8086
    SUB              reg16,reg16              8086
    SUB              reg32,mem                386
    SUB              reg32,reg32              386
    SUB              reg64,mem                X64
    SUB              reg64,reg64              X64
    SUB              rm16,imm8                8086
    SUB              rm32,imm8                386
    SUB              rm64,imm8                X64
    SUB              reg_al,imm               8086
    SUB              reg_ax,imm               8086
    SUB              reg_eax,imm              386
    SUB              reg_rax,imm              X64
    SUB              rm8,imm                  8086
    SUB              rm16,imm                 8086
    SUB              rm32,imm                 386
    SUB              rm64,imm                 X64
    SUB              mem,imm8                 8086
    SUB              mem,imm16                8086
    SUB              mem,imm32                386
    SVDC             mem80,reg_sreg           486,CYRIXM
    SVLDT            mem80                    486,CYRIXM,ND
    SVTS             mem80                    486,CYRIXM
    SWAPGS                                    X64
    SYSCALL                                   P6,AMD
    SYSENTER                                  P6
    SYSEXIT                                   P6,PRIV
    SYSRET                                    P6,PRIV,AMD
    TEST             mem,reg8                 8086
    TEST             reg8,reg8                8086
    TEST             mem,reg16                8086
    TEST             reg16,reg16              8086
    TEST             mem,reg32                386
    TEST             reg32,reg32              386
    TEST             mem,reg64                X64
    TEST             reg64,reg64              X64
    TEST             reg8,mem                 8086
    TEST             reg16,mem                8086
    TEST             reg32,mem                386
    TEST             reg64,mem                X64
    TEST             reg_al,imm               8086
    TEST             reg_ax,imm               8086
    TEST             reg_eax,imm              386
    TEST             reg_rax,imm              X64
    TEST             rm8,imm                  8086
    TEST             rm16,imm                 8086
    TEST             rm32,imm                 386
    TEST             rm64,imm                 X64
    TEST             mem,imm8                 8086
    TEST             mem,imm16                8086
    TEST             mem,imm32                386
    UD0                                       186,UNDOC
    UD1                                       186,UNDOC
    UD2B                                      186,UNDOC,ND
    UD2                                       186
    UD2A                                      186,ND
    UMOV             mem,reg8                 386,UNDOC,ND
    UMOV             reg8,reg8                386,UNDOC,ND
    UMOV             mem,reg16                386,UNDOC,ND
    UMOV             reg16,reg16              386,UNDOC,ND
    UMOV             mem,reg32                386,UNDOC,ND
    UMOV             reg32,reg32              386,UNDOC,ND
    UMOV             reg8,mem                 386,UNDOC,ND
    UMOV             reg8,reg8                386,UNDOC,ND
    UMOV             reg16,mem                386,UNDOC,ND
    UMOV             reg16,reg16              386,UNDOC,ND
    UMOV             reg32,mem                386,UNDOC,ND
    UMOV             reg32,reg32              386,UNDOC,ND
    VERR             mem                      286,PROT
    VERR             mem16                    286,PROT
    VERR             reg16                    286,PROT
    VERW             mem                      286,PROT
    VERW             mem16                    286,PROT
    VERW             reg16                    286,PROT
    WAIT                                      8086
    FWAIT                                     8086
    WBINVD                                    486,PRIV
    WRSHR            rm32                     P6,CYRIXM
    WRMSR                                     PENT,PRIV
    XADD             mem,reg8                 486
    XADD             reg8,reg8                486
    XADD             mem,reg16                486
    XADD             reg16,reg16              486
    XADD             mem,reg32                486
    XADD             reg32,reg32              486
    XADD             mem,reg64                X64
    XADD             reg64,reg64              X64
    XBTS             reg16,mem                386,SW,UNDOC,ND
    XBTS             reg16,reg16              386,UNDOC,ND
    XBTS             reg32,mem                386,SD,UNDOC,ND
    XBTS             reg32,reg32              386,UNDOC,ND
    XCHG             reg_ax,reg16             8086
    XCHG             reg_eax,reg32na          386
    XCHG             reg_rax,reg64            X64
    XCHG             reg16,reg_ax             8086
    XCHG             reg32na,reg_eax          386
    XCHG             reg64,reg_rax            X64
    XCHG             reg_eax,reg_eax          386,NOLONG
    XCHG             reg8,mem                 8086
    XCHG             reg8,reg8                8086
    XCHG             reg16,mem                8086
    XCHG             reg16,reg16              8086
    XCHG             reg32,mem                386
    XCHG             reg32,reg32              386
    XCHG             reg64,mem                X64
    XCHG             reg64,reg64              X64
    XCHG             mem,reg8                 8086
    XCHG             reg8,reg8                8086
    XCHG             mem,reg16                8086
    XCHG             reg16,reg16              8086
    XCHG             mem,reg32                386
    XCHG             reg32,reg32              386
    XCHG             mem,reg64                X64
    XCHG             reg64,reg64              X64
    XLATB                                     8086
    XLAT                                      8086
    XOR              mem,reg8                 8086
    XOR              reg8,reg8                8086
    XOR              mem,reg16                8086
    XOR              reg16,reg16              8086
    XOR              mem,reg32                386
    XOR              reg32,reg32              386
    XOR              mem,reg64                X64
    XOR              reg64,reg64              X64
    XOR              reg8,mem                 8086
    XOR              reg8,reg8                8086
    XOR              reg16,mem                8086
    XOR              reg16,reg16              8086
    XOR              reg32,mem                386
    XOR              reg32,reg32              386
    XOR              reg64,mem                X64
    XOR              reg64,reg64              X64
    XOR              rm16,imm8                8086
    XOR              rm32,imm8                386
    XOR              rm64,imm8                X64
    XOR              reg_al,imm               8086
    XOR              reg_ax,imm               8086
    XOR              reg_eax,imm              386
    XOR              reg_rax,imm              X64
    XOR              rm8,imm                  8086
    XOR              rm16,imm                 8086
    XOR              rm32,imm                 386
    XOR              rm64,imm                 X64
    XOR              mem,imm8                 8086
    XOR              mem,imm16                8086
    XOR              mem,imm32                386
    CMOVcc           reg16,mem                P6
    CMOVcc           reg16,reg16              P6
    CMOVcc           reg32,mem                P6
    CMOVcc           reg32,reg32              P6
    CMOVcc           reg64,mem                X64
    CMOVcc           reg64,reg64              X64
    Jcc              imm|near                 386
    Jcc              imm16|near               386
    Jcc              imm32|near               386
    Jcc              imm|short                8086,ND
    Jcc              imm                      8086,ND
    Jcc              imm                      386,ND
    Jcc              imm                      8086,ND
    Jcc              imm                      8086
    SETcc            mem                      386
    SETcc            reg8                     386

#### B.1.3 Katmai Streaming SIMD instructions (SSE -- a.k.a. KNI, XMM, MMX2)

    ADDPS            xmmreg,xmmrm             KATMAI,SSE
    ADDSS            xmmreg,xmmrm             KATMAI,SSE,SD
    ANDNPS           xmmreg,xmmrm             KATMAI,SSE
    ANDPS            xmmreg,xmmrm             KATMAI,SSE
    CMPEQPS          xmmreg,xmmrm             KATMAI,SSE
    CMPEQSS          xmmreg,xmmrm             KATMAI,SSE
    CMPLEPS          xmmreg,xmmrm             KATMAI,SSE
    CMPLESS          xmmreg,xmmrm             KATMAI,SSE
    CMPLTPS          xmmreg,xmmrm             KATMAI,SSE
    CMPLTSS          xmmreg,xmmrm             KATMAI,SSE
    CMPNEQPS         xmmreg,xmmrm             KATMAI,SSE
    CMPNEQSS         xmmreg,xmmrm             KATMAI,SSE
    CMPNLEPS         xmmreg,xmmrm             KATMAI,SSE
    CMPNLESS         xmmreg,xmmrm             KATMAI,SSE
    CMPNLTPS         xmmreg,xmmrm             KATMAI,SSE
    CMPNLTSS         xmmreg,xmmrm             KATMAI,SSE
    CMPORDPS         xmmreg,xmmrm             KATMAI,SSE
    CMPORDSS         xmmreg,xmmrm             KATMAI,SSE
    CMPUNORDPS       xmmreg,xmmrm             KATMAI,SSE
    CMPUNORDSS       xmmreg,xmmrm             KATMAI,SSE
    CMPPS            xmmreg,mem,imm           KATMAI,SSE
    CMPPS            xmmreg,xmmreg,imm        KATMAI,SSE
    CMPSS            xmmreg,mem,imm           KATMAI,SSE
    CMPSS            xmmreg,xmmreg,imm        KATMAI,SSE
    COMISS           xmmreg,xmmrm             KATMAI,SSE
    CVTPI2PS         xmmreg,mmxrm             KATMAI,SSE,MMX
    CVTPS2PI         mmxreg,xmmrm             KATMAI,SSE,MMX
    CVTSI2SS         xmmreg,mem               KATMAI,SSE,SD,AR1,ND
    CVTSI2SS         xmmreg,rm32              KATMAI,SSE,SD,AR1
    CVTSI2SS         xmmreg,rm64              X64,SSE,AR1
    CVTSS2SI         reg32,xmmreg             KATMAI,SSE,SD,AR1
    CVTSS2SI         reg32,mem                KATMAI,SSE,SD,AR1
    CVTSS2SI         reg64,xmmreg             X64,SSE,SD,AR1
    CVTSS2SI         reg64,mem                X64,SSE,SD,AR1
    CVTTPS2PI        mmxreg,xmmrm             KATMAI,SSE,MMX
    CVTTSS2SI        reg32,xmmrm              KATMAI,SSE,SD,AR1
    CVTTSS2SI        reg64,xmmrm              X64,SSE,SD,AR1
    DIVPS            xmmreg,xmmrm             KATMAI,SSE
    DIVSS            xmmreg,xmmrm             KATMAI,SSE
    LDMXCSR          mem                      KATMAI,SSE,SD
    MAXPS            xmmreg,xmmrm             KATMAI,SSE
    MAXSS            xmmreg,xmmrm             KATMAI,SSE
    MINPS            xmmreg,xmmrm             KATMAI,SSE
    MINSS            xmmreg,xmmrm             KATMAI,SSE
    MOVAPS           xmmreg,mem               KATMAI,SSE
    MOVAPS           mem,xmmreg               KATMAI,SSE
    MOVAPS           xmmreg,xmmreg            KATMAI,SSE
    MOVAPS           xmmreg,xmmreg            KATMAI,SSE
    MOVHPS           xmmreg,mem               KATMAI,SSE
    MOVHPS           mem,xmmreg               KATMAI,SSE
    MOVLHPS          xmmreg,xmmreg            KATMAI,SSE
    MOVLPS           xmmreg,mem               KATMAI,SSE
    MOVLPS           mem,xmmreg               KATMAI,SSE
    MOVHLPS          xmmreg,xmmreg            KATMAI,SSE
    MOVMSKPS         reg32,xmmreg             KATMAI,SSE
    MOVMSKPS         reg64,xmmreg             X64,SSE
    MOVNTPS          mem,xmmreg               KATMAI,SSE
    MOVSS            xmmreg,mem               KATMAI,SSE
    MOVSS            mem,xmmreg               KATMAI,SSE
    MOVSS            xmmreg,xmmreg            KATMAI,SSE
    MOVSS            xmmreg,xmmreg            KATMAI,SSE
    MOVUPS           xmmreg,mem               KATMAI,SSE
    MOVUPS           mem,xmmreg               KATMAI,SSE
    MOVUPS           xmmreg,xmmreg            KATMAI,SSE
    MOVUPS           xmmreg,xmmreg            KATMAI,SSE
    MULPS            xmmreg,xmmrm             KATMAI,SSE
    MULSS            xmmreg,xmmrm             KATMAI,SSE
    ORPS             xmmreg,xmmrm             KATMAI,SSE
    RCPPS            xmmreg,xmmrm             KATMAI,SSE
    RCPSS            xmmreg,xmmrm             KATMAI,SSE
    RSQRTPS          xmmreg,xmmrm             KATMAI,SSE
    RSQRTSS          xmmreg,xmmrm             KATMAI,SSE
    SHUFPS           xmmreg,mem,imm           KATMAI,SSE
    SHUFPS           xmmreg,xmmreg,imm        KATMAI,SSE
    SQRTPS           xmmreg,xmmrm             KATMAI,SSE
    SQRTSS           xmmreg,xmmrm             KATMAI,SSE
    STMXCSR          mem                      KATMAI,SSE,SD
    SUBPS            xmmreg,xmmrm             KATMAI,SSE
    SUBSS            xmmreg,xmmrm             KATMAI,SSE
    UCOMISS          xmmreg,xmmrm             KATMAI,SSE
    UNPCKHPS         xmmreg,xmmrm             KATMAI,SSE
    UNPCKLPS         xmmreg,xmmrm             KATMAI,SSE
    XORPS            xmmreg,xmmrm             KATMAI,SSE

#### B.1.4 Introduced in Deschutes but necessary for SSE support

    FXRSTOR          mem                      P6,SSE,FPU
    FXSAVE           mem                      P6,SSE,FPU

#### B.1.5 XSAVE group (AVX and extended state)

    XGETBV                                    NEHALEM
    XSETBV                                    NEHALEM,PRIV
    XSAVE            mem                      NEHALEM
    XRSTOR           mem                      NEHALEM

#### B.1.6 Generic memory operations

    PREFETCHNTA      mem                      KATMAI
    PREFETCHT0       mem                      KATMAI
    PREFETCHT1       mem                      KATMAI
    PREFETCHT2       mem                      KATMAI
    SFENCE                                    KATMAI

#### B.1.7 New MMX instructions introduced in Katmai

    MASKMOVQ         mmxreg,mmxreg            KATMAI,MMX
    MOVNTQ           mem,mmxreg               KATMAI,MMX
    PAVGB            mmxreg,mmxrm             KATMAI,MMX
    PAVGW            mmxreg,mmxrm             KATMAI,MMX
    PEXTRW           reg32,mmxreg,imm         KATMAI,MMX
    PINSRW           mmxreg,reg16,imm         KATMAI,MMX
    PINSRW           mmxreg,reg32,imm         KATMAI,MMX,ND
    PINSRW           mmxreg,mem,imm           KATMAI,MMX
    PINSRW           mmxreg,mem16,imm         KATMAI,MMX,ND
    PMAXSW           mmxreg,mmxrm             KATMAI,MMX
    PMAXUB           mmxreg,mmxrm             KATMAI,MMX
    PMINSW           mmxreg,mmxrm             KATMAI,MMX
    PMINUB           mmxreg,mmxrm             KATMAI,MMX
    PMOVMSKB         reg32,mmxreg             KATMAI,MMX
    PMULHUW          mmxreg,mmxrm             KATMAI,MMX
    PSADBW           mmxreg,mmxrm             KATMAI,MMX
    PSHUFW           mmxreg,mmxrm,imm         KATMAI,MMX2

#### B.1.8 AMD Enhanced 3DNow! (Athlon) instructions

    PF2IW            mmxreg,mmxrm             PENT,3DNOW
    PFNACC           mmxreg,mmxrm             PENT,3DNOW
    PFPNACC          mmxreg,mmxrm             PENT,3DNOW
    PI2FW            mmxreg,mmxrm             PENT,3DNOW
    PSWAPD           mmxreg,mmxrm             PENT,3DNOW

#### B.1.9 Willamette SSE2 Cacheability Instructions

    MASKMOVDQU       xmmreg,xmmreg            WILLAMETTE,SSE2
    CLFLUSH          mem                      WILLAMETTE,SSE2
    MOVNTDQ          mem,xmmreg               WILLAMETTE,SSE2,SO
    MOVNTI           mem,reg32                WILLAMETTE,SD
    MOVNTI           mem,reg64                X64
    MOVNTPD          mem,xmmreg               WILLAMETTE,SSE2,SO
    LFENCE                                    WILLAMETTE,SSE2
    MFENCE                                    WILLAMETTE,SSE2

#### B.1.10 Willamette MMX instructions (SSE2 SIMD Integer Instructions)

    MOVD             xmmreg,reg32             WILLAMETTE,SSE2
    MOVD             reg32,xmmreg             WILLAMETTE,SSE2
    MOVD             mem,xmmreg               WILLAMETTE,SSE2,SD
    MOVD             xmmreg,mem               WILLAMETTE,SSE2,SD
    MOVDQA           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVDQA           mem,xmmreg               WILLAMETTE,SSE2,SO
    MOVDQA           xmmreg,mem               WILLAMETTE,SSE2,SO
    MOVDQA           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVDQU           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVDQU           mem,xmmreg               WILLAMETTE,SSE2,SO
    MOVDQU           xmmreg,mem               WILLAMETTE,SSE2,SO
    MOVDQU           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVDQ2Q          mmxreg,xmmreg            WILLAMETTE,SSE2
    MOVQ             xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVQ             xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVQ             mem,xmmreg               WILLAMETTE,SSE2
    MOVQ             xmmreg,mem               WILLAMETTE,SSE2
    MOVQ             xmmreg,rm64              X64,SSE2
    MOVQ             rm64,xmmreg              X64,SSE2
    MOVQ2DQ          xmmreg,mmxreg            WILLAMETTE,SSE2
    PACKSSWB         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PACKSSDW         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PACKUSWB         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDB            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDQ            mmxreg,mmxrm             WILLAMETTE,SSE2,SO
    PADDQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDSB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDUSB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PADDUSW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PAND             xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PANDN            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PAVGB            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PAVGW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PCMPEQB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PCMPEQW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PCMPEQD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PCMPGTB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PCMPGTW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PCMPGTD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PEXTRW           reg32,xmmreg,imm         WILLAMETTE,SSE2
    PINSRW           xmmreg,reg16,imm         WILLAMETTE,SSE2
    PINSRW           xmmreg,reg32,imm         WILLAMETTE,SSE2,ND
    PINSRW           xmmreg,mem,imm           WILLAMETTE,SSE2
    PINSRW           xmmreg,mem16,imm         WILLAMETTE,SSE2,ND
    PMADDWD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMAXSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMAXUB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMINSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMINUB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMOVMSKB         reg32,xmmreg             WILLAMETTE,SSE2
    PMULHUW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMULHW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMULLW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PMULUDQ          mmxreg,mmxrm             WILLAMETTE,SSE2,SO
    PMULUDQ          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    POR              xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSADBW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSHUFD           xmmreg,xmmreg,imm        WILLAMETTE,SSE2
    PSHUFD           xmmreg,mem,imm           WILLAMETTE,SSE22
    PSHUFHW          xmmreg,xmmreg,imm        WILLAMETTE,SSE2
    PSHUFHW          xmmreg,mem,imm           WILLAMETTE,SSE22
    PSHUFLW          xmmreg,xmmreg,imm        WILLAMETTE,SSE2
    PSHUFLW          xmmreg,mem,imm           WILLAMETTE,SSE22
    PSLLDQ           xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSLLW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSLLW            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSLLD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSLLD            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSLLQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSLLQ            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSRAW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSRAW            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSRAD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSRAD            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSRLDQ           xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSRLW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSRLW            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSRLD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSRLD            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSRLQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSRLQ            xmmreg,imm               WILLAMETTE,SSE2,AR1
    PSUBB            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSUBW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSUBD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSUBQ            mmxreg,mmxrm             WILLAMETTE,SSE2,SO
    PSUBQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSUBSB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSUBSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSUBUSB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PSUBUSW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKHBW        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKHWD        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKHDQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKHQDQ       xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKLBW        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKLWD        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKLDQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PUNPCKLQDQ       xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    PXOR             xmmreg,xmmrm             WILLAMETTE,SSE2,SO

#### B.1.11 Willamette Streaming SIMD instructions (SSE2)

    ADDPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    ADDSD            xmmreg,xmmrm             WILLAMETTE,SSE2
    ANDNPD           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    ANDPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPEQPD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPEQSD          xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPLEPD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPLESD          xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPLTPD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPLTSD          xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPNEQPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPNEQSD         xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPNLEPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPNLESD         xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPNLTPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPNLTSD         xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPORDPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPORDSD         xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPUNORDPD       xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CMPUNORDSD       xmmreg,xmmrm             WILLAMETTE,SSE2
    CMPPD            xmmreg,xmmrm,imm         WILLAMETTE,SSE22
    CMPSD            xmmreg,xmmrm,imm         WILLAMETTE,SSE2
    COMISD           xmmreg,xmmrm             WILLAMETTE,SSE2
    CVTDQ2PD         xmmreg,xmmrm             WILLAMETTE,SSE2
    CVTDQ2PS         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTPD2DQ         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTPD2PI         mmxreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTPD2PS         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTPI2PD         xmmreg,mmxrm             WILLAMETTE,SSE2
    CVTPS2DQ         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTPS2PD         xmmreg,xmmrm             WILLAMETTE,SSE2
    CVTSD2SI         reg32,xmmreg             WILLAMETTE,SSE2,AR1
    CVTSD2SI         reg32,mem                WILLAMETTE,SSE2,AR1
    CVTSD2SI         reg64,xmmreg             X64,SSE2,AR1
    CVTSD2SI         reg64,mem                X64,SSE2,AR1
    CVTSD2SS         xmmreg,xmmrm             WILLAMETTE,SSE2
    CVTSI2SD         xmmreg,mem               WILLAMETTE,SSE2,SD,AR1,ND
    CVTSI2SD         xmmreg,rm32              WILLAMETTE,SSE2,SD,AR1
    CVTSI2SD         xmmreg,rm64              X64,SSE2,AR1
    CVTSS2SD         xmmreg,xmmrm             WILLAMETTE,SSE2,SD
    CVTTPD2PI        mmxreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTTPD2DQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTTPS2DQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    CVTTSD2SI        reg32,xmmreg             WILLAMETTE,SSE2,AR1
    CVTTSD2SI        reg32,mem                WILLAMETTE,SSE2,AR1
    CVTTSD2SI        reg64,xmmreg             X64,SSE2,AR1
    CVTTSD2SI        reg64,mem                X64,SSE2,AR1
    DIVPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    DIVSD            xmmreg,xmmrm             WILLAMETTE,SSE2
    MAXPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    MAXSD            xmmreg,xmmrm             WILLAMETTE,SSE2
    MINPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    MINSD            xmmreg,xmmrm             WILLAMETTE,SSE2
    MOVAPD           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVAPD           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVAPD           mem,xmmreg               WILLAMETTE,SSE2,SO
    MOVAPD           xmmreg,mem               WILLAMETTE,SSE2,SO
    MOVHPD           mem,xmmreg               WILLAMETTE,SSE2
    MOVHPD           xmmreg,mem               WILLAMETTE,SSE2
    MOVLPD           mem,xmmreg               WILLAMETTE,SSE2
    MOVLPD           xmmreg,mem               WILLAMETTE,SSE2
    MOVMSKPD         reg32,xmmreg             WILLAMETTE,SSE2
    MOVMSKPD         reg64,xmmreg             X64,SSE2
    MOVSD            xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVSD            xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVSD            mem,xmmreg               WILLAMETTE,SSE2
    MOVSD            xmmreg,mem               WILLAMETTE,SSE2
    MOVUPD           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVUPD           xmmreg,xmmreg            WILLAMETTE,SSE2
    MOVUPD           mem,xmmreg               WILLAMETTE,SSE2,SO
    MOVUPD           xmmreg,mem               WILLAMETTE,SSE2,SO
    MULPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    MULSD            xmmreg,xmmrm             WILLAMETTE,SSE2
    ORPD             xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    SHUFPD           xmmreg,xmmreg,imm        WILLAMETTE,SSE2
    SHUFPD           xmmreg,mem,imm           WILLAMETTE,SSE2
    SQRTPD           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    SQRTSD           xmmreg,xmmrm             WILLAMETTE,SSE2
    SUBPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    SUBSD            xmmreg,xmmrm             WILLAMETTE,SSE2
    UCOMISD          xmmreg,xmmrm             WILLAMETTE,SSE2
    UNPCKHPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    UNPCKLPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
    XORPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO

#### B.1.12 Prescott New Instructions (SSE3)

    ADDSUBPD         xmmreg,xmmrm             PRESCOTT,SSE3,SO
    ADDSUBPS         xmmreg,xmmrm             PRESCOTT,SSE3,SO
    HADDPD           xmmreg,xmmrm             PRESCOTT,SSE3,SO
    HADDPS           xmmreg,xmmrm             PRESCOTT,SSE3,SO
    HSUBPD           xmmreg,xmmrm             PRESCOTT,SSE3,SO
    HSUBPS           xmmreg,xmmrm             PRESCOTT,SSE3,SO
    LDDQU            xmmreg,mem               PRESCOTT,SSE3,SO
    MOVDDUP          xmmreg,xmmrm             PRESCOTT,SSE3
    MOVSHDUP         xmmreg,xmmrm             PRESCOTT,SSE3
    MOVSLDUP         xmmreg,xmmrm             PRESCOTT,SSE3

#### B.1.13 VMX Instructions

    VMCALL                                    VMX
    VMCLEAR          mem                      VMX
    VMLAUNCH                                  VMX
    VMLOAD                                    X64,VMX
    VMMCALL                                   X64,VMX
    VMPTRLD          mem                      VMX
    VMPTRST          mem                      VMX
    VMREAD           rm32,reg32               VMX,NOLONG,SD
    VMREAD           rm64,reg64               X64,VMX
    VMRESUME                                  VMX
    VMRUN                                     X64,VMX
    VMSAVE                                    X64,VMX
    VMWRITE          reg32,rm32               VMX,NOLONG,SD
    VMWRITE          reg64,rm64               X64,VMX
    VMXOFF                                    VMX
    VMXON            mem                      VMX

#### B.1.14 Extended Page Tables VMX instructions

    INVEPT           reg32,mem                VMX,SO,NOLONG
    INVEPT           reg64,mem                VMX,SO,LONG
    INVVPID          reg32,mem                VMX,SO,NOLONG
    INVVPID          reg64,mem                VMX,SO,LONG

#### B.1.15 Tejas New Instructions (SSSE3)

    PABSB            mmxreg,mmxrm             SSSE3,MMX
    PABSB            xmmreg,xmmrm             SSSE3
    PABSW            mmxreg,mmxrm             SSSE3,MMX
    PABSW            xmmreg,xmmrm             SSSE3
    PABSD            mmxreg,mmxrm             SSSE3,MMX
    PABSD            xmmreg,xmmrm             SSSE3
    PALIGNR          mmxreg,mmxrm,imm         SSSE3,MMX
    PALIGNR          xmmreg,xmmrm,imm         SSSE3
    PHADDW           mmxreg,mmxrm             SSSE3,MMX
    PHADDW           xmmreg,xmmrm             SSSE3
    PHADDD           mmxreg,mmxrm             SSSE3,MMX
    PHADDD           xmmreg,xmmrm             SSSE3
    PHADDSW          mmxreg,mmxrm             SSSE3,MMX
    PHADDSW          xmmreg,xmmrm             SSSE3
    PHSUBW           mmxreg,mmxrm             SSSE3,MMX
    PHSUBW           xmmreg,xmmrm             SSSE3
    PHSUBD           mmxreg,mmxrm             SSSE3,MMX
    PHSUBD           xmmreg,xmmrm             SSSE3
    PHSUBSW          mmxreg,mmxrm             SSSE3,MMX
    PHSUBSW          xmmreg,xmmrm             SSSE3
    PMADDUBSW        mmxreg,mmxrm             SSSE3,MMX
    PMADDUBSW        xmmreg,xmmrm             SSSE3
    PMULHRSW         mmxreg,mmxrm             SSSE3,MMX
    PMULHRSW         xmmreg,xmmrm             SSSE3
    PSHUFB           mmxreg,mmxrm             SSSE3,MMX
    PSHUFB           xmmreg,xmmrm             SSSE3
    PSIGNB           mmxreg,mmxrm             SSSE3,MMX
    PSIGNB           xmmreg,xmmrm             SSSE3
    PSIGNW           mmxreg,mmxrm             SSSE3,MMX
    PSIGNW           xmmreg,xmmrm             SSSE3
    PSIGND           mmxreg,mmxrm             SSSE3,MMX
    PSIGND           xmmreg,xmmrm             SSSE3

#### B.1.16 AMD SSE4A

    EXTRQ            xmmreg,imm,imm           SSE4A,AMD
    EXTRQ            xmmreg,xmmreg            SSE4A,AMD
    INSERTQ          xmmreg,xmmreg,imm,imm    SSE4A,AMD
    INSERTQ          xmmreg,xmmreg            SSE4A,AMD
    MOVNTSD          mem,xmmreg               SSE4A,AMD
    MOVNTSS          mem,xmmreg               SSE4A,AMD,SD

#### B.1.17 New instructions in Barcelona

    LZCNT            reg16,rm16               P6,AMD
    LZCNT            reg32,rm32               P6,AMD
    LZCNT            reg64,rm64               P6,AMD

#### B.1.18 Penryn New Instructions (SSE4.1)

    BLENDPD          xmmreg,xmmrm,imm         SSE41
    BLENDPS          xmmreg,xmmrm,imm         SSE41
    BLENDVPD         xmmreg,xmmrm,xmm0        SSE41
    BLENDVPS         xmmreg,xmmrm,xmm0        SSE41
    DPPD             xmmreg,xmmrm,imm         SSE41
    DPPS             xmmreg,xmmrm,imm         SSE41
    EXTRACTPS        rm32,xmmreg,imm          SSE41
    EXTRACTPS        reg64,xmmreg,imm         SSE41,X64
    INSERTPS         xmmreg,xmmrm,imm         SSE41,SD
    MOVNTDQA         xmmreg,mem               SSE41
    MPSADBW          xmmreg,xmmrm,imm         SSE41
    PACKUSDW         xmmreg,xmmrm             SSE41
    PBLENDVB         xmmreg,xmmrm,xmm0        SSE41
    PBLENDW          xmmreg,xmmrm,imm         SSE41
    PCMPEQQ          xmmreg,xmmrm             SSE41
    PEXTRB           reg32,xmmreg,imm         SSE41
    PEXTRB           mem8,xmmreg,imm          SSE41
    PEXTRB           reg64,xmmreg,imm         SSE41,X64
    PEXTRD           rm32,xmmreg,imm          SSE41
    PEXTRQ           rm64,xmmreg,imm          SSE41,X64
    PEXTRW           reg32,xmmreg,imm         SSE41
    PEXTRW           mem16,xmmreg,imm         SSE41
    PEXTRW           reg64,xmmreg,imm         SSE41,X64
    PHMINPOSUW       xmmreg,xmmrm             SSE41
    PINSRB           xmmreg,reg32,imm         SSE41
    PINSRB           xmmreg,mem8,imm          SSE41
    PINSRD           xmmreg,rm32,imm          SSE41
    PINSRQ           xmmreg,rm64,imm          SSE41,X64
    PMAXSB           xmmreg,xmmrm             SSE41
    PMAXSD           xmmreg,xmmrm             SSE41
    PMAXUD           xmmreg,xmmrm             SSE41
    PMAXUW           xmmreg,xmmrm             SSE41
    PMINSB           xmmreg,xmmrm             SSE41
    PMINSD           xmmreg,xmmrm             SSE41
    PMINUD           xmmreg,xmmrm             SSE41
    PMINUW           xmmreg,xmmrm             SSE41
    PMOVSXBW         xmmreg,xmmrm             SSE41
    PMOVSXBD         xmmreg,xmmrm             SSE41,SD
    PMOVSXBQ         xmmreg,xmmrm             SSE41,SW
    PMOVSXWD         xmmreg,xmmrm             SSE41
    PMOVSXWQ         xmmreg,xmmrm             SSE41,SD
    PMOVSXDQ         xmmreg,xmmrm             SSE41
    PMOVZXBW         xmmreg,xmmrm             SSE41
    PMOVZXBD         xmmreg,xmmrm             SSE41,SD
    PMOVZXBQ         xmmreg,xmmrm             SSE41,SW
    PMOVZXWD         xmmreg,xmmrm             SSE41
    PMOVZXWQ         xmmreg,xmmrm             SSE41,SD
    PMOVZXDQ         xmmreg,xmmrm             SSE41
    PMULDQ           xmmreg,xmmrm             SSE41
    PMULLD           xmmreg,xmmrm             SSE41
    PTEST            xmmreg,xmmrm             SSE41
    ROUNDPD          xmmreg,xmmrm,imm         SSE41
    ROUNDPS          xmmreg,xmmrm,imm         SSE41
    ROUNDSD          xmmreg,xmmrm,imm         SSE41
    ROUNDSS          xmmreg,xmmrm,imm         SSE41

#### B.1.19 Nehalem New Instructions (SSE4.2)

    CRC32            reg32,rm8                SSE42
    CRC32            reg32,rm16               SSE42
    CRC32            reg32,rm32               SSE42
    CRC32            reg64,rm8                SSE42,X64
    CRC32            reg64,rm64               SSE42,X64
    PCMPESTRI        xmmreg,xmmrm,imm         SSE42
    PCMPESTRM        xmmreg,xmmrm,imm         SSE42
    PCMPISTRI        xmmreg,xmmrm,imm         SSE42
    PCMPISTRM        xmmreg,xmmrm,imm         SSE42
    PCMPGTQ          xmmreg,xmmrm             SSE42
    POPCNT           reg16,rm16               NEHALEM
    POPCNT           reg32,rm32               NEHALEM
    POPCNT           reg64,rm32               NEHALEM,X64

#### B.1.20 AMD SSE5 instructions

    FMADDPS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMADDPS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMADDPS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMADDPS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FMADDPD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMADDPD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMADDPD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMADDPD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FMADDSS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMADDSS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMADDSS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMADDSS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FMADDSD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMADDSD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMADDSD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMADDSD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FMSUBPS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMSUBPS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMSUBPS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMSUBPS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FMSUBPD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMSUBPD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMSUBPD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMSUBPD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FMSUBSS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMSUBSS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMSUBSS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMSUBSS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FMSUBSD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FMSUBSD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FMSUBSD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FMSUBSD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMADDPS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMADDPS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMADDPS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMADDPS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMADDPD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMADDPD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMADDPD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMADDPD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMADDSS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMADDSS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMADDSS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMADDSS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMADDSD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMADDSD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMADDSD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMADDSD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMSUBPS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMSUBPS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMSUBPS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMSUBPS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMSUBPD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMSUBPD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMSUBPD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMSUBPD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMSUBSS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMSUBSS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMSUBSS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMSUBSS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    FNMSUBSD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    FNMSUBSD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    FNMSUBSD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    FNMSUBSD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    COMEQPS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMLTPS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMLEPS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNORDPS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNEQPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNLTPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNLEPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMORDPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUEQPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMULTPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMULEPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMFALSEPS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMNEQPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMNLTPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMNLEPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMTRUEPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMPS            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    COMEQPD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMLTPD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMLEPD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNORDPD       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNEQPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNLTPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUNLEPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMORDPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMUEQPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMULTPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMULEPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMFALSEPD       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMNEQPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMNLTPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMNLEPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMTRUEPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    COMPD            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    COMEQSS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMLTSS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMLESS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMUNORDSS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMUNEQSS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMUNLTSS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMUNLESS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMORDSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMUEQSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMULTSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMULESS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMFALSESS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMNEQSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMNLTSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMNLESS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMTRUESS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
    COMSS            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SD
    COMEQSD          xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMLTSD          xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMLESD          xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMUNORDSD       xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMUNEQSD        xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMUNLTSD        xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMUNLESD        xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMORDSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMUEQSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMULTSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMULESD         xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMFALSESD       xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMNEQSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMNLTSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMNLESD         xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMTRUESD        xmmreg,xmmreg,xmmrm      SSE5,AMD
    COMSD            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD
    PCOMLTB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLEB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGEB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSEB       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUEB        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMB            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PCOMLTW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLEW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGEW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSEW       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUEW        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMW            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PCOMLTD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLED          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGED          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSED       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUED        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMD            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PCOMLTQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLEQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGEQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSEQ       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUEQ        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMQ            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PCOMLTUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLEUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGEUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQUB        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSEUB      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUEUB       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMUB           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PCOMLTUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLEUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGEUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQUW        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSEUW      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUEUW       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMUW           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PCOMLTUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLEUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGEUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQUD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSEUD      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUEUD       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMUD           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PCOMLTUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMLEUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGTUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMGEUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMEQUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMNEQUQ        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMFALSEUQ      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMTRUEUQ       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
    PCOMUQ           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
    PERMPS           xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    PERMPS           xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    PERMPS           xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PERMPS           xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    PERMPD           xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    PERMPD           xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    PERMPD           xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PERMPD           xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    PCMOV            xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    PCMOV            xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    PCMOV            xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PCMOV            xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    PPERM            xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
    PPERM            xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
    PPERM            xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PPERM            xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
    PMACSSWW         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSWW          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSSWD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSWD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSSDD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSDD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSSDQL        xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSDQL         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSSDQH        xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMACSDQH         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMADCSSWD        xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PMADCSWD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
    PROTB            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PROTB            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PROTW            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PROTW            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PROTD            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PROTD            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PROTQ            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PROTQ            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHLB            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHLB            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHLW            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHLW            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHLD            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHLD            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHLQ            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHLQ            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHAB            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHAB            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHAW            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHAW            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHAD            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHAD            xmmreg,xmmrm,xmmreg      SSE5,AMD
    PSHAQ            xmmreg,xmmreg,xmmrm      SSE5,AMD
    PSHAQ            xmmreg,xmmrm,xmmreg      SSE5,AMD
    FRCZPS           xmmreg,xmmrm             SSE5,AMD
    FRCZPD           xmmreg,xmmrm             SSE5,AMD
    FRCZSS           xmmreg,xmmrm             SSE5,AMD
    FRCZSD           xmmreg,xmmrm             SSE5,AMD
    CVTPH2PS         xmmreg,xmmrm             SSE5,AMD
    CVTPS2PH         xmmrm,xmmreg             SSE5,AMD
    PHADDBW          xmmreg,xmmrm             SSE5,AMD
    PHADDBD          xmmreg,xmmrm             SSE5,AMD
    PHADDBQ          xmmreg,xmmrm             SSE5,AMD
    PHADDWD          xmmreg,xmmrm             SSE5,AMD
    PHADDWQ          xmmreg,xmmrm             SSE5,AMD
    PHADDDQ          xmmreg,xmmrm             SSE5,AMD
    PHADDUBW         xmmreg,xmmrm             SSE5,AMD
    PHADDUBD         xmmreg,xmmrm             SSE5,AMD
    PHADDUBQ         xmmreg,xmmrm             SSE5,AMD
    PHADDUWD         xmmreg,xmmrm             SSE5,AMD
    PHADDUWQ         xmmreg,xmmrm             SSE5,AMD
    PHADDUDQ         xmmreg,xmmrm             SSE5,AMD
    PHSUBBW          xmmreg,xmmrm             SSE5,AMD
    PHSUBWD          xmmreg,xmmrm             SSE5,AMD
    PHSUBDQ          xmmreg,xmmrm             SSE5,AMD
    PROTB            xmmreg,xmmrm,imm         SSE5,AMD
    PROTW            xmmreg,xmmrm,imm         SSE5,AMD
    PROTD            xmmreg,xmmrm,imm         SSE5,AMD
    PROTQ            xmmreg,xmmrm,imm         SSE5,AMD
    ROUNDPS          xmmreg,xmmrm,imm         SSE5,AMD
    ROUNDPD          xmmreg,xmmrm,imm         SSE5,AMD
    ROUNDSS          xmmreg,xmmrm,imm         SSE5,AMD
    ROUNDSD          xmmreg,xmmrm,imm         SSE5,AMD

#### B.1.21 Intel SMX

    GETSEC                                    KATMAI

#### B.1.22 Geode (Cyrix) 3DNow! additions

    PFRCPV           mmxreg,mmxrm             PENT,3DNOW,CYRIX
    PFRSQRTV         mmxreg,mmxrm             PENT,3DNOW,CYRIX

#### B.1.23 Intel new instructions in ???

    MOVBE            reg16,mem16              NEHALEM
    MOVBE            reg32,mem32              NEHALEM
    MOVBE            reg64,mem64              NEHALEM
    MOVBE            mem16,reg16              NEHALEM
    MOVBE            mem32,reg32              NEHALEM
    MOVBE            mem64,reg64              NEHALEM

#### B.1.24 Intel AES instructions

    AESENC           xmmreg,xmmrm             WESTMERE,SO
    AESENCLAST       xmmreg,xmmrm             WESTMERE,SO
    AESDEC           xmmreg,xmmrm             WESTMERE,SO
    AESDECLAST       xmmreg,xmmrm             WESTMERE,SO
    AESIMC           xmmreg,xmmrm             WESTMERE,SO
    AESKEYGENASSIST  xmmreg,xmmrm,imm         WESTMERE,SO

#### B.1.25 Intel AVX AES instructions

    VAESENC          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VAESENC          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VAESENCLAST      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VAESENCLAST      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VAESDEC          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VAESDEC          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VAESDECLAST      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VAESDECLAST      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VAESIMC          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VAESKEYGENASSIST xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO

#### B.1.26 Intel AVX instructions

    VADDPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VADDPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VADDPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VADDPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VADDPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VADDPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VADDPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VADDPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VADDSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VADDSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
    VADDSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VADDSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VADDSUBPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VADDSUBPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VADDSUBPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VADDSUBPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VADDSUBPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VADDSUBPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VADDSUBPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VADDSUBPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VANDPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VANDPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VANDPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VANDPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VANDPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VANDPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VANDPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VANDPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VANDNPD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VANDNPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VANDNPD          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VANDNPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VANDNPS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VANDNPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VANDNPS          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VANDNPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VBLENDPD         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VBLENDPD         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VBLENDPD         ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VBLENDPD         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VBLENDPS         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VBLENDPS         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VBLENDPS         ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VBLENDPS         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VBLENDVPD        xmmreg,xmmreg,xmmrm,xmmrm AVX,SANDYBRIDGE,SO
    VBLENDVPD        xmmreg,xmmrm,xmm0        AVX,SANDYBRIDGE,SO
    VBLENDVPD        ymmreg,ymmreg,ymmrm,ymmrm AVX,SANDYBRIDGE,SY
    VBLENDVPD        ymmreg,ymmrm,ymm0        AVX,SANDYBRIDGE,SY
    VBLENDVPS        xmmreg,xmmreg,xmmrm,xmmrm AVX,SANDYBRIDGE,SO
    VBLENDVPS        xmmreg,xmmrm,xmm0        AVX,SANDYBRIDGE,SO
    VBLENDVPS        ymmreg,ymmreg,ymmrm,ymmrm AVX,SANDYBRIDGE,SY
    VBLENDVPD        ymmreg,ymmrm,ymm0        AVX,SANDYBRIDGE,SY
    VBROADCASTSS     xmmreg,mem               AVX,SANDYBRIDGE,SD
    VBROADCASTSS     ymmreg,mem               AVX,SANDYBRIDGE,SD
    VBROADCASTSD     ymmreg,mem               AVX,SANDYBRIDGE
    VBROADCASTF128   ymmreg,mem               AVX,SANDYBRIDGE,SO
    VCMPEQPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLTPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLTPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLTPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLTPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLEPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLEPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLEPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLEPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPUNORDPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPUNORDPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPUNORDPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPUNORDPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLTPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLTPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLTPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLTPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLEPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLEPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLEPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLEPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPORDPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPORDPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPORDPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPORDPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPEQ_UQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQ_UQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQ_UQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQ_UQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGEPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGEPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGEPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGEPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGTPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGTPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGTPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGTPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPFALSEPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPFALSEPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPFALSEPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPFALSEPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQ_OQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQ_OQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQ_OQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQ_OQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGEPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGEPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGEPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGEPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGTPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGTPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGTPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGTPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPTRUEPD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPTRUEPD       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPTRUEPD       ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPTRUEPD       ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPEQ_OSPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQ_OSPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQ_OSPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQ_OSPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLT_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLT_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLT_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLT_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLE_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLE_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLE_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLE_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPUNORD_SPD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPUNORD_SPD    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPUNORD_SPD    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPUNORD_SPD    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQ_USPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQ_USPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQ_USPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQ_USPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLT_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLT_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLT_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLT_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLE_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLE_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLE_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLE_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPORD_SPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPORD_SPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPORD_SPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPORS_SPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPEQ_USPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQ_USPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQ_USPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQ_USPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGE_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGE_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGE_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGE_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGT_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGT_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGT_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGT_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPFALSE_OSPD   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPFALSE_OSPD   xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPFALSE_OSPD   ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPFALSE_OSPD   ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQ_OSPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQ_OSPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQ_OSPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQ_OSPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGE_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGE_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGE_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGE_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGT_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGT_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGT_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGT_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPTRUE_USPD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPTRUE_USPD    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPTRUE_USPD    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPTRUE_USPD    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPPD           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VCMPPD           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VCMPPD           ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VCMPPD           ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VCMPEQPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLTPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLTPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLTPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLTPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLEPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLEPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLEPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLEPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPUNORDPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPUNORDPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPUNORDPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPUNORDPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLTPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLTPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLTPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLTPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLEPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLEPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLEPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLEPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPORDPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPORDPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPORDPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPORDPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPEQ_UQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQ_UQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQ_UQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQ_UQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGEPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGEPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGEPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGEPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGTPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGTPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGTPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGTPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPFALSEPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPFALSEPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPFALSEPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPFALSEPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQ_OQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQ_OQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQ_OQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQ_OQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGEPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGEPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGEPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGEPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGTPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGTPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGTPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGTPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPTRUEPS       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPTRUEPS       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPTRUEPS       ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPTRUEPS       ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPEQ_OSPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQ_OSPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQ_OSPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQ_OSPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLT_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLT_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLT_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLT_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPLE_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPLE_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPLE_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPLE_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPUNORD_SPS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPUNORD_SPS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPUNORD_SPS    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPUNORD_SPS    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQ_USPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQ_USPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQ_USPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQ_USPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLT_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLT_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLT_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLT_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNLE_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNLE_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNLE_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNLE_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPORD_SPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPORD_SPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPORD_SPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPORS_SPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPEQ_USPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPEQ_USPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPEQ_USPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPEQ_USPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGE_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGE_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGE_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGE_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNGT_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNGT_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNGT_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNGT_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPFALSE_OSPS   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPFALSE_OSPS   xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPFALSE_OSPS   ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPFALSE_OSPS   ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPNEQ_OSPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPNEQ_OSPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPNEQ_OSPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPNEQ_OSPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGE_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGE_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGE_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGE_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPGT_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPGT_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPGT_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPGT_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPTRUE_USPS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VCMPTRUE_USPS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCMPTRUE_USPS    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VCMPTRUE_USPS    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCMPPS           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VCMPPS           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VCMPPS           ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VCMPPS           ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VCMPEQSD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPEQSD         xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPLTSD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPLTSD         xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPLESD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPLESD         xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPUNORDSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPUNORDSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNEQSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNEQSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNLTSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNLTSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNLESD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNLESD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPORDSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPORDSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPEQ_UQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPEQ_UQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNGESD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNGESD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNGTSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNGTSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPFALSESD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPFALSESD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNEQ_OQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNEQ_OQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPGESD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPGESD         xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPGTSD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPGTSD         xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPTRUESD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPTRUESD       xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPEQ_OSSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPEQ_OSSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPLT_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPLT_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPLE_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPLE_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPUNORD_SSD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPUNORD_SSD    xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNEQ_USSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNEQ_USSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNLT_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNLT_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNLE_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNLE_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPORD_SSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPORD_SSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPEQ_USSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPEQ_USSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNGE_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNGE_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNGT_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNGT_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPFALSE_OSSD   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPFALSE_OSSD   xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPNEQ_OSSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPNEQ_OSSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPGE_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPGE_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPGT_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPGT_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPTRUE_USSD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCMPTRUE_USSD    xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCMPSD           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE
    VCMPSD           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE
    VCMPEQSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPEQSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPLTSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPLTSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPLESS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPLESS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPUNORDSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPUNORDSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNEQSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNEQSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNLTSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNLTSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNLESS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNLESS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPORDSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPORDSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPEQ_UQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPEQ_UQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNGESS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNGESS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNGTSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNGTSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPFALSESS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPFALSESS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNEQ_OQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNEQ_OQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPGESS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPGESS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPGTSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPGTSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPTRUESS       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPTRUESS       xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPEQ_OSSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPEQ_OSSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPLT_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPLT_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPLE_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPLE_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPUNORD_SSS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPUNORD_SSS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNEQ_USSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNEQ_USSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNLT_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNLT_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNLE_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNLE_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPORD_SSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPORD_SSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPEQ_USSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPEQ_USSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNGE_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNGE_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNGT_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNGT_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPFALSE_OSSS   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPFALSE_OSSS   xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPNEQ_OSSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPNEQ_OSSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPGE_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPGE_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPGT_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPGT_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPTRUE_USSS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCMPTRUE_USSS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCMPSS           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SD
    VCMPSS           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SD
    VCOMISD          xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCOMISS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCVTDQ2PD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCVTDQ2PD        ymmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCVTDQ2PS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCVTDQ2PS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCVTPD2DQ        xmmreg,xmmreg            AVX,SANDYBRIDGE
    VCVTPD2DQ        xmmreg,mem128            AVX,SANDYBRIDGE
    VCVTPD2DQ        xmmreg,ymmreg            AVX,SANDYBRIDGE
    VCVTPD2DQ        xmmreg,mem256            AVX,SANDYBRIDGE
    VCVTPD2PS        xmmreg,xmmreg            AVX,SANDYBRIDGE
    VCVTPD2PS        xmmreg,mem128            AVX,SANDYBRIDGE
    VCVTPD2PS        xmmreg,ymmreg            AVX,SANDYBRIDGE
    VCVTPD2PS        xmmreg,mem256            AVX,SANDYBRIDGE
    VCVTPS2DQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCVTPS2DQ        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCVTPS2PD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCVTPS2PD        ymmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCVTSD2SI        reg32,xmmrm              AVX,SANDYBRIDGE
    VCVTSD2SI        reg64,xmmrm              AVX,SANDYBRIDGE,LONG
    VCVTSD2SS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VCVTSD2SS        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VCVTSI2SD        xmmreg,xmmreg,rm32       AVX,SANDYBRIDGE
    VCVTSI2SD        xmmreg,rm32              AVX,SANDYBRIDGE
    VCVTSI2SD        xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SD,ND
    VCVTSI2SD        xmmreg,mem               AVX,SANDYBRIDGE,SD,ND
    VCVTSI2SD        xmmreg,xmmreg,rm64       AVX,SANDYBRIDGE,LONG
    VCVTSI2SD        xmmreg,rm64              AVX,SANDYBRIDGE,LONG
    VCVTSI2SS        xmmreg,xmmreg,rm32       AVX,SANDYBRIDGE
    VCVTSI2SS        xmmreg,rm32              AVX,SANDYBRIDGE
    VCVTSI2SS        xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SD,ND
    VCVTSI2SS        xmmreg,mem               AVX,SANDYBRIDGE,SD,ND
    VCVTSI2SS        xmmreg,xmmreg,rm64       AVX,SANDYBRIDGE,LONG
    VCVTSI2SS        xmmreg,rm64              AVX,SANDYBRIDGE,LONG
    VCVTSS2SD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VCVTSS2SD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VCVTSS2SI        reg32,xmmrm              AVX,SANDYBRIDGE,SD
    VCVTSS2SI        reg64,xmmrm              AVX,SANDYBRIDGE,SD,LONG
    VCVTTPD2DQ       xmmreg,xmmreg            AVX,SANDYBRIDGE
    VCVTTPD2DQ       xmmreg,mem128            AVX,SANDYBRIDGE
    VCVTTPD2DQ       xmmreg,ymmreg            AVX,SANDYBRIDGE
    VCVTTPD2DQ       xmmreg,mem256            AVX,SANDYBRIDGE
    VCVTTPS2DQ       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VCVTTPS2DQ       ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VCVTTSD2SI       reg32,xmmrm              AVX,SANDYBRIDGE
    VCVTTSD2SI       reg64,xmmrm              AVX,SANDYBRIDGE,LONG
    VCVTTSS2SI       reg32,xmmrm              AVX,SANDYBRIDGE,SD
    VCVTTSS2SI       reg64,xmmrm              AVX,SANDYBRIDGE,SD,LONG
    VDIVPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VDIVPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VDIVPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VDIVPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VDIVPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VDIVPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VDIVPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VDIVPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VDIVSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VDIVSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
    VDIVSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VDIVSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VDPPD            xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VDPPD            xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VDPPS            xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VDPPS            xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VDPPS            ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VDPPS            ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VEXTRACTF128     xmmrm,xmmreg,imm         AVX,SANDYBRIDGE,SO
    VEXTRACTPS       rm32,xmmreg,imm          AVX,SANDYBRIDGE,SD
    VHADDPD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VHADDPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VHADDPD          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VHADDPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VHADDPS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VHADDPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VHADDPS          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VHADDPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VHSUBPD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VHSUBPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VHSUBPD          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VHSUBPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VHSUBPS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VHSUBPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VHSUBPS          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VHSUBPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VINSERTF128      ymmreg,ymmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VINSERTPS        xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SD
    VINSERTPS        xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SD
    VLDDQU           xmmreg,mem               AVX,SANDYBRIDGE,SO
    VLDQQU           ymmreg,mem               AVX,SANDYBRIDGE,SY
    VLDDQU           ymmreg,mem               AVX,SANDYBRIDGE,SY
    VLDMXCSR         mem32                    AVX,SANDYBRIDGE,SD
    VMASKMOVDQU      xmmreg,xmmreg            AVX,SANDYBRIDGE
    VMASKMOVPS       xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SO
    VMASKMOVPS       ymmreg,ymmreg,mem        AVX,SANDYBRIDGE,SY
    VMASKMOVPS       mem,xmmreg,xmmreg        AVX,SANDYBRIDGE,SO
    VMASKMOVPS       mem,xmmreg,xmmreg        AVX,SANDYBRIDGE,SY
    VMASKMOVPD       xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SO
    VMASKMOVPD       ymmreg,ymmreg,mem        AVX,SANDYBRIDGE,SY
    VMASKMOVPD       mem,xmmreg,xmmreg        AVX,SANDYBRIDGE,SO
    VMASKMOVPD       mem,ymmreg,ymmreg        AVX,SANDYBRIDGE,SY
    VMAXPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VMAXPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMAXPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VMAXPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMAXPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VMAXPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMAXPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VMAXPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMAXSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VMAXSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
    VMAXSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VMAXSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VMINPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VMINPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMINPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VMINPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMINPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VMINPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMINPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VMINPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMINSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VMINSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
    VMINSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VMINSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VMOVAPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVAPD          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
    VMOVAPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVAPD          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMOVAPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVAPS          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
    VMOVAPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVAPS          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMOVQ            xmmreg,xmmrm             AVX,SANDYBRIDGE
    VMOVQ            xmmrm,xmmreg             AVX,SANDYBRIDGE
    VMOVD            xmmreg,rm32              AVX,SANDYBRIDGE,SD
    VMOVQ            xmmreg,rm64              AVX,SANDYBRIDGE,LONG
    VMOVD            rm32,xmmreg              AVX,SANDYBRIDGE,SD
    VMOVQ            rm64,xmmreg              AVX,SANDYBRIDGE,LONG
    VMOVDDUP         xmmreg,xmmrm             AVX,SANDYBRIDGE
    VMOVDDUP         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVDQA          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVDQA          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
    VMOVQQA          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVQQA          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMOVDQA          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVDQA          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMOVDQU          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVDQU          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
    VMOVQQU          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVQQU          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMOVDQU          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVDQU          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMOVHLPS         xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
    VMOVHLPS         xmmreg,xmmreg            AVX,SANDYBRIDGE
    VMOVHPD          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
    VMOVHPD          xmmreg,mem               AVX,SANDYBRIDGE
    VMOVHPD          mem,xmmreg               AVX,SANDYBRIDGE
    VMOVHPS          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
    VMOVHPS          xmmreg,mem               AVX,SANDYBRIDGE
    VMOVHPS          mem,xmmreg               AVX,SANDYBRIDGE
    VMOVLHPS         xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
    VMOVLHPS         xmmreg,xmmreg            AVX,SANDYBRIDGE
    VMOVLPD          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
    VMOVLPD          xmmreg,mem               AVX,SANDYBRIDGE
    VMOVLPD          mem,xmmreg               AVX,SANDYBRIDGE
    VMOVLPS          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
    VMOVLPS          xmmreg,mem               AVX,SANDYBRIDGE
    VMOVLPS          mem,xmmreg               AVX,SANDYBRIDGE
    VMOVMSKPD        reg64,xmmreg             AVX,SANDYBRIDGE,LONG
    VMOVMSKPD        reg32,xmmreg             AVX,SANDYBRIDGE
    VMOVMSKPD        reg64,ymmreg             AVX,SANDYBRIDGE,LONG
    VMOVMSKPD        reg32,ymmreg             AVX,SANDYBRIDGE
    VMOVMSKPS        reg64,xmmreg             AVX,SANDYBRIDGE,LONG
    VMOVMSKPS        reg32,xmmreg             AVX,SANDYBRIDGE
    VMOVMSKPS        reg64,ymmreg             AVX,SANDYBRIDGE,LONG
    VMOVMSKPS        reg32,ymmreg             AVX,SANDYBRIDGE
    VMOVNTDQ         mem,xmmreg               AVX,SANDYBRIDGE,SO
    VMOVNTQQ         mem,ymmreg               AVX,SANDYBRIDGE,SY
    VMOVNTDQ         mem,ymmreg               AVX,SANDYBRIDGE,SY
    VMOVNTDQA        xmmreg,mem               AVX,SANDYBRIDGE,SO
    VMOVNTPD         mem,xmmreg               AVX,SANDYBRIDGE,SO
    VMOVNTPD         mem,ymmreg               AVX,SANDYBRIDGE,SY
    VMOVNTPS         mem,xmmreg               AVX,SANDYBRIDGE,SO
    VMOVNTPS         mem,ymmreg               AVX,SANDYBRIDGE,SO
    VMOVSD           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
    VMOVSD           xmmreg,xmmreg            AVX,SANDYBRIDGE
    VMOVSD           xmmreg,mem               AVX,SANDYBRIDGE
    VMOVSD           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
    VMOVSD           xmmreg,xmmreg            AVX,SANDYBRIDGE
    VMOVSD           mem,xmmreg               AVX,SANDYBRIDGE
    VMOVSHDUP        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVSHDUP        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVSLDUP        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVSLDUP        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVSS           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
    VMOVSS           xmmreg,xmmreg            AVX,SANDYBRIDGE
    VMOVSS           xmmreg,mem               AVX,SANDYBRIDGE
    VMOVSS           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
    VMOVSS           xmmreg,xmmreg            AVX,SANDYBRIDGE
    VMOVSS           mem,xmmreg               AVX,SANDYBRIDGE
    VMOVUPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVUPD          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
    VMOVUPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVUPD          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMOVUPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMOVUPS          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
    VMOVUPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMOVUPS          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
    VMPSADBW         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VMPSADBW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VMULPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VMULPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMULPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VMULPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMULPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VMULPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VMULPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VMULPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VMULSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VMULSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
    VMULSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VMULSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VORPD            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VORPD            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VORPD            ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VORPD            ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VORPS            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VORPS            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VORPS            ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VORPS            ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VPABSB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPABSW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPABSD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPACKSSWB        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPACKSSWB        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPACKSSDW        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPACKSSDW        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPACKUSWB        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPACKUSWB        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPACKUSDW        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPACKUSDW        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDB           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDUSB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDUSB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPADDUSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPADDUSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPALIGNR         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VPALIGNR         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPAND            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPAND            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPANDN           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPANDN           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPAVGB           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPAVGB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPAVGW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPAVGW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPBLENDVB        xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
    VPBLENDVB        xmmreg,xmmrm,xmmreg      AVX,SANDYBRIDGE,SO
    VPBLENDW         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VPBLENDW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPCMPESTRI       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPCMPESTRM       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPCMPISTRI       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPCMPISTRM       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPCMPEQB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPEQB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPCMPEQW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPEQW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPCMPEQD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPEQD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPCMPEQQ         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPEQQ         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPCMPGTB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPGTB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPCMPGTW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPGTW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPCMPGTD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPGTD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPCMPGTQ         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPCMPGTQ         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPERMILPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPERMILPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VPERMILPD        xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPERMILPD        ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VPERMILTD2PD     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
    VPERMILTD2PD     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
    VPERMILTD2PD     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
    VPERMILTD2PD     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
    VPERMILMO2PD     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
    VPERMILMO2PD     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
    VPERMILMO2PD     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
    VPERMILMO2PD     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
    VPERMILMZ2PD     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
    VPERMILMZ2PD     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
    VPERMILMZ2PD     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
    VPERMILMZ2PD     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
    VPERMIL2PD       xmmreg,xmmreg,xmmrm,xmmreg,imm AVX,SANDYBRIDGE,SO
    VPERMIL2PD       xmmreg,xmmreg,xmmreg,xmmrm,imm AVX,SANDYBRIDGE,SO
    VPERMIL2PD       ymmreg,ymmreg,ymmrm,ymmreg,imm AVX,SANDYBRIDGE,SY
    VPERMIL2PD       ymmreg,ymmreg,ymmreg,ymmrm,imm AVX,SANDYBRIDGE,SY
    VPERMILPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPERMILPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VPERMILPS        xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPERMILPS        ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VPERMILTD2PS     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
    VPERMILTD2PS     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
    VPERMILTD2PS     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
    VPERMILTD2PS     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
    VPERMILMO2PS     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
    VPERMILMO2PS     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
    VPERMILMO2PS     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
    VPERMILMO2PS     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
    VPERMILMZ2PS     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
    VPERMILMZ2PS     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
    VPERMILMZ2PS     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
    VPERMILMZ2PS     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
    VPERMIL2PS       xmmreg,xmmreg,xmmrm,xmmreg,imm AVX,SANDYBRIDGE,SO
    VPERMIL2PS       xmmreg,xmmreg,xmmreg,xmmrm,imm AVX,SANDYBRIDGE,SO
    VPERMIL2PS       ymmreg,ymmreg,ymmrm,ymmreg,imm AVX,SANDYBRIDGE,SY
    VPERMIL2PS       ymmreg,ymmreg,ymmreg,ymmrm,imm AVX,SANDYBRIDGE,SY
    VPERM2F128       ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VPEXTRB          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
    VPEXTRB          reg32,xmmreg,imm         AVX,SANDYBRIDGE
    VPEXTRB          mem,xmmreg,imm           AVX,SANDYBRIDGE
    VPEXTRW          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
    VPEXTRW          reg32,xmmreg,imm         AVX,SANDYBRIDGE
    VPEXTRW          mem,xmmreg,imm           AVX,SANDYBRIDGE,SW
    VPEXTRW          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
    VPEXTRW          reg32,xmmreg,imm         AVX,SANDYBRIDGE
    VPEXTRW          mem,xmmreg,imm           AVX,SANDYBRIDGE,SW
    VPEXTRD          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
    VPEXTRD          rm32,xmmreg,imm          AVX,SANDYBRIDGE,SD
    VPEXTRQ          rm64,xmmreg,imm          AVX,SANDYBRIDGE,LONG
    VPHADDW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPHADDW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPHADDD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPHADDD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPHADDSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPHADDSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPHMINPOSUW      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPHSUBW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPHSUBW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPHSUBD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPHSUBD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPHSUBSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPHSUBSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPINSRB          xmmreg,xmmreg,reg32,imm  AVX,SANDYBRIDGE
    VPINSRB          xmmreg,reg32,imm         AVX,SANDYBRIDGE
    VPINSRB          xmmreg,xmmreg,mem,imm    AVX,SANDYBRIDGE
    VPINSRB          xmmreg,reg32,mem,imm     AVX,SANDYBRIDGE
    VPINSRW          xmmreg,xmmreg,reg32,imm  AVX,SANDYBRIDGE
    VPINSRW          xmmreg,reg32,imm         AVX,SANDYBRIDGE
    VPINSRW          xmmreg,xmmreg,mem,imm    AVX,SANDYBRIDGE,SW
    VPINSRW          xmmreg,reg32,mem,imm     AVX,SANDYBRIDGE,SW
    VPINSRD          xmmreg,xmmreg,rm32,imm   AVX,SANDYBRIDGE,SD
    VPINSRD          xmmreg,rm32,imm          AVX,SANDYBRIDGE,SD
    VPINSRQ          xmmreg,xmmreg,rm64,imm   AVX,SANDYBRIDGE,LONG
    VPINSRQ          xmmreg,rm64,imm          AVX,SANDYBRIDGE,SD,LONG
    VPMADDWD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMADDWD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMADDUBSW       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMADDUBSW       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMAXSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMAXSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMAXSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMAXSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMAXSD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMAXSD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMAXUB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMAXUB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMAXUW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMAXUW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMAXUD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMAXUD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMINSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMINSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMINSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMINSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMINSD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMINSD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMINUB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMINUB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMINUW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMINUW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMINUD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMINUD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMOVMSKB        reg64,xmmreg             AVX,SANDYBRIDGE,LONG
    VPMOVMSKB        reg32,xmmreg             AVX,SANDYBRIDGE
    VPMOVSXBW        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VPMOVSXBD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VPMOVSXBQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SW
    VPMOVSXWD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VPMOVSXWQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VPMOVSXDQ        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VPMOVZXBW        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VPMOVZXBD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VPMOVZXBQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SW
    VPMOVZXWD        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VPMOVZXWQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VPMOVZXDQ        xmmreg,xmmrm             AVX,SANDYBRIDGE
    VPMULHUW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMULHUW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMULHRSW        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMULHRSW        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMULHW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMULHW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMULLW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMULLW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMULLD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMULLD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMULUDQ         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMULUDQ         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPMULDQ          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPMULDQ          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPOR             xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPOR             xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSADBW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSADBW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSHUFB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSHUFB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSHUFD          xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPSHUFHW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPSHUFLW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VPSIGNB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSIGNB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSIGNW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSIGNW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSIGND          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSIGND          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSLLDQ          xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSLLDQ          xmmreg,imm               AVX,SANDYBRIDGE
    VPSRLDQ          xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSRLDQ          xmmreg,imm               AVX,SANDYBRIDGE
    VPSLLW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSLLW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSLLW           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSLLW           xmmreg,imm               AVX,SANDYBRIDGE
    VPSLLD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSLLD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSLLD           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSLLD           xmmreg,imm               AVX,SANDYBRIDGE
    VPSLLQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSLLQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSLLQ           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSLLQ           xmmreg,imm               AVX,SANDYBRIDGE
    VPSRAW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSRAW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSRAW           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSRAW           xmmreg,imm               AVX,SANDYBRIDGE
    VPSRAD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSRAD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSRAD           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSRAD           xmmreg,imm               AVX,SANDYBRIDGE
    VPSRLW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSRLW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSRLW           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSRLW           xmmreg,imm               AVX,SANDYBRIDGE
    VPSRLD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSRLD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSRLD           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSRLD           xmmreg,imm               AVX,SANDYBRIDGE
    VPSRLQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSRLQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSRLQ           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
    VPSRLQ           xmmreg,imm               AVX,SANDYBRIDGE
    VPTEST           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPTEST           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VPSUBB           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSUBW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSUBD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSUBQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSUBSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSUBSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSUBUSB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBUSB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPSUBUSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPSUBUSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKHBW       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKHBW       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKHWD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKHWD       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKHDQ       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKHDQ       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKHQDQ      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKHQDQ      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKLBW       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKLBW       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKLWD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKLWD       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKLDQ       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKLDQ       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPUNPCKLQDQ      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPUNPCKLQDQ      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VPXOR            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VPXOR            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VRCPPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VRCPPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VRCPSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VRCPSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VRSQRTPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VRSQRTPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VRSQRTSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VRSQRTSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VROUNDPD         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VROUNDPD         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VROUNDPS         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VROUNDPS         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VROUNDSD         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE
    VROUNDSD         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE
    VROUNDSS         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SD
    VROUNDSS         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SD
    VSHUFPD          xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VSHUFPD          xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VSHUFPD          ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VSHUFPD          ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VSHUFPS          xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
    VSHUFPS          xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
    VSHUFPS          ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
    VSHUFPS          ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
    VSQRTPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VSQRTPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VSQRTPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VSQRTPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VSQRTSD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VSQRTSD          xmmreg,xmmrm             AVX,SANDYBRIDGE
    VSQRTSS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VSQRTSS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VSTMXCSR         mem                      AVX,SANDYBRIDGE,SD
    VSUBPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VSUBPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VSUBPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VSUBPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VSUBPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VSUBPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VSUBPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VSUBPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VSUBSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
    VSUBSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
    VSUBSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
    VSUBSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VTESTPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VTESTPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VTESTPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VTESTPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VUCOMISD         xmmreg,xmmrm             AVX,SANDYBRIDGE
    VUCOMISS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
    VUNPCKHPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VUNPCKHPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VUNPCKHPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VUNPCKHPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VUNPCKHPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VUNPCKHPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VUNPCKHPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VUNPCKHPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VUNPCKLPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VUNPCKLPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VUNPCKLPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VUNPCKLPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VUNPCKLPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VUNPCKLPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VUNPCKLPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VUNPCKLPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VXORPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VXORPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VXORPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VXORPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VXORPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
    VXORPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
    VXORPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
    VXORPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
    VZEROALL                                  AVX,SANDYBRIDGE
    VZEROUPPER                                AVX,SANDYBRIDGE

#### B.1.27 Intel Carry-Less Multiplication instructions (CLMUL)

    PCLMULLQLQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
    PCLMULHQLQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
    PCLMULLQHQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
    PCLMULHQHQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
    PCLMULQDQ        xmmreg,xmmrm,imm         SSE,SANDYBRIDGE,SO

#### B.1.28 Intel Fused Multiply-Add instructions (FMA)

    VFMADDPD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMADDPD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMADDPD         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMADDPD         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMADDPS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMADDPS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMADDPS         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMADDPS         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMADDSD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
    VFMADDSD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
    VFMADDSS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
    VFMADDSS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD
    VFMADDSUBPD      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMADDSUBPD      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMADDSUBPD      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMADDSUBPD      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMADDSUBPS      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMADDSUBPS      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMADDSUBPS      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMADDSUBPS      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMSUBADDPD      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMSUBADDPD      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMSUBADDPD      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMSUBADDPD      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMSUBADDPS      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMSUBADDPS      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMSUBADDPS      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMSUBADDPS      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMSUBPD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMSUBPD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMSUBPD         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMSUBPD         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMSUBPS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFMSUBPS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFMSUBPS         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
    VFMSUBPS         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
    VFMSUBSD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
    VFMSUBSD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
    VFMSUBSS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
    VFMSUBSS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD
    VFNMADDPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFNMADDPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFNMADDPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
    VFNMADDPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
    VFNMADDPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFNMADDPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFNMADDPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
    VFNMADDPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
    VFNMADDSD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
    VFNMADDSD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
    VFNMADDSS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
    VFNMADDSS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD
    VFNMSUBPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFNMSUBPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFNMSUBPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
    VFNMSUBPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
    VFNMSUBPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
    VFNMSUBPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
    VFNMSUBPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
    VFNMSUBPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
    VFNMSUBSD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
    VFNMSUBSD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
    VFNMSUBSS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
    VFNMSUBSS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD

#### B.1.29 VIA (Centaur) security instructions

    XSTORE                                    PENT,CYRIX
    XCRYPTECB                                 PENT,CYRIX
    XCRYPTCBC                                 PENT,CYRIX
    XCRYPTCTR                                 PENT,CYRIX
    XCRYPTCFB                                 PENT,CYRIX
    XCRYPTOFB                                 PENT,CYRIX
    MONTMUL                                   PENT,CYRIX
    XSHA1                                     PENT,CYRIX
    XSHA256                                   PENT,CYRIX

#### B.1.30 Systematic names for the hinting nop instructions

    HINT_NOP0        rm16                     P6,UNDOC
    HINT_NOP0        rm32                     P6,UNDOC
    HINT_NOP0        rm64                     X64,UNDOC
    HINT_NOP1        rm16                     P6,UNDOC
    HINT_NOP1        rm32                     P6,UNDOC
    HINT_NOP1        rm64                     X64,UNDOC
    HINT_NOP2        rm16                     P6,UNDOC
    HINT_NOP2        rm32                     P6,UNDOC
    HINT_NOP2        rm64                     X64,UNDOC
    HINT_NOP3        rm16                     P6,UNDOC
    HINT_NOP3        rm32                     P6,UNDOC
    HINT_NOP3        rm64                     X64,UNDOC
    HINT_NOP4        rm16                     P6,UNDOC
    HINT_NOP4        rm32                     P6,UNDOC
    HINT_NOP4        rm64                     X64,UNDOC
    HINT_NOP5        rm16                     P6,UNDOC
    HINT_NOP5        rm32                     P6,UNDOC
    HINT_NOP5        rm64                     X64,UNDOC
    HINT_NOP6        rm16                     P6,UNDOC
    HINT_NOP6        rm32                     P6,UNDOC
    HINT_NOP6        rm64                     X64,UNDOC
    HINT_NOP7        rm16                     P6,UNDOC
    HINT_NOP7        rm32                     P6,UNDOC
    HINT_NOP7        rm64                     X64,UNDOC
    HINT_NOP8        rm16                     P6,UNDOC
    HINT_NOP8        rm32                     P6,UNDOC
    HINT_NOP8        rm64                     X64,UNDOC
    HINT_NOP9        rm16                     P6,UNDOC
    HINT_NOP9        rm32                     P6,UNDOC
    HINT_NOP9        rm64                     X64,UNDOC
    HINT_NOP10       rm16                     P6,UNDOC
    HINT_NOP10       rm32                     P6,UNDOC
    HINT_NOP10       rm64                     X64,UNDOC
    HINT_NOP11       rm16                     P6,UNDOC
    HINT_NOP11       rm32                     P6,UNDOC
    HINT_NOP11       rm64                     X64,UNDOC
    HINT_NOP12       rm16                     P6,UNDOC
    HINT_NOP12       rm32                     P6,UNDOC
    HINT_NOP12       rm64                     X64,UNDOC
    HINT_NOP13       rm16                     P6,UNDOC
    HINT_NOP13       rm32                     P6,UNDOC
    HINT_NOP13       rm64                     X64,UNDOC
    HINT_NOP14       rm16                     P6,UNDOC
    HINT_NOP14       rm32                     P6,UNDOC
    HINT_NOP14       rm64                     X64,UNDOC
    HINT_NOP15       rm16                     P6,UNDOC
    HINT_NOP15       rm32                     P6,UNDOC
    HINT_NOP15       rm64                     X64,UNDOC
    HINT_NOP16       rm16                     P6,UNDOC
    HINT_NOP16       rm32                     P6,UNDOC
    HINT_NOP16       rm64                     X64,UNDOC
    HINT_NOP17       rm16                     P6,UNDOC
    HINT_NOP17       rm32                     P6,UNDOC
    HINT_NOP17       rm64                     X64,UNDOC
    HINT_NOP18       rm16                     P6,UNDOC
    HINT_NOP18       rm32                     P6,UNDOC
    HINT_NOP18       rm64                     X64,UNDOC
    HINT_NOP19       rm16                     P6,UNDOC
    HINT_NOP19       rm32                     P6,UNDOC
    HINT_NOP19       rm64                     X64,UNDOC
    HINT_NOP20       rm16                     P6,UNDOC
    HINT_NOP20       rm32                     P6,UNDOC
    HINT_NOP20       rm64                     X64,UNDOC
    HINT_NOP21       rm16                     P6,UNDOC
    HINT_NOP21       rm32                     P6,UNDOC
    HINT_NOP21       rm64                     X64,UNDOC
    HINT_NOP22       rm16                     P6,UNDOC
    HINT_NOP22       rm32                     P6,UNDOC
    HINT_NOP22       rm64                     X64,UNDOC
    HINT_NOP23       rm16                     P6,UNDOC
    HINT_NOP23       rm32                     P6,UNDOC
    HINT_NOP23       rm64                     X64,UNDOC
    HINT_NOP24       rm16                     P6,UNDOC
    HINT_NOP24       rm32                     P6,UNDOC
    HINT_NOP24       rm64                     X64,UNDOC
    HINT_NOP25       rm16                     P6,UNDOC
    HINT_NOP25       rm32                     P6,UNDOC
    HINT_NOP25       rm64                     X64,UNDOC
    HINT_NOP26       rm16                     P6,UNDOC
    HINT_NOP26       rm32                     P6,UNDOC
    HINT_NOP26       rm64                     X64,UNDOC
    HINT_NOP27       rm16                     P6,UNDOC
    HINT_NOP27       rm32                     P6,UNDOC
    HINT_NOP27       rm64                     X64,UNDOC
    HINT_NOP28       rm16                     P6,UNDOC
    HINT_NOP28       rm32                     P6,UNDOC
    HINT_NOP28       rm64                     X64,UNDOC
    HINT_NOP29       rm16                     P6,UNDOC
    HINT_NOP29       rm32                     P6,UNDOC
    HINT_NOP29       rm64                     X64,UNDOC
    HINT_NOP30       rm16                     P6,UNDOC
    HINT_NOP30       rm32                     P6,UNDOC
    HINT_NOP30       rm64                     X64,UNDOC
    HINT_NOP31       rm16                     P6,UNDOC
    HINT_NOP31       rm32                     P6,UNDOC
    HINT_NOP31       rm64                     X64,UNDOC
    HINT_NOP32       rm16                     P6,UNDOC
    HINT_NOP32       rm32                     P6,UNDOC
    HINT_NOP32       rm64                     X64,UNDOC
    HINT_NOP33       rm16                     P6,UNDOC
    HINT_NOP33       rm32                     P6,UNDOC
    HINT_NOP33       rm64                     X64,UNDOC
    HINT_NOP34       rm16                     P6,UNDOC
    HINT_NOP34       rm32                     P6,UNDOC
    HINT_NOP34       rm64                     X64,UNDOC
    HINT_NOP35       rm16                     P6,UNDOC
    HINT_NOP35       rm32                     P6,UNDOC
    HINT_NOP35       rm64                     X64,UNDOC
    HINT_NOP36       rm16                     P6,UNDOC
    HINT_NOP36       rm32                     P6,UNDOC
    HINT_NOP36       rm64                     X64,UNDOC
    HINT_NOP37       rm16                     P6,UNDOC
    HINT_NOP37       rm32                     P6,UNDOC
    HINT_NOP37       rm64                     X64,UNDOC
    HINT_NOP38       rm16                     P6,UNDOC
    HINT_NOP38       rm32                     P6,UNDOC
    HINT_NOP38       rm64                     X64,UNDOC
    HINT_NOP39       rm16                     P6,UNDOC
    HINT_NOP39       rm32                     P6,UNDOC
    HINT_NOP39       rm64                     X64,UNDOC
    HINT_NOP40       rm16                     P6,UNDOC
    HINT_NOP40       rm32                     P6,UNDOC
    HINT_NOP40       rm64                     X64,UNDOC
    HINT_NOP41       rm16                     P6,UNDOC
    HINT_NOP41       rm32                     P6,UNDOC
    HINT_NOP41       rm64                     X64,UNDOC
    HINT_NOP42       rm16                     P6,UNDOC
    HINT_NOP42       rm32                     P6,UNDOC
    HINT_NOP42       rm64                     X64,UNDOC
    HINT_NOP43       rm16                     P6,UNDOC
    HINT_NOP43       rm32                     P6,UNDOC
    HINT_NOP43       rm64                     X64,UNDOC
    HINT_NOP44       rm16                     P6,UNDOC
    HINT_NOP44       rm32                     P6,UNDOC
    HINT_NOP44       rm64                     X64,UNDOC
    HINT_NOP45       rm16                     P6,UNDOC
    HINT_NOP45       rm32                     P6,UNDOC
    HINT_NOP45       rm64                     X64,UNDOC
    HINT_NOP46       rm16                     P6,UNDOC
    HINT_NOP46       rm32                     P6,UNDOC
    HINT_NOP46       rm64                     X64,UNDOC
    HINT_NOP47       rm16                     P6,UNDOC
    HINT_NOP47       rm32                     P6,UNDOC
    HINT_NOP47       rm64                     X64,UNDOC
    HINT_NOP48       rm16                     P6,UNDOC
    HINT_NOP48       rm32                     P6,UNDOC
    HINT_NOP48       rm64                     X64,UNDOC
    HINT_NOP49       rm16                     P6,UNDOC
    HINT_NOP49       rm32                     P6,UNDOC
    HINT_NOP49       rm64                     X64,UNDOC
    HINT_NOP50       rm16                     P6,UNDOC
    HINT_NOP50       rm32                     P6,UNDOC
    HINT_NOP50       rm64                     X64,UNDOC
    HINT_NOP51       rm16                     P6,UNDOC
    HINT_NOP51       rm32                     P6,UNDOC
    HINT_NOP51       rm64                     X64,UNDOC
    HINT_NOP52       rm16                     P6,UNDOC
    HINT_NOP52       rm32                     P6,UNDOC
    HINT_NOP52       rm64                     X64,UNDOC
    HINT_NOP53       rm16                     P6,UNDOC
    HINT_NOP53       rm32                     P6,UNDOC
    HINT_NOP53       rm64                     X64,UNDOC
    HINT_NOP54       rm16                     P6,UNDOC
    HINT_NOP54       rm32                     P6,UNDOC
    HINT_NOP54       rm64                     X64,UNDOC
    HINT_NOP55       rm16                     P6,UNDOC
    HINT_NOP55       rm32                     P6,UNDOC
    HINT_NOP55       rm64                     X64,UNDOC
    HINT_NOP56       rm16                     P6,UNDOC
    HINT_NOP56       rm32                     P6,UNDOC
    HINT_NOP56       rm64                     X64,UNDOC
    HINT_NOP57       rm16                     P6,UNDOC
    HINT_NOP57       rm32                     P6,UNDOC
    HINT_NOP57       rm64                     X64,UNDOC
    HINT_NOP58       rm16                     P6,UNDOC
    HINT_NOP58       rm32                     P6,UNDOC
    HINT_NOP58       rm64                     X64,UNDOC
    HINT_NOP59       rm16                     P6,UNDOC
    HINT_NOP59       rm32                     P6,UNDOC
    HINT_NOP59       rm64                     X64,UNDOC
    HINT_NOP60       rm16                     P6,UNDOC
    HINT_NOP60       rm32                     P6,UNDOC
    HINT_NOP60       rm64                     X64,UNDOC
    HINT_NOP61       rm16                     P6,UNDOC
    HINT_NOP61       rm32                     P6,UNDOC
    HINT_NOP61       rm64                     X64,UNDOC
    HINT_NOP62       rm16                     P6,UNDOC
    HINT_NOP62       rm32                     P6,UNDOC
    HINT_NOP62       rm64                     X64,UNDOC
    HINT_NOP63       rm16                     P6,UNDOC
    HINT_NOP63       rm32                     P6,UNDOC
    HINT_NOP63       rm64                     X64,UNDOC

Next Chapter | Previous Chapter | Contents | Index