
\S{} Special instructions...

\c DB                                        
\c DW                                        
\c DD                                        
\c DQ                                        
\c DT                                        
\c DO                                        
\c DY                                        
\c RESB             imm                      8086
\c RESW                                      
\c RESD                                      
\c RESQ                                      
\c REST                                      
\c RESO                                      
\c RESY                                      

\S{} Conventional instructions

\c AAA                                       8086,NOLONG
\c AAD                                       8086,NOLONG
\c AAD              imm                      8086,NOLONG
\c AAM                                       8086,NOLONG
\c AAM              imm                      8086,NOLONG
\c AAS                                       8086,NOLONG
\c ADC              mem,reg8                 8086
\c ADC              reg8,reg8                8086
\c ADC              mem,reg16                8086
\c ADC              reg16,reg16              8086
\c ADC              mem,reg32                386
\c ADC              reg32,reg32              386
\c ADC              mem,reg64                X64
\c ADC              reg64,reg64              X64
\c ADC              reg8,mem                 8086
\c ADC              reg8,reg8                8086
\c ADC              reg16,mem                8086
\c ADC              reg16,reg16              8086
\c ADC              reg32,mem                386
\c ADC              reg32,reg32              386
\c ADC              reg64,mem                X64
\c ADC              reg64,reg64              X64
\c ADC              rm16,imm8                8086
\c ADC              rm32,imm8                386
\c ADC              rm64,imm8                X64
\c ADC              reg_al,imm               8086
\c ADC              reg_ax,imm               8086
\c ADC              reg_eax,imm              386
\c ADC              reg_rax,imm              X64
\c ADC              rm8,imm                  8086
\c ADC              rm16,imm                 8086
\c ADC              rm32,imm                 386
\c ADC              rm64,imm                 X64
\c ADC              mem,imm8                 8086
\c ADC              mem,imm16                8086
\c ADC              mem,imm32                386
\c ADD              mem,reg8                 8086
\c ADD              reg8,reg8                8086
\c ADD              mem,reg16                8086
\c ADD              reg16,reg16              8086
\c ADD              mem,reg32                386
\c ADD              reg32,reg32              386
\c ADD              mem,reg64                X64
\c ADD              reg64,reg64              X64
\c ADD              reg8,mem                 8086
\c ADD              reg8,reg8                8086
\c ADD              reg16,mem                8086
\c ADD              reg16,reg16              8086
\c ADD              reg32,mem                386
\c ADD              reg32,reg32              386
\c ADD              reg64,mem                X64
\c ADD              reg64,reg64              X64
\c ADD              rm16,imm8                8086
\c ADD              rm32,imm8                386
\c ADD              rm64,imm8                X64
\c ADD              reg_al,imm               8086
\c ADD              reg_ax,imm               8086
\c ADD              reg_eax,imm              386
\c ADD              reg_rax,imm              X64
\c ADD              rm8,imm                  8086
\c ADD              rm16,imm                 8086
\c ADD              rm32,imm                 386
\c ADD              rm64,imm                 X64
\c ADD              mem,imm8                 8086
\c ADD              mem,imm16                8086
\c ADD              mem,imm32                386
\c AND              mem,reg8                 8086
\c AND              reg8,reg8                8086
\c AND              mem,reg16                8086
\c AND              reg16,reg16              8086
\c AND              mem,reg32                386
\c AND              reg32,reg32              386
\c AND              mem,reg64                X64
\c AND              reg64,reg64              X64
\c AND              reg8,mem                 8086
\c AND              reg8,reg8                8086
\c AND              reg16,mem                8086
\c AND              reg16,reg16              8086
\c AND              reg32,mem                386
\c AND              reg32,reg32              386
\c AND              reg64,mem                X64
\c AND              reg64,reg64              X64
\c AND              rm16,imm8                8086
\c AND              rm32,imm8                386
\c AND              rm64,imm8                X64
\c AND              reg_al,imm               8086
\c AND              reg_ax,imm               8086
\c AND              reg_eax,imm              386
\c AND              reg_rax,imm              X64
\c AND              rm8,imm                  8086
\c AND              rm16,imm                 8086
\c AND              rm32,imm                 386
\c AND              rm64,imm                 X64
\c AND              mem,imm8                 8086
\c AND              mem,imm16                8086
\c AND              mem,imm32                386
\c ARPL             mem,reg16                286,PROT,NOLONG
\c ARPL             reg16,reg16              286,PROT,NOLONG
\c BB0_RESET                                 PENT,CYRIX,ND
\c BB1_RESET                                 PENT,CYRIX,ND
\c BOUND            reg16,mem                186,NOLONG
\c BOUND            reg32,mem                386,NOLONG
\c BSF              reg16,mem                386
\c BSF              reg16,reg16              386
\c BSF              reg32,mem                386
\c BSF              reg32,reg32              386
\c BSF              reg64,mem                X64
\c BSF              reg64,reg64              X64
\c BSR              reg16,mem                386
\c BSR              reg16,reg16              386
\c BSR              reg32,mem                386
\c BSR              reg32,reg32              386
\c BSR              reg64,mem                X64
\c BSR              reg64,reg64              X64
\c BSWAP            reg32                    486
\c BSWAP            reg64                    X64
\c BT               mem,reg16                386
\c BT               reg16,reg16              386
\c BT               mem,reg32                386
\c BT               reg32,reg32              386
\c BT               mem,reg64                X64
\c BT               reg64,reg64              X64
\c BT               rm16,imm                 386
\c BT               rm32,imm                 386
\c BT               rm64,imm                 X64
\c BTC              mem,reg16                386
\c BTC              reg16,reg16              386
\c BTC              mem,reg32                386
\c BTC              reg32,reg32              386
\c BTC              mem,reg64                X64
\c BTC              reg64,reg64              X64
\c BTC              rm16,imm                 386
\c BTC              rm32,imm                 386
\c BTC              rm64,imm                 X64
\c BTR              mem,reg16                386
\c BTR              reg16,reg16              386
\c BTR              mem,reg32                386
\c BTR              reg32,reg32              386
\c BTR              mem,reg64                X64
\c BTR              reg64,reg64              X64
\c BTR              rm16,imm                 386
\c BTR              rm32,imm                 386
\c BTR              rm64,imm                 X64
\c BTS              mem,reg16                386
\c BTS              reg16,reg16              386
\c BTS              mem,reg32                386
\c BTS              reg32,reg32              386
\c BTS              mem,reg64                X64
\c BTS              reg64,reg64              X64
\c BTS              rm16,imm                 386
\c BTS              rm32,imm                 386
\c BTS              rm64,imm                 X64
\c CALL             imm                      8086
\c CALL             imm|near                 8086
\c CALL             imm|far                  8086,ND,NOLONG
\c CALL             imm16                    8086
\c CALL             imm16|near               8086
\c CALL             imm16|far                8086,ND,NOLONG
\c CALL             imm32                    386
\c CALL             imm32|near               386
\c CALL             imm32|far                386,ND,NOLONG
\c CALL             imm:imm                  8086,NOLONG
\c CALL             imm16:imm                8086,NOLONG
\c CALL             imm:imm16                8086,NOLONG
\c CALL             imm32:imm                386,NOLONG
\c CALL             imm:imm32                386,NOLONG
\c CALL             mem|far                  8086,NOLONG
\c CALL             mem|far                  X64
\c CALL             mem16|far                8086
\c CALL             mem32|far                386
\c CALL             mem64|far                X64
\c CALL             mem|near                 8086
\c CALL             mem16|near               8086
\c CALL             mem32|near               386,NOLONG
\c CALL             mem64|near               X64
\c CALL             reg16                    8086
\c CALL             reg32                    386,NOLONG
\c CALL             reg64                    X64
\c CALL             mem                      8086
\c CALL             mem16                    8086
\c CALL             mem32                    386,NOLONG
\c CALL             mem64                    X64
\c CBW                                       8086
\c CDQ                                       386
\c CDQE                                      X64
\c CLC                                       8086
\c CLD                                       8086
\c CLGI                                      X64,AMD
\c CLI                                       8086
\c CLTS                                      286,PRIV
\c CMC                                       8086
\c CMP              mem,reg8                 8086
\c CMP              reg8,reg8                8086
\c CMP              mem,reg16                8086
\c CMP              reg16,reg16              8086
\c CMP              mem,reg32                386
\c CMP              reg32,reg32              386
\c CMP              mem,reg64                X64
\c CMP              reg64,reg64              X64
\c CMP              reg8,mem                 8086
\c CMP              reg8,reg8                8086
\c CMP              reg16,mem                8086
\c CMP              reg16,reg16              8086
\c CMP              reg32,mem                386
\c CMP              reg32,reg32              386
\c CMP              reg64,mem                X64
\c CMP              reg64,reg64              X64
\c CMP              rm16,imm8                8086
\c CMP              rm32,imm8                386
\c CMP              rm64,imm8                X64
\c CMP              reg_al,imm               8086
\c CMP              reg_ax,imm               8086
\c CMP              reg_eax,imm              386
\c CMP              reg_rax,imm              X64
\c CMP              rm8,imm                  8086
\c CMP              rm16,imm                 8086
\c CMP              rm32,imm                 386
\c CMP              rm64,imm                 X64
\c CMP              mem,imm8                 8086
\c CMP              mem,imm16                8086
\c CMP              mem,imm32                386
\c CMPSB                                     8086
\c CMPSD                                     386
\c CMPSQ                                     X64
\c CMPSW                                     8086
\c CMPXCHG          mem,reg8                 PENT
\c CMPXCHG          reg8,reg8                PENT
\c CMPXCHG          mem,reg16                PENT
\c CMPXCHG          reg16,reg16              PENT
\c CMPXCHG          mem,reg32                PENT
\c CMPXCHG          reg32,reg32              PENT
\c CMPXCHG          mem,reg64                X64
\c CMPXCHG          reg64,reg64              X64
\c CMPXCHG486       mem,reg8                 486,UNDOC,ND
\c CMPXCHG486       reg8,reg8                486,UNDOC,ND
\c CMPXCHG486       mem,reg16                486,UNDOC,ND
\c CMPXCHG486       reg16,reg16              486,UNDOC,ND
\c CMPXCHG486       mem,reg32                486,UNDOC,ND
\c CMPXCHG486       reg32,reg32              486,UNDOC,ND
\c CMPXCHG8B        mem                      PENT
\c CMPXCHG16B       mem                      X64
\c CPUID                                     PENT
\c CPU_READ                                  PENT,CYRIX
\c CPU_WRITE                                 PENT,CYRIX
\c CQO                                       X64
\c CWD                                       8086
\c CWDE                                      386
\c DAA                                       8086,NOLONG
\c DAS                                       8086,NOLONG
\c DEC              reg16                    8086,NOLONG
\c DEC              reg32                    386,NOLONG
\c DEC              rm8                      8086
\c DEC              rm16                     8086
\c DEC              rm32                     386
\c DEC              rm64                     X64
\c DIV              rm8                      8086
\c DIV              rm16                     8086
\c DIV              rm32                     386
\c DIV              rm64                     X64
\c DMINT                                     P6,CYRIX
\c EMMS                                      PENT,MMX
\c ENTER            imm,imm                  186
\c EQU              imm                      8086
\c EQU              imm:imm                  8086
\c F2XM1                                     8086,FPU
\c FABS                                      8086,FPU
\c FADD             mem32                    8086,FPU
\c FADD             mem64                    8086,FPU
\c FADD             fpureg|to                8086,FPU
\c FADD             fpureg                   8086,FPU
\c FADD             fpureg,fpu0              8086,FPU
\c FADD             fpu0,fpureg              8086,FPU
\c FADD                                      8086,FPU,ND
\c FADDP            fpureg                   8086,FPU
\c FADDP            fpureg,fpu0              8086,FPU
\c FADDP                                     8086,FPU,ND
\c FBLD             mem80                    8086,FPU
\c FBLD             mem                      8086,FPU
\c FBSTP            mem80                    8086,FPU
\c FBSTP            mem                      8086,FPU
\c FCHS                                      8086,FPU
\c FCLEX                                     8086,FPU
\c FCMOVB           fpureg                   P6,FPU
\c FCMOVB           fpu0,fpureg              P6,FPU
\c FCMOVB                                    P6,FPU,ND
\c FCMOVBE          fpureg                   P6,FPU
\c FCMOVBE          fpu0,fpureg              P6,FPU
\c FCMOVBE                                   P6,FPU,ND
\c FCMOVE           fpureg                   P6,FPU
\c FCMOVE           fpu0,fpureg              P6,FPU
\c FCMOVE                                    P6,FPU,ND
\c FCMOVNB          fpureg                   P6,FPU
\c FCMOVNB          fpu0,fpureg              P6,FPU
\c FCMOVNB                                   P6,FPU,ND
\c FCMOVNBE         fpureg                   P6,FPU
\c FCMOVNBE         fpu0,fpureg              P6,FPU
\c FCMOVNBE                                  P6,FPU,ND
\c FCMOVNE          fpureg                   P6,FPU
\c FCMOVNE          fpu0,fpureg              P6,FPU
\c FCMOVNE                                   P6,FPU,ND
\c FCMOVNU          fpureg                   P6,FPU
\c FCMOVNU          fpu0,fpureg              P6,FPU
\c FCMOVNU                                   P6,FPU,ND
\c FCMOVU           fpureg                   P6,FPU
\c FCMOVU           fpu0,fpureg              P6,FPU
\c FCMOVU                                    P6,FPU,ND
\c FCOM             mem32                    8086,FPU
\c FCOM             mem64                    8086,FPU
\c FCOM             fpureg                   8086,FPU
\c FCOM             fpu0,fpureg              8086,FPU
\c FCOM                                      8086,FPU,ND
\c FCOMI            fpureg                   P6,FPU
\c FCOMI            fpu0,fpureg              P6,FPU
\c FCOMI                                     P6,FPU,ND
\c FCOMIP           fpureg                   P6,FPU
\c FCOMIP           fpu0,fpureg              P6,FPU
\c FCOMIP                                    P6,FPU,ND
\c FCOMP            mem32                    8086,FPU
\c FCOMP            mem64                    8086,FPU
\c FCOMP            fpureg                   8086,FPU
\c FCOMP            fpu0,fpureg              8086,FPU
\c FCOMP                                     8086,FPU,ND
\c FCOMPP                                    8086,FPU
\c FCOS                                      386,FPU
\c FDECSTP                                   8086,FPU
\c FDISI                                     8086,FPU
\c FDIV             mem32                    8086,FPU
\c FDIV             mem64                    8086,FPU
\c FDIV             fpureg|to                8086,FPU
\c FDIV             fpureg                   8086,FPU
\c FDIV             fpureg,fpu0              8086,FPU
\c FDIV             fpu0,fpureg              8086,FPU
\c FDIV                                      8086,FPU,ND
\c FDIVP            fpureg                   8086,FPU
\c FDIVP            fpureg,fpu0              8086,FPU
\c FDIVP                                     8086,FPU,ND
\c FDIVR            mem32                    8086,FPU
\c FDIVR            mem64                    8086,FPU
\c FDIVR            fpureg|to                8086,FPU
\c FDIVR            fpureg,fpu0              8086,FPU
\c FDIVR            fpureg                   8086,FPU
\c FDIVR            fpu0,fpureg              8086,FPU
\c FDIVR                                     8086,FPU,ND
\c FDIVRP           fpureg                   8086,FPU
\c FDIVRP           fpureg,fpu0              8086,FPU
\c FDIVRP                                    8086,FPU,ND
\c FEMMS                                     PENT,3DNOW
\c FENI                                      8086,FPU
\c FFREE            fpureg                   8086,FPU
\c FFREE                                     8086,FPU
\c FFREEP           fpureg                   286,FPU,UNDOC
\c FFREEP                                    286,FPU,UNDOC
\c FIADD            mem32                    8086,FPU
\c FIADD            mem16                    8086,FPU
\c FICOM            mem32                    8086,FPU
\c FICOM            mem16                    8086,FPU
\c FICOMP           mem32                    8086,FPU
\c FICOMP           mem16                    8086,FPU
\c FIDIV            mem32                    8086,FPU
\c FIDIV            mem16                    8086,FPU
\c FIDIVR           mem32                    8086,FPU
\c FIDIVR           mem16                    8086,FPU
\c FILD             mem32                    8086,FPU
\c FILD             mem16                    8086,FPU
\c FILD             mem64                    8086,FPU
\c FIMUL            mem32                    8086,FPU
\c FIMUL            mem16                    8086,FPU
\c FINCSTP                                   8086,FPU
\c FINIT                                     8086,FPU
\c FIST             mem32                    8086,FPU
\c FIST             mem16                    8086,FPU
\c FISTP            mem32                    8086,FPU
\c FISTP            mem16                    8086,FPU
\c FISTP            mem64                    8086,FPU
\c FISTTP           mem16                    PRESCOTT,FPU
\c FISTTP           mem32                    PRESCOTT,FPU
\c FISTTP           mem64                    PRESCOTT,FPU
\c FISUB            mem32                    8086,FPU
\c FISUB            mem16                    8086,FPU
\c FISUBR           mem32                    8086,FPU
\c FISUBR           mem16                    8086,FPU
\c FLD              mem32                    8086,FPU
\c FLD              mem64                    8086,FPU
\c FLD              mem80                    8086,FPU
\c FLD              fpureg                   8086,FPU
\c FLD                                       8086,FPU,ND
\c FLD1                                      8086,FPU
\c FLDCW            mem                      8086,FPU,SW
\c FLDENV           mem                      8086,FPU
\c FLDL2E                                    8086,FPU
\c FLDL2T                                    8086,FPU
\c FLDLG2                                    8086,FPU
\c FLDLN2                                    8086,FPU
\c FLDPI                                     8086,FPU
\c FLDZ                                      8086,FPU
\c FMUL             mem32                    8086,FPU
\c FMUL             mem64                    8086,FPU
\c FMUL             fpureg|to                8086,FPU
\c FMUL             fpureg,fpu0              8086,FPU
\c FMUL             fpureg                   8086,FPU
\c FMUL             fpu0,fpureg              8086,FPU
\c FMUL                                      8086,FPU,ND
\c FMULP            fpureg                   8086,FPU
\c FMULP            fpureg,fpu0              8086,FPU
\c FMULP                                     8086,FPU,ND
\c FNCLEX                                    8086,FPU
\c FNDISI                                    8086,FPU
\c FNENI                                     8086,FPU
\c FNINIT                                    8086,FPU
\c FNOP                                      8086,FPU
\c FNSAVE           mem                      8086,FPU
\c FNSTCW           mem                      8086,FPU,SW
\c FNSTENV          mem                      8086,FPU
\c FNSTSW           mem                      8086,FPU,SW
\c FNSTSW           reg_ax                   286,FPU
\c FPATAN                                    8086,FPU
\c FPREM                                     8086,FPU
\c FPREM1                                    386,FPU
\c FPTAN                                     8086,FPU
\c FRNDINT                                   8086,FPU
\c FRSTOR           mem                      8086,FPU
\c FSAVE            mem                      8086,FPU
\c FSCALE                                    8086,FPU
\c FSETPM                                    286,FPU
\c FSIN                                      386,FPU
\c FSINCOS                                   386,FPU
\c FSQRT                                     8086,FPU
\c FST              mem32                    8086,FPU
\c FST              mem64                    8086,FPU
\c FST              fpureg                   8086,FPU
\c FST                                       8086,FPU,ND
\c FSTCW            mem                      8086,FPU,SW
\c FSTENV           mem                      8086,FPU
\c FSTP             mem32                    8086,FPU
\c FSTP             mem64                    8086,FPU
\c FSTP             mem80                    8086,FPU
\c FSTP             fpureg                   8086,FPU
\c FSTP                                      8086,FPU,ND
\c FSTSW            mem                      8086,FPU,SW
\c FSTSW            reg_ax                   286,FPU
\c FSUB             mem32                    8086,FPU
\c FSUB             mem64                    8086,FPU
\c FSUB             fpureg|to                8086,FPU
\c FSUB             fpureg,fpu0              8086,FPU
\c FSUB             fpureg                   8086,FPU
\c FSUB             fpu0,fpureg              8086,FPU
\c FSUB                                      8086,FPU,ND
\c FSUBP            fpureg                   8086,FPU
\c FSUBP            fpureg,fpu0              8086,FPU
\c FSUBP                                     8086,FPU,ND
\c FSUBR            mem32                    8086,FPU
\c FSUBR            mem64                    8086,FPU
\c FSUBR            fpureg|to                8086,FPU
\c FSUBR            fpureg,fpu0              8086,FPU
\c FSUBR            fpureg                   8086,FPU
\c FSUBR            fpu0,fpureg              8086,FPU
\c FSUBR                                     8086,FPU,ND
\c FSUBRP           fpureg                   8086,FPU
\c FSUBRP           fpureg,fpu0              8086,FPU
\c FSUBRP                                    8086,FPU,ND
\c FTST                                      8086,FPU
\c FUCOM            fpureg                   386,FPU
\c FUCOM            fpu0,fpureg              386,FPU
\c FUCOM                                     386,FPU,ND
\c FUCOMI           fpureg                   P6,FPU
\c FUCOMI           fpu0,fpureg              P6,FPU
\c FUCOMI                                    P6,FPU,ND
\c FUCOMIP          fpureg                   P6,FPU
\c FUCOMIP          fpu0,fpureg              P6,FPU
\c FUCOMIP                                   P6,FPU,ND
\c FUCOMP           fpureg                   386,FPU
\c FUCOMP           fpu0,fpureg              386,FPU
\c FUCOMP                                    386,FPU,ND
\c FUCOMPP                                   386,FPU
\c FXAM                                      8086,FPU
\c FXCH             fpureg                   8086,FPU
\c FXCH             fpureg,fpu0              8086,FPU
\c FXCH             fpu0,fpureg              8086,FPU
\c FXCH                                      8086,FPU,ND
\c FXTRACT                                   8086,FPU
\c FYL2X                                     8086,FPU
\c FYL2XP1                                   8086,FPU
\c HLT                                       8086,PRIV
\c IBTS             mem,reg16                386,SW,UNDOC,ND
\c IBTS             reg16,reg16              386,UNDOC,ND
\c IBTS             mem,reg32                386,SD,UNDOC,ND
\c IBTS             reg32,reg32              386,UNDOC,ND
\c ICEBP                                     386,ND
\c IDIV             rm8                      8086
\c IDIV             rm16                     8086
\c IDIV             rm32                     386
\c IDIV             rm64                     X64
\c IMUL             rm8                      8086
\c IMUL             rm16                     8086
\c IMUL             rm32                     386
\c IMUL             rm64                     X64
\c IMUL             reg16,mem                386
\c IMUL             reg16,reg16              386
\c IMUL             reg32,mem                386
\c IMUL             reg32,reg32              386
\c IMUL             reg64,mem                X64
\c IMUL             reg64,reg64              X64
\c IMUL             reg16,mem,imm8           186
\c IMUL             reg16,mem,sbyte16        186,ND
\c IMUL             reg16,mem,imm16          186
\c IMUL             reg16,mem,imm            186,ND
\c IMUL             reg16,reg16,imm8         186
\c IMUL             reg16,reg16,sbyte32      186,ND
\c IMUL             reg16,reg16,imm16        186
\c IMUL             reg16,reg16,imm          186,ND
\c IMUL             reg32,mem,imm8           386
\c IMUL             reg32,mem,sbyte64        386,ND
\c IMUL             reg32,mem,imm32          386
\c IMUL             reg32,mem,imm            386,ND
\c IMUL             reg32,reg32,imm8         386
\c IMUL             reg32,reg32,sbyte16      386,ND
\c IMUL             reg32,reg32,imm32        386
\c IMUL             reg32,reg32,imm          386,ND
\c IMUL             reg64,mem,imm8           X64
\c IMUL             reg64,mem,sbyte32        X64,ND
\c IMUL             reg64,mem,imm32          X64
\c IMUL             reg64,mem,imm            X64,ND
\c IMUL             reg64,reg64,imm8         X64
\c IMUL             reg64,reg64,sbyte64      X64,ND
\c IMUL             reg64,reg64,imm32        X64
\c IMUL             reg64,reg64,imm          X64,ND
\c IMUL             reg16,imm8               186
\c IMUL             reg16,sbyte16            186,ND
\c IMUL             reg16,imm16              186
\c IMUL             reg16,imm                186,ND
\c IMUL             reg32,imm8               386
\c IMUL             reg32,sbyte32            386,ND
\c IMUL             reg32,imm32              386
\c IMUL             reg32,imm                386,ND
\c IMUL             reg64,imm8               X64
\c IMUL             reg64,sbyte64            X64,ND
\c IMUL             reg64,imm32              X64
\c IMUL             reg64,imm                X64,ND
\c IN               reg_al,imm               8086
\c IN               reg_ax,imm               8086
\c IN               reg_eax,imm              386
\c IN               reg_al,reg_dx            8086
\c IN               reg_ax,reg_dx            8086
\c IN               reg_eax,reg_dx           386
\c INC              reg16                    8086,NOLONG
\c INC              reg32                    386,NOLONG
\c INC              rm8                      8086
\c INC              rm16                     8086
\c INC              rm32                     386
\c INC              rm64                     X64
\c INCBIN                                    
\c INSB                                      186
\c INSD                                      386
\c INSW                                      186
\c INT              imm                      8086
\c INT01                                     386,ND
\c INT1                                      386
\c INT03                                     8086,ND
\c INT3                                      8086
\c INTO                                      8086,NOLONG
\c INVD                                      486,PRIV
\c INVLPG           mem                      486,PRIV
\c INVLPGA          reg_ax,reg_ecx           X86_64,AMD,NOLONG
\c INVLPGA          reg_eax,reg_ecx          X86_64,AMD
\c INVLPGA          reg_rax,reg_ecx          X64,AMD
\c INVLPGA                                   X86_64,AMD
\c IRET                                      8086
\c IRETD                                     386
\c IRETQ                                     X64
\c IRETW                                     8086
\c JCXZ             imm                      8086,NOLONG
\c JECXZ            imm                      386
\c JMP              imm|short                8086
\c JMP              imm                      8086,ND
\c JMP              imm                      8086
\c JMP              imm|near                 8086,ND
\c JMP              imm|far                  8086,ND,NOLONG
\c JMP              imm16                    8086
\c JMP              imm16|near               8086,ND
\c JMP              imm16|far                8086,ND,NOLONG
\c JMP              imm32                    386
\c JMP              imm32|near               386,ND
\c JMP              imm32|far                386,ND,NOLONG
\c JMP              imm:imm                  8086,NOLONG
\c JMP              imm16:imm                8086,NOLONG
\c JMP              imm:imm16                8086,NOLONG
\c JMP              imm32:imm                386,NOLONG
\c JMP              imm:imm32                386,NOLONG
\c JMP              mem|far                  8086,NOLONG
\c JMP              mem|far                  X64
\c JMP              mem16|far                8086
\c JMP              mem32|far                386
\c JMP              mem64|far                X64
\c JMP              mem|near                 8086
\c JMP              mem16|near               8086
\c JMP              mem32|near               386,NOLONG
\c JMP              mem64|near               X64
\c JMP              reg16                    8086
\c JMP              reg32                    386,NOLONG
\c JMP              reg64                    X64
\c JMP              mem                      8086
\c JMP              mem16                    8086
\c JMP              mem32                    386,NOLONG
\c JMP              mem64                    X64
\c JMPE             imm                      IA64
\c JMPE             imm16                    IA64
\c JMPE             imm32                    IA64
\c JMPE             rm16                     IA64
\c JMPE             rm32                     IA64
\c JRCXZ            imm                      X64
\c LAHF                                      8086
\c LAR              reg16,mem                286,PROT,SW
\c LAR              reg16,reg16              286,PROT
\c LAR              reg16,reg32              386,PROT
\c LAR              reg16,reg64              X64,PROT,ND
\c LAR              reg32,mem                386,PROT,SW
\c LAR              reg32,reg16              386,PROT
\c LAR              reg32,reg32              386,PROT
\c LAR              reg32,reg64              X64,PROT,ND
\c LAR              reg64,mem                X64,PROT,SW
\c LAR              reg64,reg16              X64,PROT
\c LAR              reg64,reg32              X64,PROT
\c LAR              reg64,reg64              X64,PROT
\c LDS              reg16,mem                8086,NOLONG
\c LDS              reg32,mem                386,NOLONG
\c LEA              reg16,mem                8086
\c LEA              reg32,mem                386
\c LEA              reg64,mem                X64
\c LEAVE                                     186
\c LES              reg16,mem                8086,NOLONG
\c LES              reg32,mem                386,NOLONG
\c LFENCE                                    X64,AMD
\c LFS              reg16,mem                386
\c LFS              reg32,mem                386
\c LGDT             mem                      286,PRIV
\c LGS              reg16,mem                386
\c LGS              reg32,mem                386
\c LIDT             mem                      286,PRIV
\c LLDT             mem                      286,PROT,PRIV
\c LLDT             mem16                    286,PROT,PRIV
\c LLDT             reg16                    286,PROT,PRIV
\c LMSW             mem                      286,PRIV
\c LMSW             mem16                    286,PRIV
\c LMSW             reg16                    286,PRIV
\c LOADALL                                   386,UNDOC
\c LOADALL286                                286,UNDOC
\c LODSB                                     8086
\c LODSD                                     386
\c LODSQ                                     X64
\c LODSW                                     8086
\c LOOP             imm                      8086
\c LOOP             imm,reg_cx               8086,NOLONG
\c LOOP             imm,reg_ecx              386
\c LOOP             imm,reg_rcx              X64
\c LOOPE            imm                      8086
\c LOOPE            imm,reg_cx               8086,NOLONG
\c LOOPE            imm,reg_ecx              386
\c LOOPE            imm,reg_rcx              X64
\c LOOPNE           imm                      8086
\c LOOPNE           imm,reg_cx               8086,NOLONG
\c LOOPNE           imm,reg_ecx              386
\c LOOPNE           imm,reg_rcx              X64
\c LOOPNZ           imm                      8086
\c LOOPNZ           imm,reg_cx               8086,NOLONG
\c LOOPNZ           imm,reg_ecx              386
\c LOOPNZ           imm,reg_rcx              X64
\c LOOPZ            imm                      8086
\c LOOPZ            imm,reg_cx               8086,NOLONG
\c LOOPZ            imm,reg_ecx              386
\c LOOPZ            imm,reg_rcx              X64
\c LSL              reg16,mem                286,PROT,SW
\c LSL              reg16,reg16              286,PROT
\c LSL              reg16,reg32              386,PROT
\c LSL              reg16,reg64              X64,PROT,ND
\c LSL              reg32,mem                386,PROT,SW
\c LSL              reg32,reg16              386,PROT
\c LSL              reg32,reg32              386,PROT
\c LSL              reg32,reg64              X64,PROT,ND
\c LSL              reg64,mem                X64,PROT,SW
\c LSL              reg64,reg16              X64,PROT
\c LSL              reg64,reg32              X64,PROT
\c LSL              reg64,reg64              X64,PROT
\c LSS              reg16,mem                386
\c LSS              reg32,mem                386
\c LTR              mem                      286,PROT,PRIV
\c LTR              mem16                    286,PROT,PRIV
\c LTR              reg16                    286,PROT,PRIV
\c MFENCE                                    X64,AMD
\c MONITOR                                   PRESCOTT
\c MONITOR          reg_eax,reg_ecx,reg_edx  PRESCOTT,ND
\c MOV              mem,reg_sreg             8086
\c MOV              reg16,reg_sreg           8086
\c MOV              reg32,reg_sreg           386
\c MOV              reg_sreg,mem             8086
\c MOV              reg_sreg,reg16           8086
\c MOV              reg_sreg,reg32           386
\c MOV              reg_al,mem_offs          8086
\c MOV              reg_ax,mem_offs          8086
\c MOV              reg_eax,mem_offs         386
\c MOV              reg_rax,mem_offs         X64
\c MOV              mem_offs,reg_al          8086
\c MOV              mem_offs,reg_ax          8086
\c MOV              mem_offs,reg_eax         386
\c MOV              mem_offs,reg_rax         X64
\c MOV              reg32,reg_creg           386,PRIV,NOLONG
\c MOV              reg64,reg_creg           X64,PRIV
\c MOV              reg_creg,reg32           386,PRIV,NOLONG
\c MOV              reg_creg,reg64           X64,PRIV
\c MOV              reg32,reg_dreg           386,PRIV,NOLONG
\c MOV              reg64,reg_dreg           X64,PRIV
\c MOV              reg_dreg,reg32           386,PRIV,NOLONG
\c MOV              reg_dreg,reg64           X64,PRIV
\c MOV              reg32,reg_treg           386,NOLONG,ND
\c MOV              reg_treg,reg32           386,NOLONG,ND
\c MOV              mem,reg8                 8086
\c MOV              reg8,reg8                8086
\c MOV              mem,reg16                8086
\c MOV              reg16,reg16              8086
\c MOV              mem,reg32                386
\c MOV              reg32,reg32              386
\c MOV              mem,reg64                X64
\c MOV              reg64,reg64              X64
\c MOV              reg8,mem                 8086
\c MOV              reg8,reg8                8086
\c MOV              reg16,mem                8086
\c MOV              reg16,reg16              8086
\c MOV              reg32,mem                386
\c MOV              reg32,reg32              386
\c MOV              reg64,mem                X64
\c MOV              reg64,reg64              X64
\c MOV              reg8,imm                 8086
\c MOV              reg16,imm                8086
\c MOV              reg32,imm                386
\c MOV              reg64,imm                X64
\c MOV              reg64,imm32              X64
\c MOV              rm8,imm                  8086
\c MOV              rm16,imm                 8086
\c MOV              rm32,imm                 386
\c MOV              rm64,imm                 X64
\c MOV              mem,imm8                 8086
\c MOV              mem,imm16                8086
\c MOV              mem,imm32                386
\c MOVD             mmxreg,mem               PENT,MMX,SD
\c MOVD             mmxreg,reg32             PENT,MMX
\c MOVD             mem,mmxreg               PENT,MMX,SD
\c MOVD             reg32,mmxreg             PENT,MMX
\c MOVD             xmmreg,mem               X64,SD
\c MOVD             xmmreg,reg32             X64
\c MOVD             mem,xmmreg               X64,SD
\c MOVD             reg32,xmmreg             X64,SSE
\c MOVQ             mmxreg,mmxrm             PENT,MMX
\c MOVQ             mmxrm,mmxreg             PENT,MMX
\c MOVQ             mmxreg,rm64              X64,MMX
\c MOVQ             rm64,mmxreg              X64,MMX
\c MOVSB                                     8086
\c MOVSD                                     386
\c MOVSQ                                     X64
\c MOVSW                                     8086
\c MOVSX            reg16,mem                386
\c MOVSX            reg16,reg8               386
\c MOVSX            reg32,rm8                386
\c MOVSX            reg32,rm16               386
\c MOVSX            reg64,rm8                X64
\c MOVSX            reg64,rm16               X64
\c MOVSXD           reg64,rm32               X64
\c MOVSX            reg64,rm32               X64,ND
\c MOVZX            reg16,mem                386
\c MOVZX            reg16,reg8               386
\c MOVZX            reg32,rm8                386
\c MOVZX            reg32,rm16               386
\c MOVZX            reg64,rm8                X64
\c MOVZX            reg64,rm16               X64
\c MUL              rm8                      8086
\c MUL              rm16                     8086
\c MUL              rm32                     386
\c MUL              rm64                     X64
\c MWAIT                                     PRESCOTT
\c MWAIT            reg_eax,reg_ecx          PRESCOTT,ND
\c NEG              rm8                      8086
\c NEG              rm16                     8086
\c NEG              rm32                     386
\c NEG              rm64                     X64
\c NOP                                       8086
\c NOP              rm16                     P6
\c NOP              rm32                     P6
\c NOP              rm64                     X64
\c NOT              rm8                      8086
\c NOT              rm16                     8086
\c NOT              rm32                     386
\c NOT              rm64                     X64
\c OR               mem,reg8                 8086
\c OR               reg8,reg8                8086
\c OR               mem,reg16                8086
\c OR               reg16,reg16              8086
\c OR               mem,reg32                386
\c OR               reg32,reg32              386
\c OR               mem,reg64                X64
\c OR               reg64,reg64              X64
\c OR               reg8,mem                 8086
\c OR               reg8,reg8                8086
\c OR               reg16,mem                8086
\c OR               reg16,reg16              8086
\c OR               reg32,mem                386
\c OR               reg32,reg32              386
\c OR               reg64,mem                X64
\c OR               reg64,reg64              X64
\c OR               rm16,imm8                8086
\c OR               rm32,imm8                386
\c OR               rm64,imm8                X64
\c OR               reg_al,imm               8086
\c OR               reg_ax,imm               8086
\c OR               reg_eax,imm              386
\c OR               reg_rax,imm              X64
\c OR               rm8,imm                  8086
\c OR               rm16,imm                 8086
\c OR               rm32,imm                 386
\c OR               rm64,imm                 X64
\c OR               mem,imm8                 8086
\c OR               mem,imm16                8086
\c OR               mem,imm32                386
\c OUT              imm,reg_al               8086
\c OUT              imm,reg_ax               8086
\c OUT              imm,reg_eax              386
\c OUT              reg_dx,reg_al            8086
\c OUT              reg_dx,reg_ax            8086
\c OUT              reg_dx,reg_eax           386
\c OUTSB                                     186
\c OUTSD                                     386
\c OUTSW                                     186
\c PACKSSDW         mmxreg,mmxrm             PENT,MMX
\c PACKSSWB         mmxreg,mmxrm             PENT,MMX
\c PACKUSWB         mmxreg,mmxrm             PENT,MMX
\c PADDB            mmxreg,mmxrm             PENT,MMX
\c PADDD            mmxreg,mmxrm             PENT,MMX
\c PADDSB           mmxreg,mmxrm             PENT,MMX
\c PADDSIW          mmxreg,mmxrm             PENT,MMX,CYRIX
\c PADDSW           mmxreg,mmxrm             PENT,MMX
\c PADDUSB          mmxreg,mmxrm             PENT,MMX
\c PADDUSW          mmxreg,mmxrm             PENT,MMX
\c PADDW            mmxreg,mmxrm             PENT,MMX
\c PAND             mmxreg,mmxrm             PENT,MMX
\c PANDN            mmxreg,mmxrm             PENT,MMX
\c PAUSE                                     8086
\c PAVEB            mmxreg,mmxrm             PENT,MMX,CYRIX
\c PAVGUSB          mmxreg,mmxrm             PENT,3DNOW
\c PCMPEQB          mmxreg,mmxrm             PENT,MMX
\c PCMPEQD          mmxreg,mmxrm             PENT,MMX
\c PCMPEQW          mmxreg,mmxrm             PENT,MMX
\c PCMPGTB          mmxreg,mmxrm             PENT,MMX
\c PCMPGTD          mmxreg,mmxrm             PENT,MMX
\c PCMPGTW          mmxreg,mmxrm             PENT,MMX
\c PDISTIB          mmxreg,mem               PENT,MMX,CYRIX
\c PF2ID            mmxreg,mmxrm             PENT,3DNOW
\c PFACC            mmxreg,mmxrm             PENT,3DNOW
\c PFADD            mmxreg,mmxrm             PENT,3DNOW
\c PFCMPEQ          mmxreg,mmxrm             PENT,3DNOW
\c PFCMPGE          mmxreg,mmxrm             PENT,3DNOW
\c PFCMPGT          mmxreg,mmxrm             PENT,3DNOW
\c PFMAX            mmxreg,mmxrm             PENT,3DNOW
\c PFMIN            mmxreg,mmxrm             PENT,3DNOW
\c PFMUL            mmxreg,mmxrm             PENT,3DNOW
\c PFRCP            mmxreg,mmxrm             PENT,3DNOW
\c PFRCPIT1         mmxreg,mmxrm             PENT,3DNOW
\c PFRCPIT2         mmxreg,mmxrm             PENT,3DNOW
\c PFRSQIT1         mmxreg,mmxrm             PENT,3DNOW
\c PFRSQRT          mmxreg,mmxrm             PENT,3DNOW
\c PFSUB            mmxreg,mmxrm             PENT,3DNOW
\c PFSUBR           mmxreg,mmxrm             PENT,3DNOW
\c PI2FD            mmxreg,mmxrm             PENT,3DNOW
\c PMACHRIW         mmxreg,mem               PENT,MMX,CYRIX
\c PMADDWD          mmxreg,mmxrm             PENT,MMX
\c PMAGW            mmxreg,mmxrm             PENT,MMX,CYRIX
\c PMULHRIW         mmxreg,mmxrm             PENT,MMX,CYRIX
\c PMULHRWA         mmxreg,mmxrm             PENT,3DNOW
\c PMULHRWC         mmxreg,mmxrm             PENT,MMX,CYRIX
\c PMULHW           mmxreg,mmxrm             PENT,MMX
\c PMULLW           mmxreg,mmxrm             PENT,MMX
\c PMVGEZB          mmxreg,mem               PENT,MMX,CYRIX
\c PMVLZB           mmxreg,mem               PENT,MMX,CYRIX
\c PMVNZB           mmxreg,mem               PENT,MMX,CYRIX
\c PMVZB            mmxreg,mem               PENT,MMX,CYRIX
\c POP              reg16                    8086
\c POP              reg32                    386,NOLONG
\c POP              reg64                    X64
\c POP              rm16                     8086
\c POP              rm32                     386,NOLONG
\c POP              rm64                     X64
\c POP              reg_cs                   8086,UNDOC,ND
\c POP              reg_dess                 8086,NOLONG
\c POP              reg_fsgs                 386
\c POPA                                      186,NOLONG
\c POPAD                                     386,NOLONG
\c POPAW                                     186,NOLONG
\c POPF                                      8086
\c POPFD                                     386,NOLONG
\c POPFQ                                     X64
\c POPFW                                     8086
\c POR              mmxreg,mmxrm             PENT,MMX
\c PREFETCH         mem                      PENT,3DNOW
\c PREFETCHW        mem                      PENT,3DNOW
\c PSLLD            mmxreg,mmxrm             PENT,MMX
\c PSLLD            mmxreg,imm               PENT,MMX
\c PSLLQ            mmxreg,mmxrm             PENT,MMX
\c PSLLQ            mmxreg,imm               PENT,MMX
\c PSLLW            mmxreg,mmxrm             PENT,MMX
\c PSLLW            mmxreg,imm               PENT,MMX
\c PSRAD            mmxreg,mmxrm             PENT,MMX
\c PSRAD            mmxreg,imm               PENT,MMX
\c PSRAW            mmxreg,mmxrm             PENT,MMX
\c PSRAW            mmxreg,imm               PENT,MMX
\c PSRLD            mmxreg,mmxrm             PENT,MMX
\c PSRLD            mmxreg,imm               PENT,MMX
\c PSRLQ            mmxreg,mmxrm             PENT,MMX
\c PSRLQ            mmxreg,imm               PENT,MMX
\c PSRLW            mmxreg,mmxrm             PENT,MMX
\c PSRLW            mmxreg,imm               PENT,MMX
\c PSUBB            mmxreg,mmxrm             PENT,MMX
\c PSUBD            mmxreg,mmxrm             PENT,MMX
\c PSUBSB           mmxreg,mmxrm             PENT,MMX
\c PSUBSIW          mmxreg,mmxrm             PENT,MMX,CYRIX
\c PSUBSW           mmxreg,mmxrm             PENT,MMX
\c PSUBUSB          mmxreg,mmxrm             PENT,MMX
\c PSUBUSW          mmxreg,mmxrm             PENT,MMX
\c PSUBW            mmxreg,mmxrm             PENT,MMX
\c PUNPCKHBW        mmxreg,mmxrm             PENT,MMX
\c PUNPCKHDQ        mmxreg,mmxrm             PENT,MMX
\c PUNPCKHWD        mmxreg,mmxrm             PENT,MMX
\c PUNPCKLBW        mmxreg,mmxrm             PENT,MMX
\c PUNPCKLDQ        mmxreg,mmxrm             PENT,MMX
\c PUNPCKLWD        mmxreg,mmxrm             PENT,MMX
\c PUSH             reg16                    8086
\c PUSH             reg32                    386,NOLONG
\c PUSH             reg64                    X64
\c PUSH             rm16                     8086
\c PUSH             rm32                     386,NOLONG
\c PUSH             rm64                     X64
\c PUSH             reg_cs                   8086,NOLONG
\c PUSH             reg_dess                 8086,NOLONG
\c PUSH             reg_fsgs                 386
\c PUSH             imm8                     186
\c PUSH             imm16                    186,AR0,SZ
\c PUSH             imm32                    386,NOLONG,AR0,SZ
\c PUSH             imm32                    386,NOLONG,SD
\c PUSH             imm64                    X64,AR0,SZ
\c PUSHA                                     186,NOLONG
\c PUSHAD                                    386,NOLONG
\c PUSHAW                                    186,NOLONG
\c PUSHF                                     8086
\c PUSHFD                                    386,NOLONG
\c PUSHFQ                                    X64
\c PUSHFW                                    8086
\c PXOR             mmxreg,mmxrm             PENT,MMX
\c RCL              rm8,unity                8086
\c RCL              rm8,reg_cl               8086
\c RCL              rm8,imm                  186
\c RCL              rm16,unity               8086
\c RCL              rm16,reg_cl              8086
\c RCL              rm16,imm                 186
\c RCL              rm32,unity               386
\c RCL              rm32,reg_cl              386
\c RCL              rm32,imm                 386
\c RCL              rm64,unity               X64
\c RCL              rm64,reg_cl              X64
\c RCL              rm64,imm                 X64
\c RCR              rm8,unity                8086
\c RCR              rm8,reg_cl               8086
\c RCR              rm8,imm                  186
\c RCR              rm16,unity               8086
\c RCR              rm16,reg_cl              8086
\c RCR              rm16,imm                 186
\c RCR              rm32,unity               386
\c RCR              rm32,reg_cl              386
\c RCR              rm32,imm                 386
\c RCR              rm64,unity               X64
\c RCR              rm64,reg_cl              X64
\c RCR              rm64,imm                 X64
\c RDSHR            rm32                     P6,CYRIXM
\c RDMSR                                     PENT,PRIV
\c RDPMC                                     P6
\c RDTSC                                     PENT
\c RDTSCP                                    X86_64
\c RET                                       8086
\c RET              imm                      8086,SW
\c RETF                                      8086
\c RETF             imm                      8086,SW
\c RETN                                      8086
\c RETN             imm                      8086,SW
\c ROL              rm8,unity                8086
\c ROL              rm8,reg_cl               8086
\c ROL              rm8,imm                  186
\c ROL              rm16,unity               8086
\c ROL              rm16,reg_cl              8086
\c ROL              rm16,imm                 186
\c ROL              rm32,unity               386
\c ROL              rm32,reg_cl              386
\c ROL              rm32,imm                 386
\c ROL              rm64,unity               X64
\c ROL              rm64,reg_cl              X64
\c ROL              rm64,imm                 X64
\c ROR              rm8,unity                8086
\c ROR              rm8,reg_cl               8086
\c ROR              rm8,imm                  186
\c ROR              rm16,unity               8086
\c ROR              rm16,reg_cl              8086
\c ROR              rm16,imm                 186
\c ROR              rm32,unity               386
\c ROR              rm32,reg_cl              386
\c ROR              rm32,imm                 386
\c ROR              rm64,unity               X64
\c ROR              rm64,reg_cl              X64
\c ROR              rm64,imm                 X64
\c RDM                                       P6,CYRIX,ND
\c RSDC             reg_sreg,mem80           486,CYRIXM
\c RSLDT            mem80                    486,CYRIXM
\c RSM                                       PENTM
\c RSTS             mem80                    486,CYRIXM
\c SAHF                                      8086
\c SAL              rm8,unity                8086,ND
\c SAL              rm8,reg_cl               8086,ND
\c SAL              rm8,imm                  186,ND
\c SAL              rm16,unity               8086,ND
\c SAL              rm16,reg_cl              8086,ND
\c SAL              rm16,imm                 186,ND
\c SAL              rm32,unity               386,ND
\c SAL              rm32,reg_cl              386,ND
\c SAL              rm32,imm                 386,ND
\c SAL              rm64,unity               X64,ND
\c SAL              rm64,reg_cl              X64,ND
\c SAL              rm64,imm                 X64,ND
\c SALC                                      8086,UNDOC
\c SAR              rm8,unity                8086
\c SAR              rm8,reg_cl               8086
\c SAR              rm8,imm                  186
\c SAR              rm16,unity               8086
\c SAR              rm16,reg_cl              8086
\c SAR              rm16,imm                 186
\c SAR              rm32,unity               386
\c SAR              rm32,reg_cl              386
\c SAR              rm32,imm                 386
\c SAR              rm64,unity               X64
\c SAR              rm64,reg_cl              X64
\c SAR              rm64,imm                 X64
\c SBB              mem,reg8                 8086
\c SBB              reg8,reg8                8086
\c SBB              mem,reg16                8086
\c SBB              reg16,reg16              8086
\c SBB              mem,reg32                386
\c SBB              reg32,reg32              386
\c SBB              mem,reg64                X64
\c SBB              reg64,reg64              X64
\c SBB              reg8,mem                 8086
\c SBB              reg8,reg8                8086
\c SBB              reg16,mem                8086
\c SBB              reg16,reg16              8086
\c SBB              reg32,mem                386
\c SBB              reg32,reg32              386
\c SBB              reg64,mem                X64
\c SBB              reg64,reg64              X64
\c SBB              rm16,imm8                8086
\c SBB              rm32,imm8                386
\c SBB              rm64,imm8                X64
\c SBB              reg_al,imm               8086
\c SBB              reg_ax,imm               8086
\c SBB              reg_eax,imm              386
\c SBB              reg_rax,imm              X64
\c SBB              rm8,imm                  8086
\c SBB              rm16,imm                 8086
\c SBB              rm32,imm                 386
\c SBB              rm64,imm                 X64
\c SBB              mem,imm8                 8086
\c SBB              mem,imm16                8086
\c SBB              mem,imm32                386
\c SCASB                                     8086
\c SCASD                                     386
\c SCASQ                                     X64
\c SCASW                                     8086
\c SFENCE                                    X64,AMD
\c SGDT             mem                      286
\c SHL              rm8,unity                8086
\c SHL              rm8,reg_cl               8086
\c SHL              rm8,imm                  186
\c SHL              rm16,unity               8086
\c SHL              rm16,reg_cl              8086
\c SHL              rm16,imm                 186
\c SHL              rm32,unity               386
\c SHL              rm32,reg_cl              386
\c SHL              rm32,imm                 386
\c SHL              rm64,unity               X64
\c SHL              rm64,reg_cl              X64
\c SHL              rm64,imm                 X64
\c SHLD             mem,reg16,imm            3862
\c SHLD             reg16,reg16,imm          3862
\c SHLD             mem,reg32,imm            3862
\c SHLD             reg32,reg32,imm          3862
\c SHLD             mem,reg64,imm            X642
\c SHLD             reg64,reg64,imm          X642
\c SHLD             mem,reg16,reg_cl         386
\c SHLD             reg16,reg16,reg_cl       386
\c SHLD             mem,reg32,reg_cl         386
\c SHLD             reg32,reg32,reg_cl       386
\c SHLD             mem,reg64,reg_cl         X64
\c SHLD             reg64,reg64,reg_cl       X64
\c SHR              rm8,unity                8086
\c SHR              rm8,reg_cl               8086
\c SHR              rm8,imm                  186
\c SHR              rm16,unity               8086
\c SHR              rm16,reg_cl              8086
\c SHR              rm16,imm                 186
\c SHR              rm32,unity               386
\c SHR              rm32,reg_cl              386
\c SHR              rm32,imm                 386
\c SHR              rm64,unity               X64
\c SHR              rm64,reg_cl              X64
\c SHR              rm64,imm                 X64
\c SHRD             mem,reg16,imm            3862
\c SHRD             reg16,reg16,imm          3862
\c SHRD             mem,reg32,imm            3862
\c SHRD             reg32,reg32,imm          3862
\c SHRD             mem,reg64,imm            X642
\c SHRD             reg64,reg64,imm          X642
\c SHRD             mem,reg16,reg_cl         386
\c SHRD             reg16,reg16,reg_cl       386
\c SHRD             mem,reg32,reg_cl         386
\c SHRD             reg32,reg32,reg_cl       386
\c SHRD             mem,reg64,reg_cl         X64
\c SHRD             reg64,reg64,reg_cl       X64
\c SIDT             mem                      286
\c SLDT             mem                      286
\c SLDT             mem16                    286
\c SLDT             reg16                    286
\c SLDT             reg32                    386
\c SLDT             reg64                    X64,ND
\c SLDT             reg64                    X64
\c SKINIT                                    X64
\c SMI                                       386,UNDOC
\c SMINT                                     P6,CYRIX,ND
\c SMINTOLD                                  486,CYRIX,ND
\c SMSW             mem                      286
\c SMSW             mem16                    286
\c SMSW             reg16                    286
\c SMSW             reg32                    386
\c STC                                       8086
\c STD                                       8086
\c STGI                                      X64
\c STI                                       8086
\c STOSB                                     8086
\c STOSD                                     386
\c STOSQ                                     X64
\c STOSW                                     8086
\c STR              mem                      286,PROT
\c STR              mem16                    286,PROT
\c STR              reg16                    286,PROT
\c STR              reg32                    386,PROT
\c STR              reg64                    X64
\c SUB              mem,reg8                 8086
\c SUB              reg8,reg8                8086
\c SUB              mem,reg16                8086
\c SUB              reg16,reg16              8086
\c SUB              mem,reg32                386
\c SUB              reg32,reg32              386
\c SUB              mem,reg64                X64
\c SUB              reg64,reg64              X64
\c SUB              reg8,mem                 8086
\c SUB              reg8,reg8                8086
\c SUB              reg16,mem                8086
\c SUB              reg16,reg16              8086
\c SUB              reg32,mem                386
\c SUB              reg32,reg32              386
\c SUB              reg64,mem                X64
\c SUB              reg64,reg64              X64
\c SUB              rm16,imm8                8086
\c SUB              rm32,imm8                386
\c SUB              rm64,imm8                X64
\c SUB              reg_al,imm               8086
\c SUB              reg_ax,imm               8086
\c SUB              reg_eax,imm              386
\c SUB              reg_rax,imm              X64
\c SUB              rm8,imm                  8086
\c SUB              rm16,imm                 8086
\c SUB              rm32,imm                 386
\c SUB              rm64,imm                 X64
\c SUB              mem,imm8                 8086
\c SUB              mem,imm16                8086
\c SUB              mem,imm32                386
\c SVDC             mem80,reg_sreg           486,CYRIXM
\c SVLDT            mem80                    486,CYRIXM,ND
\c SVTS             mem80                    486,CYRIXM
\c SWAPGS                                    X64
\c SYSCALL                                   P6,AMD
\c SYSENTER                                  P6
\c SYSEXIT                                   P6,PRIV
\c SYSRET                                    P6,PRIV,AMD
\c TEST             mem,reg8                 8086
\c TEST             reg8,reg8                8086
\c TEST             mem,reg16                8086
\c TEST             reg16,reg16              8086
\c TEST             mem,reg32                386
\c TEST             reg32,reg32              386
\c TEST             mem,reg64                X64
\c TEST             reg64,reg64              X64
\c TEST             reg8,mem                 8086
\c TEST             reg16,mem                8086
\c TEST             reg32,mem                386
\c TEST             reg64,mem                X64
\c TEST             reg_al,imm               8086
\c TEST             reg_ax,imm               8086
\c TEST             reg_eax,imm              386
\c TEST             reg_rax,imm              X64
\c TEST             rm8,imm                  8086
\c TEST             rm16,imm                 8086
\c TEST             rm32,imm                 386
\c TEST             rm64,imm                 X64
\c TEST             mem,imm8                 8086
\c TEST             mem,imm16                8086
\c TEST             mem,imm32                386
\c UD0                                       186,UNDOC
\c UD1                                       186,UNDOC
\c UD2B                                      186,UNDOC,ND
\c UD2                                       186
\c UD2A                                      186,ND
\c UMOV             mem,reg8                 386,UNDOC,ND
\c UMOV             reg8,reg8                386,UNDOC,ND
\c UMOV             mem,reg16                386,UNDOC,ND
\c UMOV             reg16,reg16              386,UNDOC,ND
\c UMOV             mem,reg32                386,UNDOC,ND
\c UMOV             reg32,reg32              386,UNDOC,ND
\c UMOV             reg8,mem                 386,UNDOC,ND
\c UMOV             reg8,reg8                386,UNDOC,ND
\c UMOV             reg16,mem                386,UNDOC,ND
\c UMOV             reg16,reg16              386,UNDOC,ND
\c UMOV             reg32,mem                386,UNDOC,ND
\c UMOV             reg32,reg32              386,UNDOC,ND
\c VERR             mem                      286,PROT
\c VERR             mem16                    286,PROT
\c VERR             reg16                    286,PROT
\c VERW             mem                      286,PROT
\c VERW             mem16                    286,PROT
\c VERW             reg16                    286,PROT
\c WAIT                                      8086
\c FWAIT                                     8086
\c WBINVD                                    486,PRIV
\c WRSHR            rm32                     P6,CYRIXM
\c WRMSR                                     PENT,PRIV
\c XADD             mem,reg8                 486
\c XADD             reg8,reg8                486
\c XADD             mem,reg16                486
\c XADD             reg16,reg16              486
\c XADD             mem,reg32                486
\c XADD             reg32,reg32              486
\c XADD             mem,reg64                X64
\c XADD             reg64,reg64              X64
\c XBTS             reg16,mem                386,SW,UNDOC,ND
\c XBTS             reg16,reg16              386,UNDOC,ND
\c XBTS             reg32,mem                386,SD,UNDOC,ND
\c XBTS             reg32,reg32              386,UNDOC,ND
\c XCHG             reg_ax,reg16             8086
\c XCHG             reg_eax,reg32na          386
\c XCHG             reg_rax,reg64            X64
\c XCHG             reg16,reg_ax             8086
\c XCHG             reg32na,reg_eax          386
\c XCHG             reg64,reg_rax            X64
\c XCHG             reg_eax,reg_eax          386,NOLONG
\c XCHG             reg8,mem                 8086
\c XCHG             reg8,reg8                8086
\c XCHG             reg16,mem                8086
\c XCHG             reg16,reg16              8086
\c XCHG             reg32,mem                386
\c XCHG             reg32,reg32              386
\c XCHG             reg64,mem                X64
\c XCHG             reg64,reg64              X64
\c XCHG             mem,reg8                 8086
\c XCHG             reg8,reg8                8086
\c XCHG             mem,reg16                8086
\c XCHG             reg16,reg16              8086
\c XCHG             mem,reg32                386
\c XCHG             reg32,reg32              386
\c XCHG             mem,reg64                X64
\c XCHG             reg64,reg64              X64
\c XLATB                                     8086
\c XLAT                                      8086
\c XOR              mem,reg8                 8086
\c XOR              reg8,reg8                8086
\c XOR              mem,reg16                8086
\c XOR              reg16,reg16              8086
\c XOR              mem,reg32                386
\c XOR              reg32,reg32              386
\c XOR              mem,reg64                X64
\c XOR              reg64,reg64              X64
\c XOR              reg8,mem                 8086
\c XOR              reg8,reg8                8086
\c XOR              reg16,mem                8086
\c XOR              reg16,reg16              8086
\c XOR              reg32,mem                386
\c XOR              reg32,reg32              386
\c XOR              reg64,mem                X64
\c XOR              reg64,reg64              X64
\c XOR              rm16,imm8                8086
\c XOR              rm32,imm8                386
\c XOR              rm64,imm8                X64
\c XOR              reg_al,imm               8086
\c XOR              reg_ax,imm               8086
\c XOR              reg_eax,imm              386
\c XOR              reg_rax,imm              X64
\c XOR              rm8,imm                  8086
\c XOR              rm16,imm                 8086
\c XOR              rm32,imm                 386
\c XOR              rm64,imm                 X64
\c XOR              mem,imm8                 8086
\c XOR              mem,imm16                8086
\c XOR              mem,imm32                386
\c CMOVcc           reg16,mem                P6
\c CMOVcc           reg16,reg16              P6
\c CMOVcc           reg32,mem                P6
\c CMOVcc           reg32,reg32              P6
\c CMOVcc           reg64,mem                X64
\c CMOVcc           reg64,reg64              X64
\c Jcc              imm|near                 386
\c Jcc              imm16|near               386
\c Jcc              imm32|near               386
\c Jcc              imm|short                8086,ND
\c Jcc              imm                      8086,ND
\c Jcc              imm                      386,ND
\c Jcc              imm                      8086,ND
\c Jcc              imm                      8086
\c SETcc            mem                      386
\c SETcc            reg8                     386

\S{} Katmai Streaming SIMD instructions (SSE -- a.k.a. KNI, XMM, MMX2)

\c ADDPS            xmmreg,xmmrm             KATMAI,SSE
\c ADDSS            xmmreg,xmmrm             KATMAI,SSE,SD
\c ANDNPS           xmmreg,xmmrm             KATMAI,SSE
\c ANDPS            xmmreg,xmmrm             KATMAI,SSE
\c CMPEQPS          xmmreg,xmmrm             KATMAI,SSE
\c CMPEQSS          xmmreg,xmmrm             KATMAI,SSE
\c CMPLEPS          xmmreg,xmmrm             KATMAI,SSE
\c CMPLESS          xmmreg,xmmrm             KATMAI,SSE
\c CMPLTPS          xmmreg,xmmrm             KATMAI,SSE
\c CMPLTSS          xmmreg,xmmrm             KATMAI,SSE
\c CMPNEQPS         xmmreg,xmmrm             KATMAI,SSE
\c CMPNEQSS         xmmreg,xmmrm             KATMAI,SSE
\c CMPNLEPS         xmmreg,xmmrm             KATMAI,SSE
\c CMPNLESS         xmmreg,xmmrm             KATMAI,SSE
\c CMPNLTPS         xmmreg,xmmrm             KATMAI,SSE
\c CMPNLTSS         xmmreg,xmmrm             KATMAI,SSE
\c CMPORDPS         xmmreg,xmmrm             KATMAI,SSE
\c CMPORDSS         xmmreg,xmmrm             KATMAI,SSE
\c CMPUNORDPS       xmmreg,xmmrm             KATMAI,SSE
\c CMPUNORDSS       xmmreg,xmmrm             KATMAI,SSE
\c CMPPS            xmmreg,mem,imm           KATMAI,SSE
\c CMPPS            xmmreg,xmmreg,imm        KATMAI,SSE
\c CMPSS            xmmreg,mem,imm           KATMAI,SSE
\c CMPSS            xmmreg,xmmreg,imm        KATMAI,SSE
\c COMISS           xmmreg,xmmrm             KATMAI,SSE
\c CVTPI2PS         xmmreg,mmxrm             KATMAI,SSE,MMX
\c CVTPS2PI         mmxreg,xmmrm             KATMAI,SSE,MMX
\c CVTSI2SS         xmmreg,mem               KATMAI,SSE,SD,AR1,ND
\c CVTSI2SS         xmmreg,rm32              KATMAI,SSE,SD,AR1
\c CVTSI2SS         xmmreg,rm64              X64,SSE,AR1
\c CVTSS2SI         reg32,xmmreg             KATMAI,SSE,SD,AR1
\c CVTSS2SI         reg32,mem                KATMAI,SSE,SD,AR1
\c CVTSS2SI         reg64,xmmreg             X64,SSE,SD,AR1
\c CVTSS2SI         reg64,mem                X64,SSE,SD,AR1
\c CVTTPS2PI        mmxreg,xmmrm             KATMAI,SSE,MMX
\c CVTTSS2SI        reg32,xmmrm              KATMAI,SSE,SD,AR1
\c CVTTSS2SI        reg64,xmmrm              X64,SSE,SD,AR1
\c DIVPS            xmmreg,xmmrm             KATMAI,SSE
\c DIVSS            xmmreg,xmmrm             KATMAI,SSE
\c LDMXCSR          mem                      KATMAI,SSE,SD
\c MAXPS            xmmreg,xmmrm             KATMAI,SSE
\c MAXSS            xmmreg,xmmrm             KATMAI,SSE
\c MINPS            xmmreg,xmmrm             KATMAI,SSE
\c MINSS            xmmreg,xmmrm             KATMAI,SSE
\c MOVAPS           xmmreg,mem               KATMAI,SSE
\c MOVAPS           mem,xmmreg               KATMAI,SSE
\c MOVAPS           xmmreg,xmmreg            KATMAI,SSE
\c MOVAPS           xmmreg,xmmreg            KATMAI,SSE
\c MOVHPS           xmmreg,mem               KATMAI,SSE
\c MOVHPS           mem,xmmreg               KATMAI,SSE
\c MOVLHPS          xmmreg,xmmreg            KATMAI,SSE
\c MOVLPS           xmmreg,mem               KATMAI,SSE
\c MOVLPS           mem,xmmreg               KATMAI,SSE
\c MOVHLPS          xmmreg,xmmreg            KATMAI,SSE
\c MOVMSKPS         reg32,xmmreg             KATMAI,SSE
\c MOVMSKPS         reg64,xmmreg             X64,SSE
\c MOVNTPS          mem,xmmreg               KATMAI,SSE
\c MOVSS            xmmreg,mem               KATMAI,SSE
\c MOVSS            mem,xmmreg               KATMAI,SSE
\c MOVSS            xmmreg,xmmreg            KATMAI,SSE
\c MOVSS            xmmreg,xmmreg            KATMAI,SSE
\c MOVUPS           xmmreg,mem               KATMAI,SSE
\c MOVUPS           mem,xmmreg               KATMAI,SSE
\c MOVUPS           xmmreg,xmmreg            KATMAI,SSE
\c MOVUPS           xmmreg,xmmreg            KATMAI,SSE
\c MULPS            xmmreg,xmmrm             KATMAI,SSE
\c MULSS            xmmreg,xmmrm             KATMAI,SSE
\c ORPS             xmmreg,xmmrm             KATMAI,SSE
\c RCPPS            xmmreg,xmmrm             KATMAI,SSE
\c RCPSS            xmmreg,xmmrm             KATMAI,SSE
\c RSQRTPS          xmmreg,xmmrm             KATMAI,SSE
\c RSQRTSS          xmmreg,xmmrm             KATMAI,SSE
\c SHUFPS           xmmreg,mem,imm           KATMAI,SSE
\c SHUFPS           xmmreg,xmmreg,imm        KATMAI,SSE
\c SQRTPS           xmmreg,xmmrm             KATMAI,SSE
\c SQRTSS           xmmreg,xmmrm             KATMAI,SSE
\c STMXCSR          mem                      KATMAI,SSE,SD
\c SUBPS            xmmreg,xmmrm             KATMAI,SSE
\c SUBSS            xmmreg,xmmrm             KATMAI,SSE
\c UCOMISS          xmmreg,xmmrm             KATMAI,SSE
\c UNPCKHPS         xmmreg,xmmrm             KATMAI,SSE
\c UNPCKLPS         xmmreg,xmmrm             KATMAI,SSE
\c XORPS            xmmreg,xmmrm             KATMAI,SSE

\S{} Introduced in Deschutes but necessary for SSE support

\c FXRSTOR          mem                      P6,SSE,FPU
\c FXSAVE           mem                      P6,SSE,FPU

\S{} XSAVE group (AVX and extended state)

\c XGETBV                                    NEHALEM
\c XSETBV                                    NEHALEM,PRIV
\c XSAVE            mem                      NEHALEM
\c XRSTOR           mem                      NEHALEM

\S{} Generic memory operations

\c PREFETCHNTA      mem                      KATMAI
\c PREFETCHT0       mem                      KATMAI
\c PREFETCHT1       mem                      KATMAI
\c PREFETCHT2       mem                      KATMAI
\c SFENCE                                    KATMAI

\S{} New MMX instructions introduced in Katmai

\c MASKMOVQ         mmxreg,mmxreg            KATMAI,MMX
\c MOVNTQ           mem,mmxreg               KATMAI,MMX
\c PAVGB            mmxreg,mmxrm             KATMAI,MMX
\c PAVGW            mmxreg,mmxrm             KATMAI,MMX
\c PEXTRW           reg32,mmxreg,imm         KATMAI,MMX
\c PINSRW           mmxreg,reg16,imm         KATMAI,MMX
\c PINSRW           mmxreg,reg32,imm         KATMAI,MMX,ND
\c PINSRW           mmxreg,mem,imm           KATMAI,MMX
\c PINSRW           mmxreg,mem16,imm         KATMAI,MMX,ND
\c PMAXSW           mmxreg,mmxrm             KATMAI,MMX
\c PMAXUB           mmxreg,mmxrm             KATMAI,MMX
\c PMINSW           mmxreg,mmxrm             KATMAI,MMX
\c PMINUB           mmxreg,mmxrm             KATMAI,MMX
\c PMOVMSKB         reg32,mmxreg             KATMAI,MMX
\c PMULHUW          mmxreg,mmxrm             KATMAI,MMX
\c PSADBW           mmxreg,mmxrm             KATMAI,MMX
\c PSHUFW           mmxreg,mmxrm,imm         KATMAI,MMX2

\S{} AMD Enhanced 3DNow! (Athlon) instructions

\c PF2IW            mmxreg,mmxrm             PENT,3DNOW
\c PFNACC           mmxreg,mmxrm             PENT,3DNOW
\c PFPNACC          mmxreg,mmxrm             PENT,3DNOW
\c PI2FW            mmxreg,mmxrm             PENT,3DNOW
\c PSWAPD           mmxreg,mmxrm             PENT,3DNOW

\S{} Willamette SSE2 Cacheability Instructions

\c MASKMOVDQU       xmmreg,xmmreg            WILLAMETTE,SSE2
\c CLFLUSH          mem                      WILLAMETTE,SSE2
\c MOVNTDQ          mem,xmmreg               WILLAMETTE,SSE2,SO
\c MOVNTI           mem,reg32                WILLAMETTE,SD
\c MOVNTI           mem,reg64                X64
\c MOVNTPD          mem,xmmreg               WILLAMETTE,SSE2,SO
\c LFENCE                                    WILLAMETTE,SSE2
\c MFENCE                                    WILLAMETTE,SSE2

\S{} Willamette MMX instructions (SSE2 SIMD Integer Instructions)

\c MOVD             xmmreg,reg32             WILLAMETTE,SSE2
\c MOVD             reg32,xmmreg             WILLAMETTE,SSE2
\c MOVD             mem,xmmreg               WILLAMETTE,SSE2,SD
\c MOVD             xmmreg,mem               WILLAMETTE,SSE2,SD
\c MOVDQA           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVDQA           mem,xmmreg               WILLAMETTE,SSE2,SO
\c MOVDQA           xmmreg,mem               WILLAMETTE,SSE2,SO
\c MOVDQA           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVDQU           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVDQU           mem,xmmreg               WILLAMETTE,SSE2,SO
\c MOVDQU           xmmreg,mem               WILLAMETTE,SSE2,SO
\c MOVDQU           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVDQ2Q          mmxreg,xmmreg            WILLAMETTE,SSE2
\c MOVQ             xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVQ             xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVQ             mem,xmmreg               WILLAMETTE,SSE2
\c MOVQ             xmmreg,mem               WILLAMETTE,SSE2
\c MOVQ             xmmreg,rm64              X64,SSE2
\c MOVQ             rm64,xmmreg              X64,SSE2
\c MOVQ2DQ          xmmreg,mmxreg            WILLAMETTE,SSE2
\c PACKSSWB         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PACKSSDW         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PACKUSWB         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDB            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDQ            mmxreg,mmxrm             WILLAMETTE,SSE2,SO
\c PADDQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDSB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDUSB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PADDUSW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PAND             xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PANDN            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PAVGB            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PAVGW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PCMPEQB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PCMPEQW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PCMPEQD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PCMPGTB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PCMPGTW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PCMPGTD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PEXTRW           reg32,xmmreg,imm         WILLAMETTE,SSE2
\c PINSRW           xmmreg,reg16,imm         WILLAMETTE,SSE2
\c PINSRW           xmmreg,reg32,imm         WILLAMETTE,SSE2,ND
\c PINSRW           xmmreg,mem,imm           WILLAMETTE,SSE2
\c PINSRW           xmmreg,mem16,imm         WILLAMETTE,SSE2,ND
\c PMADDWD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMAXSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMAXUB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMINSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMINUB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMOVMSKB         reg32,xmmreg             WILLAMETTE,SSE2
\c PMULHUW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMULHW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMULLW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PMULUDQ          mmxreg,mmxrm             WILLAMETTE,SSE2,SO
\c PMULUDQ          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c POR              xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSADBW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSHUFD           xmmreg,xmmreg,imm        WILLAMETTE,SSE2
\c PSHUFD           xmmreg,mem,imm           WILLAMETTE,SSE22
\c PSHUFHW          xmmreg,xmmreg,imm        WILLAMETTE,SSE2
\c PSHUFHW          xmmreg,mem,imm           WILLAMETTE,SSE22
\c PSHUFLW          xmmreg,xmmreg,imm        WILLAMETTE,SSE2
\c PSHUFLW          xmmreg,mem,imm           WILLAMETTE,SSE22
\c PSLLDQ           xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSLLW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSLLW            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSLLD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSLLD            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSLLQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSLLQ            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSRAW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSRAW            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSRAD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSRAD            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSRLDQ           xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSRLW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSRLW            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSRLD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSRLD            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSRLQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSRLQ            xmmreg,imm               WILLAMETTE,SSE2,AR1
\c PSUBB            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSUBW            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSUBD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSUBQ            mmxreg,mmxrm             WILLAMETTE,SSE2,SO
\c PSUBQ            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSUBSB           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSUBSW           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSUBUSB          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PSUBUSW          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKHBW        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKHWD        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKHDQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKHQDQ       xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKLBW        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKLWD        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKLDQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PUNPCKLQDQ       xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c PXOR             xmmreg,xmmrm             WILLAMETTE,SSE2,SO

\S{} Willamette Streaming SIMD instructions (SSE2)

\c ADDPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c ADDSD            xmmreg,xmmrm             WILLAMETTE,SSE2
\c ANDNPD           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c ANDPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPEQPD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPEQSD          xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPLEPD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPLESD          xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPLTPD          xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPLTSD          xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPNEQPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPNEQSD         xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPNLEPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPNLESD         xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPNLTPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPNLTSD         xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPORDPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPORDSD         xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPUNORDPD       xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CMPUNORDSD       xmmreg,xmmrm             WILLAMETTE,SSE2
\c CMPPD            xmmreg,xmmrm,imm         WILLAMETTE,SSE22
\c CMPSD            xmmreg,xmmrm,imm         WILLAMETTE,SSE2
\c COMISD           xmmreg,xmmrm             WILLAMETTE,SSE2
\c CVTDQ2PD         xmmreg,xmmrm             WILLAMETTE,SSE2
\c CVTDQ2PS         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTPD2DQ         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTPD2PI         mmxreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTPD2PS         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTPI2PD         xmmreg,mmxrm             WILLAMETTE,SSE2
\c CVTPS2DQ         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTPS2PD         xmmreg,xmmrm             WILLAMETTE,SSE2
\c CVTSD2SI         reg32,xmmreg             WILLAMETTE,SSE2,AR1
\c CVTSD2SI         reg32,mem                WILLAMETTE,SSE2,AR1
\c CVTSD2SI         reg64,xmmreg             X64,SSE2,AR1
\c CVTSD2SI         reg64,mem                X64,SSE2,AR1
\c CVTSD2SS         xmmreg,xmmrm             WILLAMETTE,SSE2
\c CVTSI2SD         xmmreg,mem               WILLAMETTE,SSE2,SD,AR1,ND
\c CVTSI2SD         xmmreg,rm32              WILLAMETTE,SSE2,SD,AR1
\c CVTSI2SD         xmmreg,rm64              X64,SSE2,AR1
\c CVTSS2SD         xmmreg,xmmrm             WILLAMETTE,SSE2,SD
\c CVTTPD2PI        mmxreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTTPD2DQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTTPS2DQ        xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c CVTTSD2SI        reg32,xmmreg             WILLAMETTE,SSE2,AR1
\c CVTTSD2SI        reg32,mem                WILLAMETTE,SSE2,AR1
\c CVTTSD2SI        reg64,xmmreg             X64,SSE2,AR1
\c CVTTSD2SI        reg64,mem                X64,SSE2,AR1
\c DIVPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c DIVSD            xmmreg,xmmrm             WILLAMETTE,SSE2
\c MAXPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c MAXSD            xmmreg,xmmrm             WILLAMETTE,SSE2
\c MINPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c MINSD            xmmreg,xmmrm             WILLAMETTE,SSE2
\c MOVAPD           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVAPD           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVAPD           mem,xmmreg               WILLAMETTE,SSE2,SO
\c MOVAPD           xmmreg,mem               WILLAMETTE,SSE2,SO
\c MOVHPD           mem,xmmreg               WILLAMETTE,SSE2
\c MOVHPD           xmmreg,mem               WILLAMETTE,SSE2
\c MOVLPD           mem,xmmreg               WILLAMETTE,SSE2
\c MOVLPD           xmmreg,mem               WILLAMETTE,SSE2
\c MOVMSKPD         reg32,xmmreg             WILLAMETTE,SSE2
\c MOVMSKPD         reg64,xmmreg             X64,SSE2
\c MOVSD            xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVSD            xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVSD            mem,xmmreg               WILLAMETTE,SSE2
\c MOVSD            xmmreg,mem               WILLAMETTE,SSE2
\c MOVUPD           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVUPD           xmmreg,xmmreg            WILLAMETTE,SSE2
\c MOVUPD           mem,xmmreg               WILLAMETTE,SSE2,SO
\c MOVUPD           xmmreg,mem               WILLAMETTE,SSE2,SO
\c MULPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c MULSD            xmmreg,xmmrm             WILLAMETTE,SSE2
\c ORPD             xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c SHUFPD           xmmreg,xmmreg,imm        WILLAMETTE,SSE2
\c SHUFPD           xmmreg,mem,imm           WILLAMETTE,SSE2
\c SQRTPD           xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c SQRTSD           xmmreg,xmmrm             WILLAMETTE,SSE2
\c SUBPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c SUBSD            xmmreg,xmmrm             WILLAMETTE,SSE2
\c UCOMISD          xmmreg,xmmrm             WILLAMETTE,SSE2
\c UNPCKHPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c UNPCKLPD         xmmreg,xmmrm             WILLAMETTE,SSE2,SO
\c XORPD            xmmreg,xmmrm             WILLAMETTE,SSE2,SO

\S{} Prescott New Instructions (SSE3)

\c ADDSUBPD         xmmreg,xmmrm             PRESCOTT,SSE3,SO
\c ADDSUBPS         xmmreg,xmmrm             PRESCOTT,SSE3,SO
\c HADDPD           xmmreg,xmmrm             PRESCOTT,SSE3,SO
\c HADDPS           xmmreg,xmmrm             PRESCOTT,SSE3,SO
\c HSUBPD           xmmreg,xmmrm             PRESCOTT,SSE3,SO
\c HSUBPS           xmmreg,xmmrm             PRESCOTT,SSE3,SO
\c LDDQU            xmmreg,mem               PRESCOTT,SSE3,SO
\c MOVDDUP          xmmreg,xmmrm             PRESCOTT,SSE3
\c MOVSHDUP         xmmreg,xmmrm             PRESCOTT,SSE3
\c MOVSLDUP         xmmreg,xmmrm             PRESCOTT,SSE3

\S{} VMX Instructions

\c VMCALL                                    VMX
\c VMCLEAR          mem                      VMX
\c VMLAUNCH                                  VMX
\c VMLOAD                                    X64,VMX
\c VMMCALL                                   X64,VMX
\c VMPTRLD          mem                      VMX
\c VMPTRST          mem                      VMX
\c VMREAD           rm32,reg32               VMX,NOLONG,SD
\c VMREAD           rm64,reg64               X64,VMX
\c VMRESUME                                  VMX
\c VMRUN                                     X64,VMX
\c VMSAVE                                    X64,VMX
\c VMWRITE          reg32,rm32               VMX,NOLONG,SD
\c VMWRITE          reg64,rm64               X64,VMX
\c VMXOFF                                    VMX
\c VMXON            mem                      VMX

\S{} Extended Page Tables VMX instructions

\c INVEPT           reg32,mem                VMX,SO,NOLONG
\c INVEPT           reg64,mem                VMX,SO,LONG
\c INVVPID          reg32,mem                VMX,SO,NOLONG
\c INVVPID          reg64,mem                VMX,SO,LONG

\S{} Tejas New Instructions (SSSE3)

\c PABSB            mmxreg,mmxrm             SSSE3,MMX
\c PABSB            xmmreg,xmmrm             SSSE3
\c PABSW            mmxreg,mmxrm             SSSE3,MMX
\c PABSW            xmmreg,xmmrm             SSSE3
\c PABSD            mmxreg,mmxrm             SSSE3,MMX
\c PABSD            xmmreg,xmmrm             SSSE3
\c PALIGNR          mmxreg,mmxrm,imm         SSSE3,MMX
\c PALIGNR          xmmreg,xmmrm,imm         SSSE3
\c PHADDW           mmxreg,mmxrm             SSSE3,MMX
\c PHADDW           xmmreg,xmmrm             SSSE3
\c PHADDD           mmxreg,mmxrm             SSSE3,MMX
\c PHADDD           xmmreg,xmmrm             SSSE3
\c PHADDSW          mmxreg,mmxrm             SSSE3,MMX
\c PHADDSW          xmmreg,xmmrm             SSSE3
\c PHSUBW           mmxreg,mmxrm             SSSE3,MMX
\c PHSUBW           xmmreg,xmmrm             SSSE3
\c PHSUBD           mmxreg,mmxrm             SSSE3,MMX
\c PHSUBD           xmmreg,xmmrm             SSSE3
\c PHSUBSW          mmxreg,mmxrm             SSSE3,MMX
\c PHSUBSW          xmmreg,xmmrm             SSSE3
\c PMADDUBSW        mmxreg,mmxrm             SSSE3,MMX
\c PMADDUBSW        xmmreg,xmmrm             SSSE3
\c PMULHRSW         mmxreg,mmxrm             SSSE3,MMX
\c PMULHRSW         xmmreg,xmmrm             SSSE3
\c PSHUFB           mmxreg,mmxrm             SSSE3,MMX
\c PSHUFB           xmmreg,xmmrm             SSSE3
\c PSIGNB           mmxreg,mmxrm             SSSE3,MMX
\c PSIGNB           xmmreg,xmmrm             SSSE3
\c PSIGNW           mmxreg,mmxrm             SSSE3,MMX
\c PSIGNW           xmmreg,xmmrm             SSSE3
\c PSIGND           mmxreg,mmxrm             SSSE3,MMX
\c PSIGND           xmmreg,xmmrm             SSSE3

\S{} AMD SSE4A

\c EXTRQ            xmmreg,imm,imm           SSE4A,AMD
\c EXTRQ            xmmreg,xmmreg            SSE4A,AMD
\c INSERTQ          xmmreg,xmmreg,imm,imm    SSE4A,AMD
\c INSERTQ          xmmreg,xmmreg            SSE4A,AMD
\c MOVNTSD          mem,xmmreg               SSE4A,AMD
\c MOVNTSS          mem,xmmreg               SSE4A,AMD,SD

\S{} New instructions in Barcelona

\c LZCNT            reg16,rm16               P6,AMD
\c LZCNT            reg32,rm32               P6,AMD
\c LZCNT            reg64,rm64               P6,AMD

\S{} Penryn New Instructions (SSE4.1)

\c BLENDPD          xmmreg,xmmrm,imm         SSE41
\c BLENDPS          xmmreg,xmmrm,imm         SSE41
\c BLENDVPD         xmmreg,xmmrm,xmm0        SSE41
\c BLENDVPS         xmmreg,xmmrm,xmm0        SSE41
\c DPPD             xmmreg,xmmrm,imm         SSE41
\c DPPS             xmmreg,xmmrm,imm         SSE41
\c EXTRACTPS        rm32,xmmreg,imm          SSE41
\c EXTRACTPS        reg64,xmmreg,imm         SSE41,X64
\c INSERTPS         xmmreg,xmmrm,imm         SSE41,SD
\c MOVNTDQA         xmmreg,mem               SSE41
\c MPSADBW          xmmreg,xmmrm,imm         SSE41
\c PACKUSDW         xmmreg,xmmrm             SSE41
\c PBLENDVB         xmmreg,xmmrm,xmm0        SSE41
\c PBLENDW          xmmreg,xmmrm,imm         SSE41
\c PCMPEQQ          xmmreg,xmmrm             SSE41
\c PEXTRB           reg32,xmmreg,imm         SSE41
\c PEXTRB           mem8,xmmreg,imm          SSE41
\c PEXTRB           reg64,xmmreg,imm         SSE41,X64
\c PEXTRD           rm32,xmmreg,imm          SSE41
\c PEXTRQ           rm64,xmmreg,imm          SSE41,X64
\c PEXTRW           reg32,xmmreg,imm         SSE41
\c PEXTRW           mem16,xmmreg,imm         SSE41
\c PEXTRW           reg64,xmmreg,imm         SSE41,X64
\c PHMINPOSUW       xmmreg,xmmrm             SSE41
\c PINSRB           xmmreg,reg32,imm         SSE41
\c PINSRB           xmmreg,mem8,imm          SSE41
\c PINSRD           xmmreg,rm32,imm          SSE41
\c PINSRQ           xmmreg,rm64,imm          SSE41,X64
\c PMAXSB           xmmreg,xmmrm             SSE41
\c PMAXSD           xmmreg,xmmrm             SSE41
\c PMAXUD           xmmreg,xmmrm             SSE41
\c PMAXUW           xmmreg,xmmrm             SSE41
\c PMINSB           xmmreg,xmmrm             SSE41
\c PMINSD           xmmreg,xmmrm             SSE41
\c PMINUD           xmmreg,xmmrm             SSE41
\c PMINUW           xmmreg,xmmrm             SSE41
\c PMOVSXBW         xmmreg,xmmrm             SSE41
\c PMOVSXBD         xmmreg,xmmrm             SSE41,SD
\c PMOVSXBQ         xmmreg,xmmrm             SSE41,SW
\c PMOVSXWD         xmmreg,xmmrm             SSE41
\c PMOVSXWQ         xmmreg,xmmrm             SSE41,SD
\c PMOVSXDQ         xmmreg,xmmrm             SSE41
\c PMOVZXBW         xmmreg,xmmrm             SSE41
\c PMOVZXBD         xmmreg,xmmrm             SSE41,SD
\c PMOVZXBQ         xmmreg,xmmrm             SSE41,SW
\c PMOVZXWD         xmmreg,xmmrm             SSE41
\c PMOVZXWQ         xmmreg,xmmrm             SSE41,SD
\c PMOVZXDQ         xmmreg,xmmrm             SSE41
\c PMULDQ           xmmreg,xmmrm             SSE41
\c PMULLD           xmmreg,xmmrm             SSE41
\c PTEST            xmmreg,xmmrm             SSE41
\c ROUNDPD          xmmreg,xmmrm,imm         SSE41
\c ROUNDPS          xmmreg,xmmrm,imm         SSE41
\c ROUNDSD          xmmreg,xmmrm,imm         SSE41
\c ROUNDSS          xmmreg,xmmrm,imm         SSE41

\S{} Nehalem New Instructions (SSE4.2)

\c CRC32            reg32,rm8                SSE42
\c CRC32            reg32,rm16               SSE42
\c CRC32            reg32,rm32               SSE42
\c CRC32            reg64,rm8                SSE42,X64
\c CRC32            reg64,rm64               SSE42,X64
\c PCMPESTRI        xmmreg,xmmrm,imm         SSE42
\c PCMPESTRM        xmmreg,xmmrm,imm         SSE42
\c PCMPISTRI        xmmreg,xmmrm,imm         SSE42
\c PCMPISTRM        xmmreg,xmmrm,imm         SSE42
\c PCMPGTQ          xmmreg,xmmrm             SSE42
\c POPCNT           reg16,rm16               NEHALEM
\c POPCNT           reg32,rm32               NEHALEM
\c POPCNT           reg64,rm32               NEHALEM,X64

\S{} AMD SSE5 instructions

\c FMADDPS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMADDPS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMADDPS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMADDPS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FMADDPD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMADDPD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMADDPD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMADDPD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FMADDSS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMADDSS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMADDSS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMADDSS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FMADDSD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMADDSD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMADDSD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMADDSD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FMSUBPS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMSUBPS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMSUBPS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMSUBPS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FMSUBPD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMSUBPD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMSUBPD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMSUBPD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FMSUBSS          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMSUBSS          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMSUBSS          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMSUBSS          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FMSUBSD          xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FMSUBSD          xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FMSUBSD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FMSUBSD          xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMADDPS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMADDPS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMADDPS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMADDPS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMADDPD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMADDPD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMADDPD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMADDPD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMADDSS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMADDSS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMADDSS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMADDSS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMADDSD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMADDSD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMADDSD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMADDSD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMSUBPS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMSUBPS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMSUBPS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMSUBPS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMSUBPD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMSUBPD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMSUBPD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMSUBPD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMSUBSS         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMSUBSS         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMSUBSS         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMSUBSS         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c FNMSUBSD         xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c FNMSUBSD         xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c FNMSUBSD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c FNMSUBSD         xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c COMEQPS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMLTPS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMLEPS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNORDPS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNEQPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNLTPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNLEPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMORDPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUEQPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMULTPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMULEPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMFALSEPS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMNEQPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMNLTPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMNLEPS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMTRUEPS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMPS            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c COMEQPD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMLTPD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMLEPD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNORDPD       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNEQPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNLTPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUNLEPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMORDPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMUEQPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMULTPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMULEPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMFALSEPD       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMNEQPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMNLTPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMNLEPD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMTRUEPD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c COMPD            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c COMEQSS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMLTSS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMLESS          xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMUNORDSS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMUNEQSS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMUNLTSS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMUNLESS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMORDSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMUEQSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMULTSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMULESS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMFALSESS       xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMNEQSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMNLTSS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMNLESS         xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMTRUESS        xmmreg,xmmreg,xmmrm      SSE5,AMD,SD
\c COMSS            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SD
\c COMEQSD          xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMLTSD          xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMLESD          xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMUNORDSD       xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMUNEQSD        xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMUNLTSD        xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMUNLESD        xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMORDSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMUEQSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMULTSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMULESD         xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMFALSESD       xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMNEQSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMNLTSD         xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMNLESD         xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMTRUESD        xmmreg,xmmreg,xmmrm      SSE5,AMD
\c COMSD            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD
\c PCOMLTB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLEB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGEB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQB          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSEB       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUEB        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMB            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PCOMLTW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLEW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGEW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQW          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSEW       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUEW        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMW            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PCOMLTD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLED          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGED          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQD          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSED       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUED        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMD            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PCOMLTQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLEQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGEQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQQ          xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSEQ       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUEQ        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMQ            xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PCOMLTUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLEUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGEUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQUB         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQUB        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSEUB      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUEUB       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMUB           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PCOMLTUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLEUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGEUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQUW         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQUW        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSEUW      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUEUW       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMUW           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PCOMLTUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLEUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGEUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQUD         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQUD        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSEUD      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUEUD       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMUD           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PCOMLTUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMLEUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGTUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMGEUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMEQUQ         xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMNEQUQ        xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMFALSEUQ      xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMTRUEUQ       xmmreg,xmmreg,xmmrm      SSE5,AMD,SO
\c PCOMUQ           xmmreg,xmmreg,xmmrm,imm  SSE5,AMD,SO
\c PERMPS           xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c PERMPS           xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c PERMPS           xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PERMPS           xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c PERMPD           xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c PERMPD           xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c PERMPD           xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PERMPD           xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c PCMOV            xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c PCMOV            xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c PCMOV            xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PCMOV            xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c PPERM            xmmreg,=0,xmmreg,xmmrm   SSE5,AMD
\c PPERM            xmmreg,=0,xmmrm,xmmreg   SSE5,AMD
\c PPERM            xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PPERM            xmmreg,xmmrm,xmmreg,=0   SSE5,AMD
\c PMACSSWW         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSWW          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSSWD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSWD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSSDD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSDD          xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSSDQL        xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSDQL         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSSDQH        xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMACSDQH         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMADCSSWD        xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PMADCSWD         xmmreg,xmmreg,xmmrm,=0   SSE5,AMD
\c PROTB            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PROTB            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PROTW            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PROTW            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PROTD            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PROTD            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PROTQ            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PROTQ            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHLB            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHLB            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHLW            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHLW            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHLD            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHLD            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHLQ            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHLQ            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHAB            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHAB            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHAW            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHAW            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHAD            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHAD            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c PSHAQ            xmmreg,xmmreg,xmmrm      SSE5,AMD
\c PSHAQ            xmmreg,xmmrm,xmmreg      SSE5,AMD
\c FRCZPS           xmmreg,xmmrm             SSE5,AMD
\c FRCZPD           xmmreg,xmmrm             SSE5,AMD
\c FRCZSS           xmmreg,xmmrm             SSE5,AMD
\c FRCZSD           xmmreg,xmmrm             SSE5,AMD
\c CVTPH2PS         xmmreg,xmmrm             SSE5,AMD
\c CVTPS2PH         xmmrm,xmmreg             SSE5,AMD
\c PHADDBW          xmmreg,xmmrm             SSE5,AMD
\c PHADDBD          xmmreg,xmmrm             SSE5,AMD
\c PHADDBQ          xmmreg,xmmrm             SSE5,AMD
\c PHADDWD          xmmreg,xmmrm             SSE5,AMD
\c PHADDWQ          xmmreg,xmmrm             SSE5,AMD
\c PHADDDQ          xmmreg,xmmrm             SSE5,AMD
\c PHADDUBW         xmmreg,xmmrm             SSE5,AMD
\c PHADDUBD         xmmreg,xmmrm             SSE5,AMD
\c PHADDUBQ         xmmreg,xmmrm             SSE5,AMD
\c PHADDUWD         xmmreg,xmmrm             SSE5,AMD
\c PHADDUWQ         xmmreg,xmmrm             SSE5,AMD
\c PHADDUDQ         xmmreg,xmmrm             SSE5,AMD
\c PHSUBBW          xmmreg,xmmrm             SSE5,AMD
\c PHSUBWD          xmmreg,xmmrm             SSE5,AMD
\c PHSUBDQ          xmmreg,xmmrm             SSE5,AMD
\c PROTB            xmmreg,xmmrm,imm         SSE5,AMD
\c PROTW            xmmreg,xmmrm,imm         SSE5,AMD
\c PROTD            xmmreg,xmmrm,imm         SSE5,AMD
\c PROTQ            xmmreg,xmmrm,imm         SSE5,AMD
\c ROUNDPS          xmmreg,xmmrm,imm         SSE5,AMD
\c ROUNDPD          xmmreg,xmmrm,imm         SSE5,AMD
\c ROUNDSS          xmmreg,xmmrm,imm         SSE5,AMD
\c ROUNDSD          xmmreg,xmmrm,imm         SSE5,AMD

\S{} Intel SMX

\c GETSEC                                    KATMAI

\S{} Geode (Cyrix) 3DNow! additions

\c PFRCPV           mmxreg,mmxrm             PENT,3DNOW,CYRIX
\c PFRSQRTV         mmxreg,mmxrm             PENT,3DNOW,CYRIX

\S{} Intel new instructions in ???

\c MOVBE            reg16,mem16              NEHALEM
\c MOVBE            reg32,mem32              NEHALEM
\c MOVBE            reg64,mem64              NEHALEM
\c MOVBE            mem16,reg16              NEHALEM
\c MOVBE            mem32,reg32              NEHALEM
\c MOVBE            mem64,reg64              NEHALEM

\S{} Intel AES instructions

\c AESENC           xmmreg,xmmrm             WESTMERE,SO
\c AESENCLAST       xmmreg,xmmrm             WESTMERE,SO
\c AESDEC           xmmreg,xmmrm             WESTMERE,SO
\c AESDECLAST       xmmreg,xmmrm             WESTMERE,SO
\c AESIMC           xmmreg,xmmrm             WESTMERE,SO
\c AESKEYGENASSIST  xmmreg,xmmrm,imm         WESTMERE,SO

\S{} Intel AVX AES instructions

\c VAESENC          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VAESENC          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VAESENCLAST      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VAESENCLAST      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VAESDEC          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VAESDEC          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VAESDECLAST      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VAESDECLAST      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VAESIMC          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VAESKEYGENASSIST xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO

\S{} Intel AVX instructions

\c VADDPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VADDPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VADDPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VADDPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VADDPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VADDPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VADDPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VADDPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VADDSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VADDSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VADDSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VADDSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VADDSUBPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VADDSUBPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VADDSUBPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VADDSUBPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VADDSUBPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VADDSUBPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VADDSUBPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VADDSUBPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VANDPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VANDPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VANDPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VANDPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VANDPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VANDPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VANDPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VANDPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VANDNPD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VANDNPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VANDNPD          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VANDNPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VANDNPS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VANDNPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VANDNPS          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VANDNPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VBLENDPD         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VBLENDPD         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VBLENDPD         ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VBLENDPD         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VBLENDPS         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VBLENDPS         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VBLENDPS         ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VBLENDPS         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VBLENDVPD        xmmreg,xmmreg,xmmrm,xmmrm AVX,SANDYBRIDGE,SO
\c VBLENDVPD        xmmreg,xmmrm,xmm0        AVX,SANDYBRIDGE,SO
\c VBLENDVPD        ymmreg,ymmreg,ymmrm,ymmrm AVX,SANDYBRIDGE,SY
\c VBLENDVPD        ymmreg,ymmrm,ymm0        AVX,SANDYBRIDGE,SY
\c VBLENDVPS        xmmreg,xmmreg,xmmrm,xmmrm AVX,SANDYBRIDGE,SO
\c VBLENDVPS        xmmreg,xmmrm,xmm0        AVX,SANDYBRIDGE,SO
\c VBLENDVPS        ymmreg,ymmreg,ymmrm,ymmrm AVX,SANDYBRIDGE,SY
\c VBLENDVPD        ymmreg,ymmrm,ymm0        AVX,SANDYBRIDGE,SY
\c VBROADCASTSS     xmmreg,mem               AVX,SANDYBRIDGE,SD
\c VBROADCASTSS     ymmreg,mem               AVX,SANDYBRIDGE,SD
\c VBROADCASTSD     ymmreg,mem               AVX,SANDYBRIDGE
\c VBROADCASTF128   ymmreg,mem               AVX,SANDYBRIDGE,SO
\c VCMPEQPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLTPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLTPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLTPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLTPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLEPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLEPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLEPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLEPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPUNORDPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPUNORDPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPUNORDPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPUNORDPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLTPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLTPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLTPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLTPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLEPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLEPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLEPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLEPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPORDPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPORDPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPORDPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPORDPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPEQ_UQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQ_UQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQ_UQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQ_UQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGEPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGEPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGEPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGEPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGTPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGTPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGTPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGTPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPFALSEPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPFALSEPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPFALSEPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPFALSEPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGEPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGEPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGEPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGEPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGTPD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGTPD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGTPD         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGTPD         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPTRUEPD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPTRUEPD       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPTRUEPD       ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPTRUEPD       ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPEQ_OSPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQ_OSPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQ_OSPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQ_OSPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLT_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLT_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLT_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLT_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLE_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLE_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLE_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLE_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPUNORD_SPD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPUNORD_SPD    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPUNORD_SPD    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPUNORD_SPD    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQ_USPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQ_USPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQ_USPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQ_USPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLT_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLT_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLT_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLT_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLE_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLE_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLE_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLE_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPORD_SPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPORD_SPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPORD_SPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPORS_SPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPEQ_USPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQ_USPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQ_USPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQ_USPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGE_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGE_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGE_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGE_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGT_UQPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGT_UQPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGT_UQPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGT_UQPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPFALSE_OSPD   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPFALSE_OSPD   xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPFALSE_OSPD   ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPFALSE_OSPD   ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OSPD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OSPD     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OSPD     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OSPD     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGE_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGE_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGE_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGE_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGT_OQPD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGT_OQPD      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGT_OQPD      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGT_OQPD      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPTRUE_USPD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPTRUE_USPD    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPTRUE_USPD    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPTRUE_USPD    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPPD           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VCMPPD           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VCMPPD           ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VCMPPD           ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VCMPEQPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLTPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLTPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLTPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLTPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLEPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLEPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLEPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLEPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPUNORDPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPUNORDPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPUNORDPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPUNORDPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLTPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLTPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLTPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLTPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLEPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLEPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLEPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLEPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPORDPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPORDPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPORDPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPORDPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPEQ_UQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQ_UQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQ_UQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQ_UQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGEPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGEPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGEPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGEPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGTPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGTPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGTPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGTPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPFALSEPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPFALSEPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPFALSEPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPFALSEPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGEPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGEPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGEPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGEPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGTPS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGTPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGTPS         ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGTPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPTRUEPS       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPTRUEPS       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPTRUEPS       ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPTRUEPS       ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPEQ_OSPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQ_OSPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQ_OSPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQ_OSPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLT_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLT_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLT_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLT_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPLE_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPLE_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPLE_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPLE_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPUNORD_SPS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPUNORD_SPS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPUNORD_SPS    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPUNORD_SPS    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQ_USPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQ_USPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQ_USPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQ_USPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLT_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLT_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLT_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLT_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNLE_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNLE_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNLE_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNLE_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPORD_SPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPORD_SPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPORD_SPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPORS_SPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPEQ_USPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPEQ_USPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPEQ_USPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPEQ_USPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGE_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGE_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGE_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGE_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNGT_UQPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNGT_UQPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNGT_UQPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNGT_UQPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPFALSE_OSPS   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPFALSE_OSPS   xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPFALSE_OSPS   ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPFALSE_OSPS   ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OSPS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OSPS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPNEQ_OSPS     ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPNEQ_OSPS     ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGE_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGE_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGE_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGE_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPGT_OQPS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPGT_OQPS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPGT_OQPS      ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPGT_OQPS      ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPTRUE_USPS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VCMPTRUE_USPS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCMPTRUE_USPS    ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VCMPTRUE_USPS    ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCMPPS           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VCMPPS           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VCMPPS           ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VCMPPS           ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VCMPEQSD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPEQSD         xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPLTSD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPLTSD         xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPLESD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPLESD         xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPUNORDSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPUNORDSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNEQSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNEQSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNLTSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNLTSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNLESD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNLESD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPORDSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPORDSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPEQ_UQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPEQ_UQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNGESD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNGESD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNGTSD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNGTSD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPFALSESD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPFALSESD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNEQ_OQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNEQ_OQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPGESD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPGESD         xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPGTSD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPGTSD         xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPTRUESD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPTRUESD       xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPEQ_OSSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPEQ_OSSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPLT_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPLT_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPLE_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPLE_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPUNORD_SSD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPUNORD_SSD    xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNEQ_USSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNEQ_USSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNLT_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNLT_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNLE_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNLE_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPORD_SSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPORD_SSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPEQ_USSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPEQ_USSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNGE_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNGE_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNGT_UQSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNGT_UQSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPFALSE_OSSD   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPFALSE_OSSD   xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPNEQ_OSSD     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPNEQ_OSSD     xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPGE_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPGE_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPGT_OQSD      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPGT_OQSD      xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPTRUE_USSD    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCMPTRUE_USSD    xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCMPSD           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE
\c VCMPSD           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE
\c VCMPEQSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPEQSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPLTSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPLTSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPLESS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPLESS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPUNORDSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPUNORDSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNEQSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNEQSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNLTSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNLTSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNLESS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNLESS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPORDSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPORDSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPEQ_UQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPEQ_UQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNGESS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNGESS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNGTSS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNGTSS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPFALSESS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPFALSESS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNEQ_OQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNEQ_OQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPGESS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPGESS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPGTSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPGTSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPTRUESS       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPTRUESS       xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPEQ_OSSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPEQ_OSSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPLT_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPLT_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPLE_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPLE_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPUNORD_SSS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPUNORD_SSS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNEQ_USSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNEQ_USSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNLT_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNLT_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNLE_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNLE_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPORD_SSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPORD_SSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPEQ_USSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPEQ_USSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNGE_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNGE_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNGT_UQSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNGT_UQSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPFALSE_OSSS   xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPFALSE_OSSS   xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPNEQ_OSSS     xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPNEQ_OSSS     xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPGE_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPGE_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPGT_OQSS      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPGT_OQSS      xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPTRUE_USSS    xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCMPTRUE_USSS    xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCMPSS           xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SD
\c VCMPSS           xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SD
\c VCOMISD          xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCOMISS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCVTDQ2PD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCVTDQ2PD        ymmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCVTDQ2PS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCVTDQ2PS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCVTPD2DQ        xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VCVTPD2DQ        xmmreg,mem128            AVX,SANDYBRIDGE
\c VCVTPD2DQ        xmmreg,ymmreg            AVX,SANDYBRIDGE
\c VCVTPD2DQ        xmmreg,mem256            AVX,SANDYBRIDGE
\c VCVTPD2PS        xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VCVTPD2PS        xmmreg,mem128            AVX,SANDYBRIDGE
\c VCVTPD2PS        xmmreg,ymmreg            AVX,SANDYBRIDGE
\c VCVTPD2PS        xmmreg,mem256            AVX,SANDYBRIDGE
\c VCVTPS2DQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCVTPS2DQ        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCVTPS2PD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCVTPS2PD        ymmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCVTSD2SI        reg32,xmmrm              AVX,SANDYBRIDGE
\c VCVTSD2SI        reg64,xmmrm              AVX,SANDYBRIDGE,LONG
\c VCVTSD2SS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VCVTSD2SS        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VCVTSI2SD        xmmreg,xmmreg,rm32       AVX,SANDYBRIDGE
\c VCVTSI2SD        xmmreg,rm32              AVX,SANDYBRIDGE
\c VCVTSI2SD        xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SD,ND
\c VCVTSI2SD        xmmreg,mem               AVX,SANDYBRIDGE,SD,ND
\c VCVTSI2SD        xmmreg,xmmreg,rm64       AVX,SANDYBRIDGE,LONG
\c VCVTSI2SD        xmmreg,rm64              AVX,SANDYBRIDGE,LONG
\c VCVTSI2SS        xmmreg,xmmreg,rm32       AVX,SANDYBRIDGE
\c VCVTSI2SS        xmmreg,rm32              AVX,SANDYBRIDGE
\c VCVTSI2SS        xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SD,ND
\c VCVTSI2SS        xmmreg,mem               AVX,SANDYBRIDGE,SD,ND
\c VCVTSI2SS        xmmreg,xmmreg,rm64       AVX,SANDYBRIDGE,LONG
\c VCVTSI2SS        xmmreg,rm64              AVX,SANDYBRIDGE,LONG
\c VCVTSS2SD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VCVTSS2SD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VCVTSS2SI        reg32,xmmrm              AVX,SANDYBRIDGE,SD
\c VCVTSS2SI        reg64,xmmrm              AVX,SANDYBRIDGE,SD,LONG
\c VCVTTPD2DQ       xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VCVTTPD2DQ       xmmreg,mem128            AVX,SANDYBRIDGE
\c VCVTTPD2DQ       xmmreg,ymmreg            AVX,SANDYBRIDGE
\c VCVTTPD2DQ       xmmreg,mem256            AVX,SANDYBRIDGE
\c VCVTTPS2DQ       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VCVTTPS2DQ       ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VCVTTSD2SI       reg32,xmmrm              AVX,SANDYBRIDGE
\c VCVTTSD2SI       reg64,xmmrm              AVX,SANDYBRIDGE,LONG
\c VCVTTSS2SI       reg32,xmmrm              AVX,SANDYBRIDGE,SD
\c VCVTTSS2SI       reg64,xmmrm              AVX,SANDYBRIDGE,SD,LONG
\c VDIVPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VDIVPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VDIVPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VDIVPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VDIVPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VDIVPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VDIVPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VDIVPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VDIVSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VDIVSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VDIVSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VDIVSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VDPPD            xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VDPPD            xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VDPPS            xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VDPPS            xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VDPPS            ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VDPPS            ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VEXTRACTF128     xmmrm,xmmreg,imm         AVX,SANDYBRIDGE,SO
\c VEXTRACTPS       rm32,xmmreg,imm          AVX,SANDYBRIDGE,SD
\c VHADDPD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VHADDPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VHADDPD          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VHADDPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VHADDPS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VHADDPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VHADDPS          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VHADDPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VHSUBPD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VHSUBPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VHSUBPD          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VHSUBPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VHSUBPS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VHSUBPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VHSUBPS          ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VHSUBPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VINSERTF128      ymmreg,ymmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VINSERTPS        xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SD
\c VINSERTPS        xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SD
\c VLDDQU           xmmreg,mem               AVX,SANDYBRIDGE,SO
\c VLDQQU           ymmreg,mem               AVX,SANDYBRIDGE,SY
\c VLDDQU           ymmreg,mem               AVX,SANDYBRIDGE,SY
\c VLDMXCSR         mem32                    AVX,SANDYBRIDGE,SD
\c VMASKMOVDQU      xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VMASKMOVPS       xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SO
\c VMASKMOVPS       ymmreg,ymmreg,mem        AVX,SANDYBRIDGE,SY
\c VMASKMOVPS       mem,xmmreg,xmmreg        AVX,SANDYBRIDGE,SO
\c VMASKMOVPS       mem,xmmreg,xmmreg        AVX,SANDYBRIDGE,SY
\c VMASKMOVPD       xmmreg,xmmreg,mem        AVX,SANDYBRIDGE,SO
\c VMASKMOVPD       ymmreg,ymmreg,mem        AVX,SANDYBRIDGE,SY
\c VMASKMOVPD       mem,xmmreg,xmmreg        AVX,SANDYBRIDGE,SO
\c VMASKMOVPD       mem,ymmreg,ymmreg        AVX,SANDYBRIDGE,SY
\c VMAXPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VMAXPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMAXPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VMAXPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMAXPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VMAXPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMAXPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VMAXPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMAXSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VMAXSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VMAXSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VMAXSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VMINPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VMINPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMINPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VMINPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMINPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VMINPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMINPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VMINPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMINSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VMINSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VMINSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VMINSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VMOVAPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVAPD          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
\c VMOVAPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVAPD          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMOVAPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVAPS          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
\c VMOVAPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVAPS          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMOVQ            xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VMOVQ            xmmrm,xmmreg             AVX,SANDYBRIDGE
\c VMOVD            xmmreg,rm32              AVX,SANDYBRIDGE,SD
\c VMOVQ            xmmreg,rm64              AVX,SANDYBRIDGE,LONG
\c VMOVD            rm32,xmmreg              AVX,SANDYBRIDGE,SD
\c VMOVQ            rm64,xmmreg              AVX,SANDYBRIDGE,LONG
\c VMOVDDUP         xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VMOVDDUP         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVDQA          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVDQA          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
\c VMOVQQA          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVQQA          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMOVDQA          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVDQA          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMOVDQU          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVDQU          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
\c VMOVQQU          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVQQU          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMOVDQU          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVDQU          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMOVHLPS         xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
\c VMOVHLPS         xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VMOVHPD          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
\c VMOVHPD          xmmreg,mem               AVX,SANDYBRIDGE
\c VMOVHPD          mem,xmmreg               AVX,SANDYBRIDGE
\c VMOVHPS          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
\c VMOVHPS          xmmreg,mem               AVX,SANDYBRIDGE
\c VMOVHPS          mem,xmmreg               AVX,SANDYBRIDGE
\c VMOVLHPS         xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
\c VMOVLHPS         xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VMOVLPD          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
\c VMOVLPD          xmmreg,mem               AVX,SANDYBRIDGE
\c VMOVLPD          mem,xmmreg               AVX,SANDYBRIDGE
\c VMOVLPS          xmmreg,xmmreg,mem        AVX,SANDYBRIDGE
\c VMOVLPS          xmmreg,mem               AVX,SANDYBRIDGE
\c VMOVLPS          mem,xmmreg               AVX,SANDYBRIDGE
\c VMOVMSKPD        reg64,xmmreg             AVX,SANDYBRIDGE,LONG
\c VMOVMSKPD        reg32,xmmreg             AVX,SANDYBRIDGE
\c VMOVMSKPD        reg64,ymmreg             AVX,SANDYBRIDGE,LONG
\c VMOVMSKPD        reg32,ymmreg             AVX,SANDYBRIDGE
\c VMOVMSKPS        reg64,xmmreg             AVX,SANDYBRIDGE,LONG
\c VMOVMSKPS        reg32,xmmreg             AVX,SANDYBRIDGE
\c VMOVMSKPS        reg64,ymmreg             AVX,SANDYBRIDGE,LONG
\c VMOVMSKPS        reg32,ymmreg             AVX,SANDYBRIDGE
\c VMOVNTDQ         mem,xmmreg               AVX,SANDYBRIDGE,SO
\c VMOVNTQQ         mem,ymmreg               AVX,SANDYBRIDGE,SY
\c VMOVNTDQ         mem,ymmreg               AVX,SANDYBRIDGE,SY
\c VMOVNTDQA        xmmreg,mem               AVX,SANDYBRIDGE,SO
\c VMOVNTPD         mem,xmmreg               AVX,SANDYBRIDGE,SO
\c VMOVNTPD         mem,ymmreg               AVX,SANDYBRIDGE,SY
\c VMOVNTPS         mem,xmmreg               AVX,SANDYBRIDGE,SO
\c VMOVNTPS         mem,ymmreg               AVX,SANDYBRIDGE,SO
\c VMOVSD           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
\c VMOVSD           xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VMOVSD           xmmreg,mem               AVX,SANDYBRIDGE
\c VMOVSD           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
\c VMOVSD           xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VMOVSD           mem,xmmreg               AVX,SANDYBRIDGE
\c VMOVSHDUP        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVSHDUP        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVSLDUP        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVSLDUP        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVSS           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
\c VMOVSS           xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VMOVSS           xmmreg,mem               AVX,SANDYBRIDGE
\c VMOVSS           xmmreg,xmmreg,xmmreg     AVX,SANDYBRIDGE
\c VMOVSS           xmmreg,xmmreg            AVX,SANDYBRIDGE
\c VMOVSS           mem,xmmreg               AVX,SANDYBRIDGE
\c VMOVUPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVUPD          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
\c VMOVUPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVUPD          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMOVUPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMOVUPS          xmmrm,xmmreg             AVX,SANDYBRIDGE,SO
\c VMOVUPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMOVUPS          ymmrm,ymmreg             AVX,SANDYBRIDGE,SY
\c VMPSADBW         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VMPSADBW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VMULPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VMULPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMULPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VMULPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMULPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VMULPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VMULPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VMULPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VMULSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VMULSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VMULSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VMULSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VORPD            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VORPD            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VORPD            ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VORPD            ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VORPS            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VORPS            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VORPS            ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VORPS            ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VPABSB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPABSW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPABSD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPACKSSWB        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPACKSSWB        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPACKSSDW        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPACKSSDW        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPACKUSWB        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPACKUSWB        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPACKUSDW        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPACKUSDW        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDB           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDUSB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDUSB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPADDUSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPADDUSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPALIGNR         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VPALIGNR         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPAND            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPAND            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPANDN           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPANDN           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPAVGB           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPAVGB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPAVGW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPAVGW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPBLENDVB        xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
\c VPBLENDVB        xmmreg,xmmrm,xmmreg      AVX,SANDYBRIDGE,SO
\c VPBLENDW         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VPBLENDW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPCMPESTRI       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPCMPESTRM       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPCMPISTRI       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPCMPISTRM       xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPCMPEQB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPEQB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPCMPEQW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPEQW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPCMPEQD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPEQD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPCMPEQQ         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPEQQ         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPCMPGTB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPGTB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPCMPGTW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPGTW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPCMPGTD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPGTD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPCMPGTQ         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPCMPGTQ         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPERMILPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPERMILPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VPERMILPD        xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPERMILPD        ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VPERMILTD2PD     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
\c VPERMILTD2PD     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
\c VPERMILTD2PD     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
\c VPERMILTD2PD     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
\c VPERMILMO2PD     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
\c VPERMILMO2PD     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
\c VPERMILMO2PD     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
\c VPERMILMO2PD     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
\c VPERMILMZ2PD     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
\c VPERMILMZ2PD     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
\c VPERMILMZ2PD     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
\c VPERMILMZ2PD     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
\c VPERMIL2PD       xmmreg,xmmreg,xmmrm,xmmreg,imm AVX,SANDYBRIDGE,SO
\c VPERMIL2PD       xmmreg,xmmreg,xmmreg,xmmrm,imm AVX,SANDYBRIDGE,SO
\c VPERMIL2PD       ymmreg,ymmreg,ymmrm,ymmreg,imm AVX,SANDYBRIDGE,SY
\c VPERMIL2PD       ymmreg,ymmreg,ymmreg,ymmrm,imm AVX,SANDYBRIDGE,SY
\c VPERMILPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPERMILPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VPERMILPS        xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPERMILPS        ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VPERMILTD2PS     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
\c VPERMILTD2PS     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
\c VPERMILTD2PS     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
\c VPERMILTD2PS     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
\c VPERMILMO2PS     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
\c VPERMILMO2PS     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
\c VPERMILMO2PS     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
\c VPERMILMO2PS     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
\c VPERMILMZ2PS     xmmreg,xmmreg,xmmrm,xmmreg AVX,SANDYBRIDGE,SO
\c VPERMILMZ2PS     xmmreg,xmmreg,xmmreg,xmmrm AVX,SANDYBRIDGE,SO
\c VPERMILMZ2PS     ymmreg,ymmreg,ymmrm,ymmreg AVX,SANDYBRIDGE,SY
\c VPERMILMZ2PS     ymmreg,ymmreg,ymmreg,ymmrm AVX,SANDYBRIDGE,SY
\c VPERMIL2PS       xmmreg,xmmreg,xmmrm,xmmreg,imm AVX,SANDYBRIDGE,SO
\c VPERMIL2PS       xmmreg,xmmreg,xmmreg,xmmrm,imm AVX,SANDYBRIDGE,SO
\c VPERMIL2PS       ymmreg,ymmreg,ymmrm,ymmreg,imm AVX,SANDYBRIDGE,SY
\c VPERMIL2PS       ymmreg,ymmreg,ymmreg,ymmrm,imm AVX,SANDYBRIDGE,SY
\c VPERM2F128       ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VPEXTRB          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
\c VPEXTRB          reg32,xmmreg,imm         AVX,SANDYBRIDGE
\c VPEXTRB          mem,xmmreg,imm           AVX,SANDYBRIDGE
\c VPEXTRW          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
\c VPEXTRW          reg32,xmmreg,imm         AVX,SANDYBRIDGE
\c VPEXTRW          mem,xmmreg,imm           AVX,SANDYBRIDGE,SW
\c VPEXTRW          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
\c VPEXTRW          reg32,xmmreg,imm         AVX,SANDYBRIDGE
\c VPEXTRW          mem,xmmreg,imm           AVX,SANDYBRIDGE,SW
\c VPEXTRD          reg64,xmmreg,imm         AVX,SANDYBRIDGE,LONG
\c VPEXTRD          rm32,xmmreg,imm          AVX,SANDYBRIDGE,SD
\c VPEXTRQ          rm64,xmmreg,imm          AVX,SANDYBRIDGE,LONG
\c VPHADDW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPHADDW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPHADDD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPHADDD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPHADDSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPHADDSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPHMINPOSUW      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPHSUBW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPHSUBW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPHSUBD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPHSUBD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPHSUBSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPHSUBSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPINSRB          xmmreg,xmmreg,reg32,imm  AVX,SANDYBRIDGE
\c VPINSRB          xmmreg,reg32,imm         AVX,SANDYBRIDGE
\c VPINSRB          xmmreg,xmmreg,mem,imm    AVX,SANDYBRIDGE
\c VPINSRB          xmmreg,reg32,mem,imm     AVX,SANDYBRIDGE
\c VPINSRW          xmmreg,xmmreg,reg32,imm  AVX,SANDYBRIDGE
\c VPINSRW          xmmreg,reg32,imm         AVX,SANDYBRIDGE
\c VPINSRW          xmmreg,xmmreg,mem,imm    AVX,SANDYBRIDGE,SW
\c VPINSRW          xmmreg,reg32,mem,imm     AVX,SANDYBRIDGE,SW
\c VPINSRD          xmmreg,xmmreg,rm32,imm   AVX,SANDYBRIDGE,SD
\c VPINSRD          xmmreg,rm32,imm          AVX,SANDYBRIDGE,SD
\c VPINSRQ          xmmreg,xmmreg,rm64,imm   AVX,SANDYBRIDGE,LONG
\c VPINSRQ          xmmreg,rm64,imm          AVX,SANDYBRIDGE,SD,LONG
\c VPMADDWD         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMADDWD         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMADDUBSW       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMADDUBSW       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMAXSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMAXSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMAXSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMAXSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMAXSD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMAXSD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMAXUB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMAXUB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMAXUW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMAXUW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMAXUD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMAXUD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMINSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMINSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMINSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMINSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMINSD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMINSD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMINUB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMINUB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMINUW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMINUW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMINUD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMINUD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMOVMSKB        reg64,xmmreg             AVX,SANDYBRIDGE,LONG
\c VPMOVMSKB        reg32,xmmreg             AVX,SANDYBRIDGE
\c VPMOVSXBW        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VPMOVSXBD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VPMOVSXBQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SW
\c VPMOVSXWD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VPMOVSXWQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VPMOVSXDQ        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VPMOVZXBW        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VPMOVZXBD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VPMOVZXBQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SW
\c VPMOVZXWD        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VPMOVZXWQ        xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VPMOVZXDQ        xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VPMULHUW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMULHUW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMULHRSW        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMULHRSW        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMULHW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMULHW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMULLW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMULLW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMULLD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMULLD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMULUDQ         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMULUDQ         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPMULDQ          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPMULDQ          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPOR             xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPOR             xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSADBW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSADBW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSHUFB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSHUFB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSHUFD          xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPSHUFHW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPSHUFLW         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VPSIGNB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSIGNB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSIGNW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSIGNW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSIGND          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSIGND          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSLLDQ          xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSLLDQ          xmmreg,imm               AVX,SANDYBRIDGE
\c VPSRLDQ          xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSRLDQ          xmmreg,imm               AVX,SANDYBRIDGE
\c VPSLLW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSLLW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSLLW           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSLLW           xmmreg,imm               AVX,SANDYBRIDGE
\c VPSLLD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSLLD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSLLD           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSLLD           xmmreg,imm               AVX,SANDYBRIDGE
\c VPSLLQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSLLQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSLLQ           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSLLQ           xmmreg,imm               AVX,SANDYBRIDGE
\c VPSRAW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSRAW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSRAW           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSRAW           xmmreg,imm               AVX,SANDYBRIDGE
\c VPSRAD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSRAD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSRAD           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSRAD           xmmreg,imm               AVX,SANDYBRIDGE
\c VPSRLW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSRLW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSRLW           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSRLW           xmmreg,imm               AVX,SANDYBRIDGE
\c VPSRLD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSRLD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSRLD           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSRLD           xmmreg,imm               AVX,SANDYBRIDGE
\c VPSRLQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSRLQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSRLQ           xmmreg,xmmreg,imm        AVX,SANDYBRIDGE
\c VPSRLQ           xmmreg,imm               AVX,SANDYBRIDGE
\c VPTEST           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPTEST           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VPSUBB           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBB           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSUBW           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBW           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSUBD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSUBQ           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBQ           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSUBSB          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBSB          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSUBSW          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBSW          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSUBUSB         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBUSB         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPSUBUSW         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPSUBUSW         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKHBW       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKHBW       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKHWD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKHWD       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKHDQ       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKHDQ       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKHQDQ      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKHQDQ      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKLBW       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKLBW       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKLWD       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKLWD       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKLDQ       xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKLDQ       xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPUNPCKLQDQ      xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPUNPCKLQDQ      xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VPXOR            xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VPXOR            xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VRCPPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VRCPPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VRCPSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VRCPSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VRSQRTPS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VRSQRTPS         ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VRSQRTSS         xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VRSQRTSS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VROUNDPD         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VROUNDPD         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VROUNDPS         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VROUNDPS         ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VROUNDSD         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE
\c VROUNDSD         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE
\c VROUNDSS         xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SD
\c VROUNDSS         xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SD
\c VSHUFPD          xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VSHUFPD          xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VSHUFPD          ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VSHUFPD          ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VSHUFPS          xmmreg,xmmreg,xmmrm,imm  AVX,SANDYBRIDGE,SO
\c VSHUFPS          xmmreg,xmmrm,imm         AVX,SANDYBRIDGE,SO
\c VSHUFPS          ymmreg,ymmreg,ymmrm,imm  AVX,SANDYBRIDGE,SY
\c VSHUFPS          ymmreg,ymmrm,imm         AVX,SANDYBRIDGE,SY
\c VSQRTPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VSQRTPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VSQRTPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VSQRTPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VSQRTSD          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VSQRTSD          xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VSQRTSS          xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VSQRTSS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VSTMXCSR         mem                      AVX,SANDYBRIDGE,SD
\c VSUBPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VSUBPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VSUBPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VSUBPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VSUBPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VSUBPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VSUBPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VSUBPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VSUBSD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE
\c VSUBSD           xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VSUBSS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SD
\c VSUBSS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VTESTPS          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VTESTPS          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VTESTPD          xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VTESTPD          ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VUCOMISD         xmmreg,xmmrm             AVX,SANDYBRIDGE
\c VUCOMISS         xmmreg,xmmrm             AVX,SANDYBRIDGE,SD
\c VUNPCKHPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VUNPCKHPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VUNPCKHPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VUNPCKHPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VUNPCKHPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VUNPCKHPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VUNPCKHPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VUNPCKHPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VUNPCKLPD        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VUNPCKLPD        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VUNPCKLPD        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VUNPCKLPD        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VUNPCKLPS        xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VUNPCKLPS        xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VUNPCKLPS        ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VUNPCKLPS        ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VXORPD           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VXORPD           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VXORPD           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VXORPD           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VXORPS           xmmreg,xmmreg,xmmrm      AVX,SANDYBRIDGE,SO
\c VXORPS           xmmreg,xmmrm             AVX,SANDYBRIDGE,SO
\c VXORPS           ymmreg,ymmreg,ymmrm      AVX,SANDYBRIDGE,SY
\c VXORPS           ymmreg,ymmrm             AVX,SANDYBRIDGE,SY
\c VZEROALL                                  AVX,SANDYBRIDGE
\c VZEROUPPER                                AVX,SANDYBRIDGE

\S{} Intel Carry-Less Multiplication instructions (CLMUL)

\c PCLMULLQLQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
\c PCLMULHQLQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
\c PCLMULLQHQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
\c PCLMULHQHQDQ     xmmreg,xmmrm             SSE,SANDYBRIDGE,SO
\c PCLMULQDQ        xmmreg,xmmrm,imm         SSE,SANDYBRIDGE,SO

\S{} Intel Fused Multiply-Add instructions (FMA)

\c VFMADDPD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMADDPD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMADDPD         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMADDPD         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMADDPS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMADDPS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMADDPS         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMADDPS         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMADDSD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
\c VFMADDSD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
\c VFMADDSS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
\c VFMADDSS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD
\c VFMADDSUBPD      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMADDSUBPD      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMADDSUBPD      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMADDSUBPD      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMADDSUBPS      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMADDSUBPS      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMADDSUBPS      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMADDSUBPS      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMSUBADDPD      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMSUBADDPD      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMSUBADDPD      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMSUBADDPD      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMSUBADDPS      xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMSUBADDPS      xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMSUBADDPS      ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMSUBADDPS      ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMSUBPD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMSUBPD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMSUBPD         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMSUBPD         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMSUBPS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFMSUBPS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFMSUBPS         ymmreg,ymmreg,ymmrm,ymmreg FMA,SANDYBRIDGE,SY
\c VFMSUBPS         ymmreg,ymmreg,ymmreg,ymmrm FMA,SANDYBRIDGE,SY
\c VFMSUBSD         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
\c VFMSUBSD         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
\c VFMSUBSS         xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
\c VFMSUBSS         xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD
\c VFNMADDPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFNMADDPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFNMADDPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
\c VFNMADDPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
\c VFNMADDPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFNMADDPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFNMADDPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
\c VFNMADDPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
\c VFNMADDSD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
\c VFNMADDSD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
\c VFNMADDSS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
\c VFNMADDSS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD
\c VFNMSUBPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFNMSUBPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFNMSUBPD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
\c VFNMSUBPD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
\c VFNMSUBPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SO
\c VFNMSUBPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SO
\c VFNMSUBPS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SY
\c VFNMSUBPS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SY
\c VFNMSUBSD        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE
\c VFNMSUBSD        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE
\c VFNMSUBSS        xmmreg,xmmreg,xmmrm,xmmreg FMA,SANDYBRIDGE,SD
\c VFNMSUBSS        xmmreg,xmmreg,xmmreg,xmmrm FMA,SANDYBRIDGE,SD

\S{} VIA (Centaur) security instructions

\c XSTORE                                    PENT,CYRIX
\c XCRYPTECB                                 PENT,CYRIX
\c XCRYPTCBC                                 PENT,CYRIX
\c XCRYPTCTR                                 PENT,CYRIX
\c XCRYPTCFB                                 PENT,CYRIX
\c XCRYPTOFB                                 PENT,CYRIX
\c MONTMUL                                   PENT,CYRIX
\c XSHA1                                     PENT,CYRIX
\c XSHA256                                   PENT,CYRIX

\S{} Systematic names for the hinting nop instructions

\c HINT_NOP0        rm16                     P6,UNDOC
\c HINT_NOP0        rm32                     P6,UNDOC
\c HINT_NOP0        rm64                     X64,UNDOC
\c HINT_NOP1        rm16                     P6,UNDOC
\c HINT_NOP1        rm32                     P6,UNDOC
\c HINT_NOP1        rm64                     X64,UNDOC
\c HINT_NOP2        rm16                     P6,UNDOC
\c HINT_NOP2        rm32                     P6,UNDOC
\c HINT_NOP2        rm64                     X64,UNDOC
\c HINT_NOP3        rm16                     P6,UNDOC
\c HINT_NOP3        rm32                     P6,UNDOC
\c HINT_NOP3        rm64                     X64,UNDOC
\c HINT_NOP4        rm16                     P6,UNDOC
\c HINT_NOP4        rm32                     P6,UNDOC
\c HINT_NOP4        rm64                     X64,UNDOC
\c HINT_NOP5        rm16                     P6,UNDOC
\c HINT_NOP5        rm32                     P6,UNDOC
\c HINT_NOP5        rm64                     X64,UNDOC
\c HINT_NOP6        rm16                     P6,UNDOC
\c HINT_NOP6        rm32                     P6,UNDOC
\c HINT_NOP6        rm64                     X64,UNDOC
\c HINT_NOP7        rm16                     P6,UNDOC
\c HINT_NOP7        rm32                     P6,UNDOC
\c HINT_NOP7        rm64                     X64,UNDOC
\c HINT_NOP8        rm16                     P6,UNDOC
\c HINT_NOP8        rm32                     P6,UNDOC
\c HINT_NOP8        rm64                     X64,UNDOC
\c HINT_NOP9        rm16                     P6,UNDOC
\c HINT_NOP9        rm32                     P6,UNDOC
\c HINT_NOP9        rm64                     X64,UNDOC
\c HINT_NOP10       rm16                     P6,UNDOC
\c HINT_NOP10       rm32                     P6,UNDOC
\c HINT_NOP10       rm64                     X64,UNDOC
\c HINT_NOP11       rm16                     P6,UNDOC
\c HINT_NOP11       rm32                     P6,UNDOC
\c HINT_NOP11       rm64                     X64,UNDOC
\c HINT_NOP12       rm16                     P6,UNDOC
\c HINT_NOP12       rm32                     P6,UNDOC
\c HINT_NOP12       rm64                     X64,UNDOC
\c HINT_NOP13       rm16                     P6,UNDOC
\c HINT_NOP13       rm32                     P6,UNDOC
\c HINT_NOP13       rm64                     X64,UNDOC
\c HINT_NOP14       rm16                     P6,UNDOC
\c HINT_NOP14       rm32                     P6,UNDOC
\c HINT_NOP14       rm64                     X64,UNDOC
\c HINT_NOP15       rm16                     P6,UNDOC
\c HINT_NOP15       rm32                     P6,UNDOC
\c HINT_NOP15       rm64                     X64,UNDOC
\c HINT_NOP16       rm16                     P6,UNDOC
\c HINT_NOP16       rm32                     P6,UNDOC
\c HINT_NOP16       rm64                     X64,UNDOC
\c HINT_NOP17       rm16                     P6,UNDOC
\c HINT_NOP17       rm32                     P6,UNDOC
\c HINT_NOP17       rm64                     X64,UNDOC
\c HINT_NOP18       rm16                     P6,UNDOC
\c HINT_NOP18       rm32                     P6,UNDOC
\c HINT_NOP18       rm64                     X64,UNDOC
\c HINT_NOP19       rm16                     P6,UNDOC
\c HINT_NOP19       rm32                     P6,UNDOC
\c HINT_NOP19       rm64                     X64,UNDOC
\c HINT_NOP20       rm16                     P6,UNDOC
\c HINT_NOP20       rm32                     P6,UNDOC
\c HINT_NOP20       rm64                     X64,UNDOC
\c HINT_NOP21       rm16                     P6,UNDOC
\c HINT_NOP21       rm32                     P6,UNDOC
\c HINT_NOP21       rm64                     X64,UNDOC
\c HINT_NOP22       rm16                     P6,UNDOC
\c HINT_NOP22       rm32                     P6,UNDOC
\c HINT_NOP22       rm64                     X64,UNDOC
\c HINT_NOP23       rm16                     P6,UNDOC
\c HINT_NOP23       rm32                     P6,UNDOC
\c HINT_NOP23       rm64                     X64,UNDOC
\c HINT_NOP24       rm16                     P6,UNDOC
\c HINT_NOP24       rm32                     P6,UNDOC
\c HINT_NOP24       rm64                     X64,UNDOC
\c HINT_NOP25       rm16                     P6,UNDOC
\c HINT_NOP25       rm32                     P6,UNDOC
\c HINT_NOP25       rm64                     X64,UNDOC
\c HINT_NOP26       rm16                     P6,UNDOC
\c HINT_NOP26       rm32                     P6,UNDOC
\c HINT_NOP26       rm64                     X64,UNDOC
\c HINT_NOP27       rm16                     P6,UNDOC
\c HINT_NOP27       rm32                     P6,UNDOC
\c HINT_NOP27       rm64                     X64,UNDOC
\c HINT_NOP28       rm16                     P6,UNDOC
\c HINT_NOP28       rm32                     P6,UNDOC
\c HINT_NOP28       rm64                     X64,UNDOC
\c HINT_NOP29       rm16                     P6,UNDOC
\c HINT_NOP29       rm32                     P6,UNDOC
\c HINT_NOP29       rm64                     X64,UNDOC
\c HINT_NOP30       rm16                     P6,UNDOC
\c HINT_NOP30       rm32                     P6,UNDOC
\c HINT_NOP30       rm64                     X64,UNDOC
\c HINT_NOP31       rm16                     P6,UNDOC
\c HINT_NOP31       rm32                     P6,UNDOC
\c HINT_NOP31       rm64                     X64,UNDOC
\c HINT_NOP32       rm16                     P6,UNDOC
\c HINT_NOP32       rm32                     P6,UNDOC
\c HINT_NOP32       rm64                     X64,UNDOC
\c HINT_NOP33       rm16                     P6,UNDOC
\c HINT_NOP33       rm32                     P6,UNDOC
\c HINT_NOP33       rm64                     X64,UNDOC
\c HINT_NOP34       rm16                     P6,UNDOC
\c HINT_NOP34       rm32                     P6,UNDOC
\c HINT_NOP34       rm64                     X64,UNDOC
\c HINT_NOP35       rm16                     P6,UNDOC
\c HINT_NOP35       rm32                     P6,UNDOC
\c HINT_NOP35       rm64                     X64,UNDOC
\c HINT_NOP36       rm16                     P6,UNDOC
\c HINT_NOP36       rm32                     P6,UNDOC
\c HINT_NOP36       rm64                     X64,UNDOC
\c HINT_NOP37       rm16                     P6,UNDOC
\c HINT_NOP37       rm32                     P6,UNDOC
\c HINT_NOP37       rm64                     X64,UNDOC
\c HINT_NOP38       rm16                     P6,UNDOC
\c HINT_NOP38       rm32                     P6,UNDOC
\c HINT_NOP38       rm64                     X64,UNDOC
\c HINT_NOP39       rm16                     P6,UNDOC
\c HINT_NOP39       rm32                     P6,UNDOC
\c HINT_NOP39       rm64                     X64,UNDOC
\c HINT_NOP40       rm16                     P6,UNDOC
\c HINT_NOP40       rm32                     P6,UNDOC
\c HINT_NOP40       rm64                     X64,UNDOC
\c HINT_NOP41       rm16                     P6,UNDOC
\c HINT_NOP41       rm32                     P6,UNDOC
\c HINT_NOP41       rm64                     X64,UNDOC
\c HINT_NOP42       rm16                     P6,UNDOC
\c HINT_NOP42       rm32                     P6,UNDOC
\c HINT_NOP42       rm64                     X64,UNDOC
\c HINT_NOP43       rm16                     P6,UNDOC
\c HINT_NOP43       rm32                     P6,UNDOC
\c HINT_NOP43       rm64                     X64,UNDOC
\c HINT_NOP44       rm16                     P6,UNDOC
\c HINT_NOP44       rm32                     P6,UNDOC
\c HINT_NOP44       rm64                     X64,UNDOC
\c HINT_NOP45       rm16                     P6,UNDOC
\c HINT_NOP45       rm32                     P6,UNDOC
\c HINT_NOP45       rm64                     X64,UNDOC
\c HINT_NOP46       rm16                     P6,UNDOC
\c HINT_NOP46       rm32                     P6,UNDOC
\c HINT_NOP46       rm64                     X64,UNDOC
\c HINT_NOP47       rm16                     P6,UNDOC
\c HINT_NOP47       rm32                     P6,UNDOC
\c HINT_NOP47       rm64                     X64,UNDOC
\c HINT_NOP48       rm16                     P6,UNDOC
\c HINT_NOP48       rm32                     P6,UNDOC
\c HINT_NOP48       rm64                     X64,UNDOC
\c HINT_NOP49       rm16                     P6,UNDOC
\c HINT_NOP49       rm32                     P6,UNDOC
\c HINT_NOP49       rm64                     X64,UNDOC
\c HINT_NOP50       rm16                     P6,UNDOC
\c HINT_NOP50       rm32                     P6,UNDOC
\c HINT_NOP50       rm64                     X64,UNDOC
\c HINT_NOP51       rm16                     P6,UNDOC
\c HINT_NOP51       rm32                     P6,UNDOC
\c HINT_NOP51       rm64                     X64,UNDOC
\c HINT_NOP52       rm16                     P6,UNDOC
\c HINT_NOP52       rm32                     P6,UNDOC
\c HINT_NOP52       rm64                     X64,UNDOC
\c HINT_NOP53       rm16                     P6,UNDOC
\c HINT_NOP53       rm32                     P6,UNDOC
\c HINT_NOP53       rm64                     X64,UNDOC
\c HINT_NOP54       rm16                     P6,UNDOC
\c HINT_NOP54       rm32                     P6,UNDOC
\c HINT_NOP54       rm64                     X64,UNDOC
\c HINT_NOP55       rm16                     P6,UNDOC
\c HINT_NOP55       rm32                     P6,UNDOC
\c HINT_NOP55       rm64                     X64,UNDOC
\c HINT_NOP56       rm16                     P6,UNDOC
\c HINT_NOP56       rm32                     P6,UNDOC
\c HINT_NOP56       rm64                     X64,UNDOC
\c HINT_NOP57       rm16                     P6,UNDOC
\c HINT_NOP57       rm32                     P6,UNDOC
\c HINT_NOP57       rm64                     X64,UNDOC
\c HINT_NOP58       rm16                     P6,UNDOC
\c HINT_NOP58       rm32                     P6,UNDOC
\c HINT_NOP58       rm64                     X64,UNDOC
\c HINT_NOP59       rm16                     P6,UNDOC
\c HINT_NOP59       rm32                     P6,UNDOC
\c HINT_NOP59       rm64                     X64,UNDOC
\c HINT_NOP60       rm16                     P6,UNDOC
\c HINT_NOP60       rm32                     P6,UNDOC
\c HINT_NOP60       rm64                     X64,UNDOC
\c HINT_NOP61       rm16                     P6,UNDOC
\c HINT_NOP61       rm32                     P6,UNDOC
\c HINT_NOP61       rm64                     X64,UNDOC
\c HINT_NOP62       rm16                     P6,UNDOC
\c HINT_NOP62       rm32                     P6,UNDOC
\c HINT_NOP62       rm64                     X64,UNDOC
\c HINT_NOP63       rm16                     P6,UNDOC
\c HINT_NOP63       rm32                     P6,UNDOC
\c HINT_NOP63       rm64                     X64,UNDOC

