API Guide Home (Online version only) |

# PalmAudioPCMParamType Struct Reference

## Detailed Description

PCM format parameters.

Definition at line 383 of file palmOneCodecFormat.h.

## Data Fields

- UInt32 sampleRate
- UInt32 sampleType
- UInt32 sampleWidth

## Field Documentation

UInt32 sampleRate

Sample rate (44100, 32000...).

Definition at line 384 of file palmOneCodecFormat.h.

UInt32 sampleType

Sample type (use the one one from Sound Manager).

Definition at line 385 of file palmOneCodecFormat.h.

UInt32 sampleWidth

Sample width (mono/stereo).

Definition at line 386 of file palmOneCodecFormat.h.

Top | Palm Developer Network © 2004-2008, Palm, Inc. All rights reserved. Generated on Fri Jun 13 10:08:15 2008 for Palm API Guide