Arco Dual Channel EIDE Adapter Delivers First 32 Bit OS/2 Warp Driver,
Supports Fast ATA Drives, CD-roms

Arco Computer Products announces the ACD-rom, a dual channel VL-bus EIDE
adapter. At $94 with an est. street price of about half, this cost
effective adapter will connect EIDE, CD-rom, serial and parallel products.
The adapter delivers the the first OS/2 Warp 32 bit driver enabling the
full speed of the operating system and the maximum data transfer rate of
Enhanced IDE.

The adapter has an advanced bios which sees the entire drive as one
partition without 3rd party software. By using this hardware solution,
users will see approximatley a 30% increase in performance. This feature
combined with the 32 bit Warp driver will receive true Mode 3 performance,
matching or exceeding the 32 bit disk and file access touted by Windows.

The board supports up to 4 IDE/EIDE drives and/or ATAPI devices. The 16C550
UART supports up to V.34 modems from the two serial ports. The enhanced
parallel port is ECP, SPP, EPP compatible for fast parallel tranfers.
Floppy support ranges up to 2.88 MB.

Setup is jumperless and software configurable.

Arco is located at 2750 N. 29th Ave. S-316, Hollywood, Fl. 33020.
Phone 800-458-1666, Fax 305-925-2889
 
 =========================================================
 From the 'New Product News' Electronic News Service on...
 AOL (Keyword = New Products) and Delphi (GO COMP PROD)
 =========================================================
 This information was processed from data provided by the
 company/author mentioned. For additional details, please
 contact them directly at the address/phone# indicated.
 Trademarks are the property of their respective owners.
 =========================================================
 All submissions for this service should be addressed to:
 BAKER ENTERPRISES,  20 Ferro Dr,  Sewell, NJ  08080  USA
 Email: rbakerpc@delphi.com  -or- RBakerPC (on AOL/Delphi)
 =========================================================
