
........Making Your Tire Sandals

First, place either foot in the center of a large piece of paper, at 
least an 8 1/2 x 14. Trace around your foot, being careful at all 
times to keep the pencil straight up and down. Next make a mark on 
each side, directly down from the point on your ankles (A) (see 
pattern at the end of this web page). Also make a mark at the point 
along the inside of your foot, directly back from your big toe (B). 

Remove your foot from the pattern. Now sketch a bigger outline 
around the tracing of your foot. Add about 3/8 inch for the toes and 
sides, but not to the back. Then use a ruler and bisect the pattern 
lengthwise, extending the line three inches past the heel. This 
serves as a guide to help you sketch the rear tab accurately. Now 
connect the marks you made by your ankles (A), extending a line 
three inches beyond each side of the pattern. These tabs will be 
sketched in front of this line. Also draw a line for the front tabs, 
extending from the single mark (B) across the pattern, perpendicular 
to the line that bisects the foot lengthwise. 

To learn more and the rest of the instructions, go to..

http://www.hollowtop.com/sandals.htm

tenzicut

